2024/4/17 9:45:03 新建项目11成功
2024/4/17 9:45:04 通讯(COM1)连接成功
2024/4/30 8:25:50 Current project(310)Loading…
2024/4/30 8:25:51 Current project(310)download finished
2024/4/30 8:25:51 Communication(COM3)Abnormal connection：Please check the parameters of the serial port configurationThe port 'COM3' does not exist.
4/30/2024 12:24:32 PM New project 13 succeeded
4/30/2024 12:24:32 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
4/30/2024 12:26:06 PM New project 53 succeeded
4/30/2024 12:26:06 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
4/30/2024 12:26:08 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
4/30/2024 12:26:08 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
5/2/2024 3:54:32 PM New project 123 succeeded
5/2/2024 3:54:32 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
5/2/2024 4:07:08 PM New project 13 succeeded
5/2/2024 4:07:08 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
5/2/2024 4:09:22 PM New project 132 succeeded
5/2/2024 4:09:23 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/02/2024 11:12:22 New project 123 succeeded
05/02/2024 11:12:22 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/02/2024 15:51:07 New project 44 succeeded
05/02/2024 15:51:07 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/03/2024 10:10:55 Current project(44)Loading…
05/03/2024 10:10:55 Current project(44)download finished
05/03/2024 10:10:55 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/03/2024 10:11:27 New project 123 succeeded
05/03/2024 10:11:28 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/03/2024 10:11:53 Current project(123)Loading…
05/03/2024 10:11:54 Current project(123)download finished
05/03/2024 10:11:54 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
05/03/2024 10:56:52 New project test succeeded
05/03/2024 10:56:52 Communication(COM3)Connection succeeded
05/03/2024 10:56:58 Read function code(C00.00 Given frequency)：37.65
05/03/2024 10:56:58 Read function code(C00.01 Output frequency)：0.00
05/03/2024 10:56:58 Read function code(C00.02 Output current)：0.0
05/03/2024 10:56:58 Read function code(C00.03 Input voltage)：383.2
05/03/2024 10:56:58 Read function code(C00.04 Output voltage)：0.0
05/03/2024 10:56:58 Read function code(C00.05 Mechanical speed)：0
05/03/2024 10:56:59 Read function code(C00.06 Given torque)：250.0
05/03/2024 10:56:59 Read function code(C00.07 Output torque)：0.0
05/03/2024 10:56:59 Read function code(C00.08 PID Given amount)：0.0
05/03/2024 10:56:59 Read function code(C00.09 PID Feedback amount)：0.0
05/03/2024 10:56:59 Read function code(C00.10 Output Power)：0.0
05/03/2024 10:56:59 Read function code(C00.11 Bus voltage)：542.4
05/03/2024 10:56:59 Read function code(C00.12 Module temperature1)：21.2
05/03/2024 10:56:59 Read function code(C00.13 Module temperature2)：21.2
05/03/2024 10:56:59 Read function code(C00.14 Input terminal X connected state)：00000000
05/03/2024 10:56:59 Read function code(C00.15 Output terminal Y connected state)：00000000
05/03/2024 10:56:59 Read function code(C00.16 Analog AI1 input value)：7.531
05/03/2024 10:56:59 Read function code(C00.17 Analog AI2 input value)：0.000
05/03/2024 10:56:59 Read function code(C00.18 Keyboard potentiometer)：0.00
05/03/2024 10:56:59 Read function code(C00.19 Pulse signal PUL input value)：0.000
05/03/2024 10:56:59 Read function code(C00.20 Analog output AO1)：7.53
05/03/2024 10:56:59 Read function code(C00.21 Analog output AO2 (extended))：0.00
05/03/2024 10:56:59 Read function code(C00.22 Counter count value)：0
05/03/2024 10:56:59 Read function code(C00.23 Running time of this power-on)：0.0
05/03/2024 10:56:59 Read function code(C00.24 Accumulated running time of this machine)：0
05/03/2024 10:56:59 Read function code(C00.25 Inverter power rated power)：2.2
05/03/2024 10:57:00 Read function code(C00.26 Inverter rated voltage)：380
05/03/2024 10:57:00 Read function code(C00.27 Inverter rated current)：6.0
05/03/2024 10:57:00 Read function code(C00.28 Software version)：60.20
05/03/2024 10:57:00 Read function code(C00.29 PGFeedback frequency)：0.00
05/03/2024 10:57:00 Read function code(C00.30 Timer )：0
05/03/2024 10:57:00 Read function code(C00.31 PID output )：0.00
05/03/2024 10:57:00 Read function code(C00.32 Software subversion)：9.92
05/03/2024 10:57:00 Read function code(C00.33 Encoder angle)：0.00
05/03/2024 10:57:00 Read function code(C00.34 Z pulse error)：0
05/03/2024 10:57:00 Read function code(C00.35 Z pulse count)：0
05/03/2024 10:57:00 Read function code(C00.36 Fault warning code)：0:No failure
05/03/2024 10:57:00 Read function code(C00.37 Cumulative power consumption (low level))：0
05/03/2024 10:57:00 Read function code(C00.38 Accumulated electricity consumption (high　level))：0
05/03/2024 10:57:00 Read function code(C00.39 Power factor angle)：0.0
05/03/2024 10:57:00 Read function code(C00.40)：0
05/03/2024 10:57:00 Read function code(C00.41)：0
05/03/2024 10:57:00 Read function code(C00.42)：0
05/03/2024 10:57:00 Read function code(C00.43)：0
05/03/2024 10:57:00 Read function code(C00.44)：0
05/03/2024 10:57:01 Read function code(C00.45)：0
05/03/2024 10:57:01 Read function code(C00.46)：0
05/03/2024 10:57:01 Read function code(C00.47)：0
05/03/2024 10:57:01 Read function code(C00.48)：0
05/03/2024 10:57:01 Read function code(C00.49)：0
05/03/2024 10:57:01 Read function code(C00.50)：0
05/03/2024 10:57:01 Read function code(C00.51)：0
05/03/2024 10:57:01 Read function code(C00.52)：0
05/03/2024 10:57:01 Read function code(C00.53)：0
05/03/2024 10:57:01 Read function code(C00.54)：30000
05/03/2024 10:57:01 Read function code(C00.55)：0
05/03/2024 10:57:01 Read function code(C00.56)：0
05/03/2024 10:57:01 Read function code(C00.57)：65425
05/03/2024 10:57:01 Read function code(C00.58)：65447
05/03/2024 10:57:01 Read function code(C00.59)：165
05/03/2024 10:57:01 Read function code(C00.60)：5412
05/03/2024 10:57:01 Read function code(C00.61)：0
05/03/2024 10:57:01 Read function code(C00.62)：0
05/03/2024 10:57:01 Read function code(C00.63)：0
05/03/2024 10:58:17 Read function code(C00.00 Given frequency)：37.65
05/03/2024 10:58:17 Read function code(C00.01 Output frequency)：0.00
05/03/2024 10:58:17 Read function code(C00.02 Output current)：0.0
05/03/2024 10:58:17 Read function code(C00.03 Input voltage)：381.6
05/03/2024 10:58:17 Read function code(C00.04 Output voltage)：0.0
05/03/2024 10:58:17 Read function code(C00.05 Mechanical speed)：0
05/03/2024 10:58:17 Read function code(C00.06 Given torque)：250.0
05/03/2024 10:58:17 Read function code(C00.07 Output torque)：0.0
05/03/2024 10:58:17 Read function code(C00.08 PID Given amount)：0.0
05/03/2024 10:58:17 Read function code(C00.09 PID Feedback amount)：0.0
05/03/2024 10:58:17 Read function code(C00.10 Output Power)：0.0
05/03/2024 10:58:17 Read function code(C00.11 Bus voltage)：539.9
05/03/2024 10:58:17 Read function code(C00.12 Module temperature1)：21.4
05/03/2024 10:58:17 Read function code(C00.13 Module temperature2)：21.4
05/03/2024 10:58:17 Read function code(C00.14 Input terminal X connected state)：00000000
05/03/2024 10:58:18 Read function code(C00.15 Output terminal Y connected state)：00000000
05/03/2024 10:58:18 Read function code(C00.16 Analog AI1 input value)：7.536
05/03/2024 10:58:18 Read function code(C00.17 Analog AI2 input value)：0.000
05/03/2024 10:58:18 Read function code(C00.18 Keyboard potentiometer)：0.00
05/03/2024 10:58:18 Read function code(C00.19 Pulse signal PUL input value)：0.000
05/03/2024 10:58:18 Read function code(C00.20 Analog output AO1)：7.53
05/03/2024 10:58:18 Read function code(C00.21 Analog output AO2 (extended))：0.00
05/03/2024 10:58:18 Read function code(C00.22 Counter count value)：0
05/03/2024 10:58:18 Read function code(C00.23 Running time of this power-on)：0.0
05/03/2024 10:58:18 Read function code(C00.24 Accumulated running time of this machine)：0
05/03/2024 10:58:18 Read function code(C00.25 Inverter power rated power)：2.2
05/03/2024 10:58:18 Read function code(C00.26 Inverter rated voltage)：380
05/03/2024 10:58:18 Read function code(C00.27 Inverter rated current)：6.0
05/03/2024 10:58:18 Read function code(C00.28 Software version)：60.20
05/03/2024 10:58:18 Read function code(C00.29 PGFeedback frequency)：0.00
05/03/2024 10:58:18 Read function code(C00.30 Timer )：0
05/03/2024 10:58:18 Read function code(C00.31 PID output )：0.00
05/03/2024 10:58:18 Read function code(C00.32 Software subversion)：9.92
05/03/2024 10:58:18 Read function code(C00.33 Encoder angle)：0.00
05/03/2024 10:58:18 Read function code(C00.34 Z pulse error)：0
05/03/2024 10:58:18 Read function code(C00.35 Z pulse count)：0
05/03/2024 10:58:18 Read function code(C00.36 Fault warning code)：0:No failure
05/03/2024 10:58:18 Read function code(C00.37 Cumulative power consumption (low level))：0
05/03/2024 10:58:18 Read function code(C00.38 Accumulated electricity consumption (high　level))：0
05/03/2024 10:58:18 Read function code(C00.39 Power factor angle)：0.0
05/03/2024 10:58:18 Read function code(C00.40)：0
05/03/2024 10:58:18 Read function code(C00.41)：0
05/03/2024 10:58:18 Read function code(C00.42)：0
05/03/2024 10:58:18 Read function code(C00.43)：0
05/03/2024 10:58:18 Read function code(C00.44)：0
05/03/2024 10:58:18 Read function code(C00.45)：0
05/03/2024 10:58:18 Read function code(C00.46)：0
05/03/2024 10:58:18 Read function code(C00.47)：0
05/03/2024 10:58:18 Read function code(C00.48)：0
05/03/2024 10:58:19 Read function code(C00.49)：0
05/03/2024 10:58:19 Read function code(C00.50)：0
05/03/2024 10:58:19 Read function code(C00.51)：0
05/03/2024 10:58:19 Read function code(C00.52)：0
05/03/2024 10:58:19 Read function code(C00.53)：0
05/03/2024 10:58:19 Read function code(C00.54)：30000
05/03/2024 10:58:19 Read function code(C00.55)：0
05/03/2024 10:58:19 Read function code(C00.56)：0
05/03/2024 10:58:19 Read function code(C00.57)：65475
05/03/2024 10:58:19 Read function code(C00.58)：88
05/03/2024 10:58:19 Read function code(C00.59)：65320
05/03/2024 10:58:19 Read function code(C00.60)：5375
05/03/2024 10:58:19 Read function code(C00.61)：0
05/03/2024 10:58:19 Read function code(C00.62)：0
05/03/2024 10:58:19 Read function code(C00.63)：0
05/03/2024 10:58:21 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 10:58:21 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 10:58:21 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 10:58:21 Read function code(F01.03 Frequency given source channel A gain)：100.0
05/03/2024 10:58:21 Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
05/03/2024 10:58:21 Read function code(F01.05 Frequency given source channel B  gain)：100.0
05/03/2024 10:58:21 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 10:58:21 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 10:58:21 Read function code(F01.08 Run command bundle )：0000
05/03/2024 10:58:21 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 10:58:21 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 10:58:22 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 10:58:22 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 10:58:22 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 10:58:22 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 10:58:22 Read function code(F01.15 Reserved)：0
05/03/2024 10:58:22 Read function code(F01.16 Reserved)：0
05/03/2024 10:58:22 Read function code(F01.17 Reserved)：0
05/03/2024 10:58:22 Read function code(F01.18 Reserved)：0
05/03/2024 10:58:22 Read function code(F01.19 Reserved)：0
05/03/2024 10:58:22 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 10:58:22 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 10:58:22 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 10:58:22 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 10:58:22 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 10:58:22 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 10:58:22 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 10:58:22 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 10:58:22 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 10:58:22 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 10:58:22 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 10:58:23 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 10:58:23 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 10:58:23 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 10:58:23 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 10:58:23 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 10:58:23 Read function code(F01.36 Reserved)：0
05/03/2024 10:58:23 Read function code(F01.37 Reserved)：0
05/03/2024 10:58:23 Read function code(F01.38 Reserved)：0
05/03/2024 10:58:23 Read function code(F01.39 Reserved)：0
05/03/2024 10:58:23 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 10:58:23 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 10:58:23 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 10:58:23 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 10:58:23 Read function code(F01.44 Reserved)：15
05/03/2024 10:58:23 Read function code(F01.45 Reserved)：50
05/03/2024 10:58:23 Read function code(F01.46 Random carrier depth )：0
05/03/2024 10:58:23 Read function code(F01.47 Reserved)：0
05/03/2024 10:58:23 Read function code(F01.48 Reserved)：0.00
05/03/2024 10:58:23 Read function code(F01.49 Reserved)：6.0
05/03/2024 10:58:42 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 10:58:42 Set function code(F01.00 Motor 1 way to control )：10-->10:PM VF control 
05/03/2024 10:58:42 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 10:58:42 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 10:58:42 Set function code(F01.03 Frequency given source channel A gain)：100.0-->100.0
05/03/2024 10:58:42 Set function code(F01.04 Frequency given source channel B)：2-->2:Current/voltage analog quantity AI1 given
05/03/2024 10:58:42 Set function code(F01.05 Frequency given source channel B  gain)：100.0-->100.0
05/03/2024 10:58:43 Set function code(F01.06 Frequency channel B reference source)：0-->0:Take the maximum output frequency as the reference source 
05/03/2024 10:58:43 Set function code(F01.07 Frequency given source selection)：0-->0:Channel A
05/03/2024 10:58:43 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 10:58:43 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 10:58:43 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 10:58:43 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 10:58:43 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 10:58:43 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 10:58:43 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 10:58:43 Set function code(F01.15 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.16 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.17 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.18 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.19 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 10:58:43 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 10:58:43 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 10:58:43 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 10:58:43 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 10:58:43 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 10:58:43 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 10:58:43 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 10:58:43 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 10:58:43 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 10:58:43 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 10:58:43 Set function code(F01.36 Reserved)：0-->0
05/03/2024 10:58:43 Set function code(F01.37 Reserved)：0-->0
05/03/2024 10:58:44 Set function code(F01.38 Reserved)：0-->0
05/03/2024 10:58:44 Set function code(F01.39 Reserved)：0-->0
05/03/2024 10:58:44 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 10:58:44 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 10:58:44 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 10:58:44 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 10:58:44 Set function code(F01.44 Reserved)：15-->15
05/03/2024 10:58:44 Set function code(F01.45 Reserved)：50-->50
05/03/2024 10:58:44 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 10:58:44 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 10:58:44 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 10:58:44 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 10:58:44 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 10:58:44 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 10:58:44 Read function code(F01.03 Frequency given source channel A gain)：100.0
05/03/2024 10:58:44 Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
05/03/2024 10:58:44 Read function code(F01.05 Frequency given source channel B  gain)：100.0
05/03/2024 10:58:44 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 10:58:45 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 10:58:45 Read function code(F01.08 Run command bundle )：0000
05/03/2024 10:58:45 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 10:58:45 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 10:58:45 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 10:58:45 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 10:58:45 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 10:58:45 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 10:58:45 Read function code(F01.15 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.16 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.17 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.18 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.19 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 10:58:45 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 10:58:45 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 10:58:45 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 10:58:45 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 10:58:45 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 10:58:45 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 10:58:45 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 10:58:45 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 10:58:45 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 10:58:45 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 10:58:45 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 10:58:45 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 10:58:45 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 10:58:45 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 10:58:45 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 10:58:45 Read function code(F01.36 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.37 Reserved)：0
05/03/2024 10:58:45 Read function code(F01.38 Reserved)：0
05/03/2024 10:58:46 Read function code(F01.39 Reserved)：0
05/03/2024 10:58:46 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 10:58:46 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 10:58:46 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 10:58:46 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 10:58:46 Read function code(F01.44 Reserved)：15
05/03/2024 10:58:46 Read function code(F01.45 Reserved)：50
05/03/2024 10:58:46 Read function code(F01.46 Random carrier depth )：0
05/03/2024 10:58:46 Read function code(F01.47 Reserved)：0
05/03/2024 10:58:46 Read function code(F01.48 Reserved)：0.00
05/03/2024 10:58:46 Read function code(F01.49 Reserved)：6.0
05/03/2024 10:58:56 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 10:58:56 Set function code(F01.00 Motor 1 way to control )：10-->10:PM VF control 
05/03/2024 10:58:56 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 10:58:56 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 10:58:56 Set function code(F01.03 Frequency given source channel A gain)：100.0-->100.0
05/03/2024 10:58:56 Set function code(F01.04 Frequency given source channel B)：2-->2:Current/voltage analog quantity AI1 given
05/03/2024 10:58:56 Set function code(F01.05 Frequency given source channel B  gain)：100.0-->100.0
05/03/2024 10:58:56 Set function code(F01.06 Frequency channel B reference source)：0-->0:Take the maximum output frequency as the reference source 
05/03/2024 10:58:56 Set function code(F01.07 Frequency given source selection)：0-->0:Channel A
05/03/2024 10:58:56 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 10:58:56 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 10:58:56 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 10:58:56 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 10:58:56 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 10:58:56 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 10:58:56 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 10:58:56 Set function code(F01.15 Reserved)：0-->0
05/03/2024 10:58:56 Set function code(F01.16 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.17 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.18 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.19 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 10:58:57 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 10:58:57 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 10:58:57 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 10:58:57 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 10:58:57 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 10:58:57 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 10:58:57 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 10:58:57 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 10:58:57 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 10:58:57 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 10:58:57 Set function code(F01.36 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.37 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.38 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.39 Reserved)：0-->0
05/03/2024 10:58:57 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 10:58:57 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 10:58:57 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 10:58:57 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 10:58:57 Set function code(F01.44 Reserved)：15-->15
05/03/2024 10:58:57 Set function code(F01.45 Reserved)：50-->50
05/03/2024 10:58:57 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 10:58:58 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 10:58:58 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 10:59:15 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 10:59:15 Set function code(F01.00 Motor 1 way to control )：10-->10:PM VF control 
05/03/2024 10:59:15 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 10:59:15 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 10:59:15 Set function code(F01.03 Frequency given source channel A gain)：100.0-->100.0
05/03/2024 10:59:15 Set function code(F01.04 Frequency given source channel B)：2-->2:Current/voltage analog quantity AI1 given
05/03/2024 10:59:15 Set function code(F01.05 Frequency given source channel B  gain)：100.0-->100.0
05/03/2024 10:59:15 Set function code(F01.06 Frequency channel B reference source)：0-->0:Take the maximum output frequency as the reference source 
05/03/2024 10:59:15 Set function code(F01.07 Frequency given source selection)：0-->0:Channel A
05/03/2024 10:59:15 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 10:59:15 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 10:59:15 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 10:59:15 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 10:59:15 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 10:59:15 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 10:59:15 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 10:59:16 Set function code(F01.15 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.16 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.17 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.18 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.19 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 10:59:16 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 10:59:16 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 10:59:16 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 10:59:16 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 10:59:16 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 10:59:16 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 10:59:16 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 10:59:16 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 10:59:16 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 10:59:16 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 10:59:16 Set function code(F01.36 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.37 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.38 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.39 Reserved)：0-->0
05/03/2024 10:59:16 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 10:59:16 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 10:59:16 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 10:59:17 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 10:59:17 Set function code(F01.44 Reserved)：15-->15
05/03/2024 10:59:17 Set function code(F01.45 Reserved)：50-->50
05/03/2024 10:59:17 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 10:59:17 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 10:59:17 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 10:59:18 Set function code(F01.03 Frequency given source channel A gain)：100.0-->0.0
05/03/2024 11:03:03 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:03:03 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:03:03 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:03:03 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:03:03 Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
05/03/2024 11:03:03 Read function code(F01.05 Frequency given source channel B  gain)：100.0
05/03/2024 11:03:03 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 11:03:03 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 11:03:03 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:03:03 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:03:03 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:03:03 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:03:03 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:03:03 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:03:03 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:03:03 Read function code(F01.15 Reserved)：0
05/03/2024 11:03:03 Read function code(F01.16 Reserved)：0
05/03/2024 11:03:03 Read function code(F01.17 Reserved)：0
05/03/2024 11:03:03 Read function code(F01.18 Reserved)：0
05/03/2024 11:03:03 Read function code(F01.19 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:03:04 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:03:04 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:03:04 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:03:04 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:03:04 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:03:04 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:03:04 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:03:04 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:03:04 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:03:04 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:03:04 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:03:04 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:03:04 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:03:04 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:03:04 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:03:04 Read function code(F01.36 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.37 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.38 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.39 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:03:04 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:03:04 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:03:04 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:03:04 Read function code(F01.44 Reserved)：15
05/03/2024 11:03:04 Read function code(F01.45 Reserved)：50
05/03/2024 11:03:04 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:03:04 Read function code(F01.47 Reserved)：0
05/03/2024 11:03:04 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:03:05 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:03:14 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:03:15 Set function code(F01.00 Motor 1 way to control )：10-->10:PM VF control 
05/03/2024 11:03:15 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:03:15 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 11:03:15 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:03:15 Set function code(F01.04 Frequency given source channel B)：2-->2:Current/voltage analog quantity AI1 given
05/03/2024 11:03:15 Set function code(F01.05 Frequency given source channel B  gain)：100.0-->100.0
05/03/2024 11:03:15 Set function code(F01.06 Frequency channel B reference source)：0-->0:Take the maximum output frequency as the reference source 
05/03/2024 11:03:15 Set function code(F01.07 Frequency given source selection)：0-->0:Channel A
05/03/2024 11:03:15 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:03:15 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:03:15 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:03:15 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:03:15 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:03:15 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:03:15 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:03:15 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:03:15 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:03:15 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:03:15 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:03:15 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:03:15 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:03:15 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:03:15 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:03:15 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:03:15 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:03:15 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:03:16 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:03:16 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:03:16 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:03:16 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:03:16 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:03:16 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:03:16 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:03:16 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:03:16 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:03:16 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:03:16 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:03:16 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:03:16 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:03:16 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:03:16 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:03:16 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:03:16 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:03:16 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:03:16 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:03:16 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:03:16 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:03:16 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:03:16 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:03:18 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:03:18 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:03:18 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:03:18 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:03:18 Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
05/03/2024 11:03:18 Read function code(F01.05 Frequency given source channel B  gain)：100.0
05/03/2024 11:03:18 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 11:03:18 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 11:03:18 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:03:19 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:03:19 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:03:19 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:03:19 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:03:19 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:03:19 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:03:19 Read function code(F01.15 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.16 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.17 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.18 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.19 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:03:19 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:03:19 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:03:19 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:03:19 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:03:19 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:03:19 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:03:19 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:03:19 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:03:19 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:03:19 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:03:19 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:03:19 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:03:19 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:03:19 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:03:19 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:03:19 Read function code(F01.36 Reserved)：0
05/03/2024 11:03:19 Read function code(F01.37 Reserved)：0
05/03/2024 11:03:20 Read function code(F01.38 Reserved)：0
05/03/2024 11:03:20 Read function code(F01.39 Reserved)：0
05/03/2024 11:03:20 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:03:20 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:03:20 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:03:20 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:03:20 Read function code(F01.44 Reserved)：15
05/03/2024 11:03:20 Read function code(F01.45 Reserved)：50
05/03/2024 11:03:20 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:03:20 Read function code(F01.47 Reserved)：0
05/03/2024 11:03:20 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:03:20 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:03:37 Set function code(F01.04 Frequency given source channel B)：2-->6:RS485 communication setting
05/03/2024 11:03:41 Set function code(F01.05 Frequency given source channel B  gain)：100.0-->10.0
05/03/2024 11:03:46 Set function code(F01.06 Frequency channel B reference source)：0-->1:Take A set frequency as reference source 
05/03/2024 11:03:51 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:03:51 Set function code(F01.00 Motor 1 way to control )：10-->10:PM VF control 
05/03/2024 11:03:51 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:03:51 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 11:03:51 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:03:51 Set function code(F01.04 Frequency given source channel B)：6-->6:RS485 communication setting
05/03/2024 11:03:51 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->10.0
05/03/2024 11:03:51 Set function code(F01.06 Frequency channel B reference source)：1-->1:Take A set frequency as reference source 
05/03/2024 11:03:51 Set function code(F01.07 Frequency given source selection)：0-->0:Channel A
05/03/2024 11:03:51 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:03:51 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:03:51 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:03:51 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:03:51 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:03:51 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:03:51 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:03:51 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:03:51 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:03:51 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:03:51 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:03:51 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:03:52 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:03:52 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:03:52 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:03:52 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:03:52 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:03:52 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:03:52 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:03:52 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:03:52 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:03:52 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:03:52 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:03:52 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:03:52 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:03:52 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:03:52 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:03:52 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:03:52 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:03:52 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:03:52 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:03:52 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:03:52 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:03:52 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:03:52 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:03:52 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:03:55 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:03:55 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:03:55 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:03:55 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:03:55 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:03:56 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:03:56 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:03:56 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 11:03:56 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:03:56 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:03:56 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:03:56 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:03:56 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:03:56 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:03:56 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:03:56 Read function code(F01.15 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.16 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.17 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.18 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.19 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:03:56 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:03:56 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:03:56 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:03:56 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:03:56 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:03:56 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:03:56 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:03:56 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:03:56 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:03:56 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:03:56 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:03:56 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:03:56 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:03:56 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:03:56 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:03:56 Read function code(F01.36 Reserved)：0
05/03/2024 11:03:56 Read function code(F01.37 Reserved)：0
05/03/2024 11:03:57 Read function code(F01.38 Reserved)：0
05/03/2024 11:03:57 Read function code(F01.39 Reserved)：0
05/03/2024 11:03:57 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:03:57 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:03:57 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:03:57 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:03:57 Read function code(F01.44 Reserved)：15
05/03/2024 11:03:57 Read function code(F01.45 Reserved)：50
05/03/2024 11:03:57 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:03:57 Read function code(F01.47 Reserved)：0
05/03/2024 11:03:57 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:03:57 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:04:02 Set function code(F01.07 Frequency given source selection)：0-->1:Channel B
05/03/2024 11:04:04 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:04:04 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:04:04 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:04:04 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:04:04 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:04:04 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:04:04 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:04:04 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:04:04 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:04:04 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:04:04 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:04:04 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:04:04 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:04:04 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:04:04 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:04:04 Read function code(F01.15 Reserved)：0
05/03/2024 11:04:04 Read function code(F01.16 Reserved)：0
05/03/2024 11:04:04 Read function code(F01.17 Reserved)：0
05/03/2024 11:04:04 Read function code(F01.18 Reserved)：0
05/03/2024 11:04:04 Read function code(F01.19 Reserved)：0
05/03/2024 11:04:04 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:04:04 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:04:05 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:04:05 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:04:05 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:04:05 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:04:05 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:04:05 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:04:05 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:04:05 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:04:05 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:04:05 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:04:05 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:04:05 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:04:05 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:04:05 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:04:05 Read function code(F01.36 Reserved)：0
05/03/2024 11:04:05 Read function code(F01.37 Reserved)：0
05/03/2024 11:04:05 Read function code(F01.38 Reserved)：0
05/03/2024 11:04:05 Read function code(F01.39 Reserved)：0
05/03/2024 11:04:05 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:04:05 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:04:05 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:04:05 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:04:05 Read function code(F01.44 Reserved)：15
05/03/2024 11:04:05 Read function code(F01.45 Reserved)：50
05/03/2024 11:04:05 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:04:05 Read function code(F01.47 Reserved)：0
05/03/2024 11:04:05 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:04:05 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:04:10 Set function code(F01.00 Motor 1 way to control )：10-->0:AM VF control 
05/03/2024 11:04:11 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:04:11 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:04:11 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:04:11 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:04:11 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:04:11 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:04:11 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:04:12 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:04:12 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:04:12 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:04:12 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:04:12 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:04:12 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:04:12 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:04:12 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:04:12 Read function code(F01.15 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.16 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.17 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.18 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.19 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:04:12 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:04:12 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:04:12 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:04:12 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:04:12 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:04:12 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:04:12 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:04:12 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:04:12 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:04:12 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:04:12 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:04:12 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:04:12 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:04:12 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:04:12 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:04:12 Read function code(F01.36 Reserved)：0
05/03/2024 11:04:12 Read function code(F01.37 Reserved)：0
05/03/2024 11:04:13 Read function code(F01.38 Reserved)：0
05/03/2024 11:04:13 Read function code(F01.39 Reserved)：0
05/03/2024 11:04:13 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:04:13 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:04:13 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:04:13 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:04:13 Read function code(F01.44 Reserved)：15
05/03/2024 11:04:13 Read function code(F01.45 Reserved)：50
05/03/2024 11:04:13 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:04:13 Read function code(F01.47 Reserved)：0
05/03/2024 11:04:13 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:04:13 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:04:24 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:04:24 Set function code(F01.00 Motor 1 way to control )：0-->0:AM VF control 
05/03/2024 11:04:24 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:04:24 Set function code(F01.02 Frequency given source channel A)：2-->2:Current/voltage analog quantity AI1 given 
05/03/2024 11:04:24 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:04:24 Set function code(F01.04 Frequency given source channel B)：6-->6:RS485 communication setting
05/03/2024 11:04:24 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->10.0
05/03/2024 11:04:24 Set function code(F01.06 Frequency channel B reference source)：1-->1:Take A set frequency as reference source 
05/03/2024 11:04:24 Set function code(F01.07 Frequency given source selection)：1-->1:Channel B
05/03/2024 11:04:24 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:04:24 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:04:24 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:04:24 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:04:24 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:04:24 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:04:24 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:04:24 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:04:24 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:04:24 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:04:24 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:04:24 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:04:24 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:04:24 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:04:25 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:04:25 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:04:25 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:04:25 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:04:25 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:04:25 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:04:25 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:04:25 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:04:25 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:04:25 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:04:25 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:04:25 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:04:25 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:04:25 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:04:25 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:04:25 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:04:25 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:04:25 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:04:25 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:04:25 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:04:25 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:04:25 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:04:29 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:04:29 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:04:29 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:04:29 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:04:29 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:04:30 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:04:30 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:04:30 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:04:30 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:04:30 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:04:30 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:04:30 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:04:30 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:04:30 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:04:30 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:04:30 Read function code(F01.15 Reserved)：0
05/03/2024 11:04:30 Read function code(F01.16 Reserved)：0
05/03/2024 11:04:30 Read function code(F01.17 Reserved)：0
05/03/2024 11:04:30 Read function code(F01.18 Reserved)：0
05/03/2024 11:04:30 Read function code(F01.19 Reserved)：0
05/03/2024 11:04:30 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:04:30 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:04:30 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:04:30 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:04:30 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:04:30 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:04:30 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:04:30 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:04:30 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:04:30 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:04:30 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:04:30 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:04:30 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:04:30 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:04:31 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:04:31 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:04:31 Read function code(F01.36 Reserved)：0
05/03/2024 11:04:31 Read function code(F01.37 Reserved)：0
05/03/2024 11:04:31 Read function code(F01.38 Reserved)：0
05/03/2024 11:04:31 Read function code(F01.39 Reserved)：0
05/03/2024 11:04:31 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:04:31 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:04:31 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:04:31 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:04:31 Read function code(F01.44 Reserved)：15
05/03/2024 11:04:31 Read function code(F01.45 Reserved)：50
05/03/2024 11:04:31 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:04:31 Read function code(F01.47 Reserved)：0
05/03/2024 11:04:31 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:04:31 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:04:40 Read function code(C00.00 Given frequency)：0.00
05/03/2024 11:04:40 Read function code(C00.01 Output frequency)：0.00
05/03/2024 11:04:40 Read function code(C00.02 Output current)：0.0
05/03/2024 11:04:40 Read function code(C00.03 Input voltage)：376.5
05/03/2024 11:04:40 Read function code(C00.04 Output voltage)：0.0
05/03/2024 11:04:40 Read function code(C00.05 Mechanical speed)：0
05/03/2024 11:04:40 Read function code(C00.06 Given torque)：250.0
05/03/2024 11:04:40 Read function code(C00.07 Output torque)：0.0
05/03/2024 11:04:40 Read function code(C00.08 PID Given amount)：0.0
05/03/2024 11:04:40 Read function code(C00.09 PID Feedback amount)：0.0
05/03/2024 11:04:40 Read function code(C00.10 Output Power)：0.0
05/03/2024 11:04:40 Read function code(C00.11 Bus voltage)：533.7
05/03/2024 11:04:40 Read function code(C00.12 Module temperature1)：22.3
05/03/2024 11:04:40 Read function code(C00.13 Module temperature2)：22.3
05/03/2024 11:04:40 Read function code(C00.14 Input terminal X connected state)：00000000
05/03/2024 11:04:40 Read function code(C00.15 Output terminal Y connected state)：00000000
05/03/2024 11:04:40 Read function code(C00.16 Analog AI1 input value)：7.541
05/03/2024 11:04:40 Read function code(C00.17 Analog AI2 input value)：0.000
05/03/2024 11:04:40 Read function code(C00.18 Keyboard potentiometer)：0.00
05/03/2024 11:04:40 Read function code(C00.19 Pulse signal PUL input value)：0.000
05/03/2024 11:04:41 Read function code(C00.20 Analog output AO1)：0.00
05/03/2024 11:04:41 Read function code(C00.21 Analog output AO2 (extended))：0.00
05/03/2024 11:04:41 Read function code(C00.22 Counter count value)：0
05/03/2024 11:04:41 Read function code(C00.23 Running time of this power-on)：0.0
05/03/2024 11:04:41 Read function code(C00.24 Accumulated running time of this machine)：0
05/03/2024 11:04:41 Read function code(C00.25 Inverter power rated power)：2.2
05/03/2024 11:04:41 Read function code(C00.26 Inverter rated voltage)：380
05/03/2024 11:04:41 Read function code(C00.27 Inverter rated current)：6.0
05/03/2024 11:04:41 Read function code(C00.28 Software version)：60.20
05/03/2024 11:04:41 Read function code(C00.29 PGFeedback frequency)：0.00
05/03/2024 11:04:41 Read function code(C00.30 Timer )：0
05/03/2024 11:04:41 Read function code(C00.31 PID output )：0.00
05/03/2024 11:04:41 Read function code(C00.32 Software subversion)：9.92
05/03/2024 11:04:41 Read function code(C00.33 Encoder angle)：0.00
05/03/2024 11:04:41 Read function code(C00.34 Z pulse error)：0
05/03/2024 11:04:41 Read function code(C00.35 Z pulse count)：0
05/03/2024 11:04:41 Read function code(C00.36 Fault warning code)：0:No failure
05/03/2024 11:04:41 Read function code(C00.37 Cumulative power consumption (low level))：0
05/03/2024 11:04:41 Read function code(C00.38 Accumulated electricity consumption (high　level))：0
05/03/2024 11:04:41 Read function code(C00.39 Power factor angle)：0.0
05/03/2024 11:04:41 Read function code(C00.40)：0
05/03/2024 11:04:41 Read function code(C00.41)：0
05/03/2024 11:04:41 Read function code(C00.42)：0
05/03/2024 11:04:41 Read function code(C00.43)：0
05/03/2024 11:04:41 Read function code(C00.44)：0
05/03/2024 11:04:41 Read function code(C00.45)：0
05/03/2024 11:04:41 Read function code(C00.46)：0
05/03/2024 11:04:41 Read function code(C00.47)：0
05/03/2024 11:04:41 Read function code(C00.48)：0
05/03/2024 11:04:42 Read function code(C00.49)：0
05/03/2024 11:04:42 Read function code(C00.50)：0
05/03/2024 11:04:42 Read function code(C00.51)：0
05/03/2024 11:04:42 Read function code(C00.52)：0
05/03/2024 11:04:42 Read function code(C00.53)：0
05/03/2024 11:04:42 Read function code(C00.54)：30000
05/03/2024 11:04:42 Read function code(C00.55)：0
05/03/2024 11:04:42 Read function code(C00.56)：0
05/03/2024 11:04:42 Read function code(C00.57)：65469
05/03/2024 11:04:42 Read function code(C00.58)：65453
05/03/2024 11:04:42 Read function code(C00.59)：171
05/03/2024 11:04:42 Read function code(C00.60)：5383
05/03/2024 11:04:42 Read function code(C00.61)：0
05/03/2024 11:04:42 Read function code(C00.62)：0
05/03/2024 11:04:42 Read function code(C00.63)：0
05/03/2024 11:05:04 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:05:04 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:05:04 Read function code(F01.02 Frequency given source channel A)：2:Current/voltage analog quantity AI1 given 
05/03/2024 11:05:04 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:05:04 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:05:04 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:05:04 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:05:04 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:05:04 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:05:04 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:05:04 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:05:04 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:05:04 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:05:04 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:05:04 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:05:04 Read function code(F01.15 Reserved)：0
05/03/2024 11:05:04 Read function code(F01.16 Reserved)：0
05/03/2024 11:05:04 Read function code(F01.17 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.18 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.19 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:05:05 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:05:05 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:05:05 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:05:05 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:05:05 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:05:05 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:05:05 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:05:05 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:05:05 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:05:05 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:05:05 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:05:05 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:05:05 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:05:05 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:05:05 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:05:05 Read function code(F01.36 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.37 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.38 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.39 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:05:05 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:05:05 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:05:05 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:05:05 Read function code(F01.44 Reserved)：15
05/03/2024 11:05:05 Read function code(F01.45 Reserved)：50
05/03/2024 11:05:05 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:05:05 Read function code(F01.47 Reserved)：0
05/03/2024 11:05:05 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:05:06 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:05:06 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:05:06 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:05:13 Set function code(F01.00 Motor 1 way to control )：0-->0:AM VF control 
05/03/2024 11:05:19 Set function code(F01.00 Motor 1 way to control )：0-->10:PM VF control 
05/03/2024 11:05:25 Set function code(F01.01 Run command channel)：1-->0:Keyboard control (External keyboard first)
05/03/2024 11:05:29 Set function code(F01.02 Frequency given source channel A)：2-->0:Keyboard numbers Given frequency
05/03/2024 11:05:31 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:05:31 Read function code(F01.01 Run command channel)：0:Keyboard control (External keyboard first)
05/03/2024 11:05:31 Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
05/03/2024 11:05:31 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:05:31 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:05:31 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:05:31 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:05:31 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:05:31 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:05:31 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:05:31 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:05:31 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:05:31 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:05:31 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:05:31 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:05:31 Read function code(F01.15 Reserved)：0
05/03/2024 11:05:31 Read function code(F01.16 Reserved)：0
05/03/2024 11:05:31 Read function code(F01.17 Reserved)：0
05/03/2024 11:05:31 Read function code(F01.18 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.19 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:05:32 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:05:32 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:05:32 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:05:32 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:05:32 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:05:32 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:05:32 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:05:32 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:05:32 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:05:32 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:05:32 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:05:32 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:05:32 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:05:32 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:05:32 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:05:32 Read function code(F01.36 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.37 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.38 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.39 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:05:32 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:05:32 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:05:32 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:05:32 Read function code(F01.44 Reserved)：15
05/03/2024 11:05:32 Read function code(F01.45 Reserved)：50
05/03/2024 11:05:32 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:05:32 Read function code(F01.47 Reserved)：0
05/03/2024 11:05:32 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:05:33 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:05:35 Read function code(F01.00 Motor 1 way to control )：10:PM VF control 
05/03/2024 11:05:35 Read function code(F01.01 Run command channel)：0:Keyboard control (External keyboard first)
05/03/2024 11:05:35 Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
05/03/2024 11:05:35 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:05:35 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:05:35 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:05:35 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:05:35 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:05:35 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:05:36 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:05:36 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:05:36 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:05:36 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:05:36 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:05:36 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:05:36 Read function code(F01.15 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.16 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.17 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.18 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.19 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:05:36 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:05:36 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:05:36 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:05:36 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:05:36 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:05:36 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:05:36 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:05:36 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:05:36 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:05:36 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:05:36 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:05:36 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:05:36 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:05:36 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:05:36 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:05:36 Read function code(F01.36 Reserved)：0
05/03/2024 11:05:36 Read function code(F01.37 Reserved)：0
05/03/2024 11:05:37 Read function code(F01.38 Reserved)：0
05/03/2024 11:05:37 Read function code(F01.39 Reserved)：0
05/03/2024 11:05:37 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:05:37 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:05:37 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:05:37 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:05:37 Read function code(F01.44 Reserved)：15
05/03/2024 11:05:37 Read function code(F01.45 Reserved)：50
05/03/2024 11:05:37 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:05:37 Read function code(F01.47 Reserved)：0
05/03/2024 11:05:37 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:05:37 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:05:44 Set function code(F01.00 Motor 1 way to control )：10-->0:AM VF control 
05/03/2024 11:05:47 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:05:47 Read function code(F01.01 Run command channel)：0:Keyboard control (External keyboard first)
05/03/2024 11:05:47 Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
05/03/2024 11:05:47 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:05:47 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:05:47 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:05:47 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:05:47 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:05:47 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:05:47 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:05:47 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:05:47 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:05:47 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:05:47 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:05:47 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:05:47 Read function code(F01.15 Reserved)：0
05/03/2024 11:05:47 Read function code(F01.16 Reserved)：0
05/03/2024 11:05:47 Read function code(F01.17 Reserved)：0
05/03/2024 11:05:47 Read function code(F01.18 Reserved)：0
05/03/2024 11:05:47 Read function code(F01.19 Reserved)：0
05/03/2024 11:05:47 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:05:47 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:05:47 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:05:47 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:05:47 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:05:47 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:05:48 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:05:48 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:05:48 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:05:48 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:05:48 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:05:48 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:05:48 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:05:48 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:05:48 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:05:48 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:05:48 Read function code(F01.36 Reserved)：0
05/03/2024 11:05:48 Read function code(F01.37 Reserved)：0
05/03/2024 11:05:48 Read function code(F01.38 Reserved)：0
05/03/2024 11:05:48 Read function code(F01.39 Reserved)：0
05/03/2024 11:05:48 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:05:48 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:05:48 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:05:48 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:05:48 Read function code(F01.44 Reserved)：15
05/03/2024 11:05:48 Read function code(F01.45 Reserved)：50
05/03/2024 11:05:48 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:05:48 Read function code(F01.47 Reserved)：0
05/03/2024 11:05:48 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:05:48 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:07:00 Set function code(F01.00 Motor 1 way to control )：0-->1:AM Open loop vector 
05/03/2024 11:07:00 Set function code(F01.01 Run command channel)：0-->1:Terminal control 
05/03/2024 11:07:01 Set function code(F01.02 Frequency given source channel A)：0-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:07:02 Read function code(F01.00 Motor 1 way to control )：1:AM Open loop vector 
05/03/2024 11:07:02 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:07:02 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:07:02 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:07:03 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:07:03 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:07:03 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:07:03 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:07:03 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:07:03 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:07:03 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:07:03 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:07:03 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:07:03 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:07:03 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:07:03 Read function code(F01.15 Reserved)：0
05/03/2024 11:07:03 Read function code(F01.16 Reserved)：0
05/03/2024 11:07:03 Read function code(F01.17 Reserved)：0
05/03/2024 11:07:03 Read function code(F01.18 Reserved)：0
05/03/2024 11:07:03 Read function code(F01.19 Reserved)：0
05/03/2024 11:07:03 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:07:03 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:07:03 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:07:03 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:07:03 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:07:03 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:07:03 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:07:03 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:07:03 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:07:03 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:07:03 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:07:03 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:07:03 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:07:04 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:07:04 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:07:04 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:07:04 Read function code(F01.36 Reserved)：0
05/03/2024 11:07:04 Read function code(F01.37 Reserved)：0
05/03/2024 11:07:04 Read function code(F01.38 Reserved)：0
05/03/2024 11:07:04 Read function code(F01.39 Reserved)：0
05/03/2024 11:07:04 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:07:04 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:07:04 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:07:04 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:07:04 Read function code(F01.44 Reserved)：15
05/03/2024 11:07:04 Read function code(F01.45 Reserved)：50
05/03/2024 11:07:04 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:07:04 Read function code(F01.47 Reserved)：0
05/03/2024 11:07:04 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:07:04 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:07:47 Set function code(F01.00 Motor 1 way to control )：1-->0:AM VF control 
05/03/2024 11:10:12 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:10:12 Set function code(F01.00 Motor 1 way to control )：0-->0:AM VF control 
05/03/2024 11:10:12 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:10:13 Set function code(F01.02 Frequency given source channel A)：1-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:10:13 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:10:13 Set function code(F01.04 Frequency given source channel B)：6-->6:RS485 communication setting
05/03/2024 11:10:13 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->10.0
05/03/2024 11:10:13 Set function code(F01.06 Frequency channel B reference source)：1-->1:Take A set frequency as reference source 
05/03/2024 11:10:13 Set function code(F01.07 Frequency given source selection)：1-->1:Channel B
05/03/2024 11:10:13 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:10:13 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:10:13 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:10:13 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:10:13 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:10:13 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:10:13 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:10:13 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:10:13 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:10:13 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:10:13 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:10:13 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:10:13 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:10:13 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:10:13 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:10:13 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:10:13 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:10:13 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:10:13 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:10:13 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:10:13 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:10:13 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:10:14 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:10:14 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:10:14 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:10:14 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:10:14 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:10:14 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:10:14 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:10:14 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:10:14 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:10:14 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:10:14 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:10:14 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:10:14 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:10:14 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:10:14 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:10:14 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:10:14 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:10:14 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:10:14 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:11:09 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:11:09 Set function code(F01.00 Motor 1 way to control )：0-->0:AM VF control 
05/03/2024 11:11:09 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:11:09 Set function code(F01.02 Frequency given source channel A)：1-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:11:09 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:11:09 Set function code(F01.04 Frequency given source channel B)：6-->6:RS485 communication setting
05/03/2024 11:11:09 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->10.0
05/03/2024 11:11:09 Set function code(F01.06 Frequency channel B reference source)：1-->1:Take A set frequency as reference source 
05/03/2024 11:11:09 Set function code(F01.07 Frequency given source selection)：1-->1:Channel B
05/03/2024 11:11:09 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:11:09 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:11:09 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:11:09 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:11:09 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:11:09 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:11:09 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:11:09 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:11:09 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:11:10 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:11:10 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:11:10 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:11:10 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:11:10 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:11:10 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:11:10 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:11:10 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:11:10 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:11:10 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:11:10 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:11:10 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:11:10 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:11:10 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:11:10 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:11:10 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:11:11 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:11:11 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:11:11 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:11:11 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:11:11 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:11:11 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:11:11 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:11:11 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:11:11 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:11:11 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:11:11 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:11:11 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:11:11 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:11:11 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:11:11 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:11:11 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:11:11 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:11:11 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:11:11 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:11:11 Read function code(F01.15 Reserved)：0
05/03/2024 11:11:11 Read function code(F01.16 Reserved)：0
05/03/2024 11:11:11 Read function code(F01.17 Reserved)：0
05/03/2024 11:11:11 Read function code(F01.18 Reserved)：0
05/03/2024 11:11:11 Read function code(F01.19 Reserved)：0
05/03/2024 11:11:11 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:11:11 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:11:11 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:11:11 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:11:11 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:11:12 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:11:12 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:11:12 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:11:12 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:11:12 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:11:12 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:11:12 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:11:12 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:11:12 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:11:12 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:11:12 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:11:12 Read function code(F01.36 Reserved)：0
05/03/2024 11:11:12 Read function code(F01.37 Reserved)：0
05/03/2024 11:11:12 Read function code(F01.38 Reserved)：0
05/03/2024 11:11:12 Read function code(F01.39 Reserved)：0
05/03/2024 11:11:12 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:11:12 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:11:12 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:11:12 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:11:12 Read function code(F01.44 Reserved)：15
05/03/2024 11:11:12 Read function code(F01.45 Reserved)：50
05/03/2024 11:11:12 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:11:12 Read function code(F01.47 Reserved)：0
05/03/2024 11:11:12 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:11:12 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:11:16 Send the function code of the current page(F01 Basic command) Batch write instructions
05/03/2024 11:11:16 Set function code(F01.00 Motor 1 way to control )：0-->0:AM VF control 
05/03/2024 11:11:16 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:11:16 Set function code(F01.02 Frequency given source channel A)：1-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:11:16 Set function code(F01.03 Frequency given source channel A gain)：0.0-->0.0
05/03/2024 11:11:16 Set function code(F01.04 Frequency given source channel B)：6-->6:RS485 communication setting
05/03/2024 11:11:16 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->10.0
05/03/2024 11:11:16 Set function code(F01.06 Frequency channel B reference source)：1-->1:Take A set frequency as reference source 
05/03/2024 11:11:16 Set function code(F01.07 Frequency given source selection)：1-->1:Channel B
05/03/2024 11:11:16 Set function code(F01.08 Run command bundle )：0000-->0000
05/03/2024 11:11:16 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->50.00
05/03/2024 11:11:16 Set function code(F01.10 Maximum frequency )：50.00-->50.00
05/03/2024 11:11:16 Set function code(F01.11 Upper frequency source selection)：0-->0:Upper limit frequency digital given
05/03/2024 11:11:16 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->50.00
05/03/2024 11:11:16 Set function code(F01.13 Lower limit frequency )：0.00-->0.00
05/03/2024 11:11:16 Set function code(F01.14 Frequency Instruction Resolution)：0-->0:0.01Hz
05/03/2024 11:11:16 Set function code(F01.15 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.16 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.17 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.18 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.19 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->0:Maximum frequency 
05/03/2024 11:11:17 Set function code(F01.21 Acceleration time unit)：2-->2:0.01S
05/03/2024 11:11:17 Set function code(F01.22 Acceleration time 1)：6.00-->6.00
05/03/2024 11:11:17 Set function code(F01.23 Deceleration time 1)：6.00-->6.00
05/03/2024 11:11:17 Set function code(F01.24 Acceleration time 2)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.25 Deceleration time 2)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.26 Acceleration time 3)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.27 Deceleration time 3)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.28 Acceleration time 4)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.29 Deceleration time 4)：10.00-->10.00
05/03/2024 11:11:17 Set function code(F01.30 S Curve acceleration and deceleration selection )：1-->1
05/03/2024 11:11:17 Set function code(F01.31 Acceleration start S-curve time )：0.20-->0.20
05/03/2024 11:11:17 Set function code(F01.32 Acceleration end S curve time )：0.20-->0.20
05/03/2024 11:11:17 Set function code(F01.33 S-curve time to start deceleration )：0.20-->0.20
05/03/2024 11:11:17 Set function code(F01.34 S-curve time at the end of deceleration)：0.20-->0.20
05/03/2024 11:11:17 Set function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00-->0.00
05/03/2024 11:11:17 Set function code(F01.36 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.37 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.38 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.39 Reserved)：0-->0
05/03/2024 11:11:17 Set function code(F01.40 PWM Carrier frequency )：4.0-->4.0
05/03/2024 11:11:17 Set function code(F01.41 PWM Control mode )：1111-->1111
05/03/2024 11:11:17 Set function code(F01.42 PWM way to control 1)：9101-->9101
05/03/2024 11:11:17 Set function code(F01.43 Dead zone compensation gain )：306-->306
05/03/2024 11:11:18 Set function code(F01.44 Reserved)：15-->15
05/03/2024 11:11:18 Set function code(F01.45 Reserved)：50-->50
05/03/2024 11:11:18 Set function code(F01.46 Random carrier depth )：0-->0
05/03/2024 11:11:18 Set function code(F01.48 Reserved)：0.00-->0.00
05/03/2024 11:11:18 Set function code(F01.49 Reserved)：6.0-->6.0
05/03/2024 11:11:18 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:11:18 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:11:18 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:11:18 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:11:18 Read function code(F01.04 Frequency given source channel B)：6:RS485 communication setting
05/03/2024 11:11:18 Read function code(F01.05 Frequency given source channel B  gain)：10.0
05/03/2024 11:11:18 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:11:18 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:11:18 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:11:18 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:11:18 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:11:18 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:11:18 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:11:18 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:11:18 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:11:18 Read function code(F01.15 Reserved)：0
05/03/2024 11:11:18 Read function code(F01.16 Reserved)：0
05/03/2024 11:11:18 Read function code(F01.17 Reserved)：0
05/03/2024 11:11:18 Read function code(F01.18 Reserved)：0
05/03/2024 11:11:18 Read function code(F01.19 Reserved)：0
05/03/2024 11:11:18 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:11:18 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:11:19 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:11:19 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:11:19 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:11:19 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:11:19 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:11:19 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:11:19 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:11:19 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:11:19 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:11:19 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:11:19 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:11:19 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:11:19 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:11:19 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:11:19 Read function code(F01.36 Reserved)：0
05/03/2024 11:11:19 Read function code(F01.37 Reserved)：0
05/03/2024 11:11:19 Read function code(F01.38 Reserved)：0
05/03/2024 11:11:19 Read function code(F01.39 Reserved)：0
05/03/2024 11:11:19 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:11:19 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:11:19 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:11:19 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:11:19 Read function code(F01.44 Reserved)：15
05/03/2024 11:11:19 Read function code(F01.45 Reserved)：50
05/03/2024 11:11:19 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:11:19 Read function code(F01.47 Reserved)：0
05/03/2024 11:11:19 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:11:19 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:14:25 Set function code(F01.00 Motor 1 way to control )：0-->1:AM Open loop vector 
05/03/2024 11:14:27 Set function code(F01.01 Run command channel)：1-->1:Terminal control 
05/03/2024 11:14:27 Set function code(F01.02 Frequency given source channel A)：1-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:14:27 Set function code(F01.03 Frequency given source channel A gain)：0.0-->1.0
05/03/2024 11:14:28 Set function code(F01.04 Frequency given source channel B)：6-->10:Option card 
05/03/2024 11:14:28 Set function code(F01.05 Frequency given source channel B  gain)：10.0-->1.0
05/03/2024 11:14:33 Set function code(F01.04 Frequency given source channel B)：10-->1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:14:37 Set function code(F01.08 Run command bundle )：0000-->1111
05/03/2024 11:14:39 Set function code(F01.09 Keyboard numbers  Setting  frequency )：50.00-->1.00
05/03/2024 11:14:39 Set function code(F01.10 Maximum frequency )：50.00-->1.00
05/03/2024 11:14:40 Set function code(F01.11 Upper frequency source selection)：0-->1:Reserved
05/03/2024 11:14:41 Set function code(F01.12 Digital setting of upper limit frequency)：50.00-->1.00
05/03/2024 11:14:41 Set function code(F01.13 Lower limit frequency )：0.00-->1.00
05/03/2024 11:14:42 Set function code(F01.14 Frequency Instruction Resolution)：0-->1:0.1Hz
05/03/2024 11:14:42 Set function code(F01.20 Base frequency of acceleration and deceleration time )：0-->1:Fixed frequency 50Hz
05/03/2024 11:14:42 Set function code(F01.21 Acceleration time unit)：2-->1:0.1S
05/03/2024 11:14:42 Set function code(F01.22 Acceleration time 1)：6.00-->1.00
05/03/2024 11:14:45 Communication(COM3)Disconnected
05/03/2024 11:14:46 Communication(COM3)Connection succeeded
05/03/2024 11:14:47 Read function code(F01.00 Motor 1 way to control )：1:AM Open loop vector 
05/03/2024 11:14:47 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:14:47 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:14:47 Read function code(F01.03 Frequency given source channel A gain)：1.0
05/03/2024 11:14:47 Read function code(F01.04 Frequency given source channel B)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:14:47 Read function code(F01.05 Frequency given source channel B  gain)：1.0
05/03/2024 11:14:47 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:14:47 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:14:47 Read function code(F01.08 Run command bundle )：1111
05/03/2024 11:14:47 Read function code(F01.09 Keyboard numbers  Setting  frequency )：1.00
05/03/2024 11:14:47 Read function code(F01.10 Maximum frequency )：1.00
05/03/2024 11:14:47 Read function code(F01.11 Upper frequency source selection)：1:Reserved
05/03/2024 11:14:48 Read function code(F01.12 Digital setting of upper limit frequency)：1.00
05/03/2024 11:14:48 Read function code(F01.13 Lower limit frequency )：1.00
05/03/2024 11:14:48 Read function code(F01.14 Frequency Instruction Resolution)：1:0.1Hz
05/03/2024 11:14:48 Read function code(F01.15 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.16 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.17 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.18 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.19 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.20 Base frequency of acceleration and deceleration time )：1:Fixed frequency 50Hz
05/03/2024 11:14:48 Read function code(F01.21 Acceleration time unit)：1:0.1S
05/03/2024 11:14:48 Read function code(F01.22 Acceleration time 1)：1.00
05/03/2024 11:14:48 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:14:48 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:14:48 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:14:48 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:14:48 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:14:48 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:14:48 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:14:48 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:14:48 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:14:48 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:14:48 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:14:48 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:14:48 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:14:48 Read function code(F01.36 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.37 Reserved)：0
05/03/2024 11:14:48 Read function code(F01.38 Reserved)：0
05/03/2024 11:14:49 Read function code(F01.39 Reserved)：0
05/03/2024 11:14:49 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:14:49 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:14:49 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:14:49 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:14:49 Read function code(F01.44 Reserved)：15
05/03/2024 11:14:49 Read function code(F01.45 Reserved)：50
05/03/2024 11:14:49 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:14:49 Read function code(F01.47 Reserved)：0
05/03/2024 11:14:49 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:14:49 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:15:03 Read function code(C00.00 Given frequency)：1.00
05/03/2024 11:15:03 Read function code(C00.01 Output frequency)：0.00
05/03/2024 11:15:03 Read function code(C00.02 Output current)：0.0
05/03/2024 11:15:03 Read function code(C00.03 Input voltage)：381.5
05/03/2024 11:15:03 Read function code(C00.04 Output voltage)：0.0
05/03/2024 11:15:03 Read function code(C00.05 Mechanical speed)：0
05/03/2024 11:15:03 Read function code(C00.06 Given torque)：250.0
05/03/2024 11:15:03 Read function code(C00.07 Output torque)：0.0
05/03/2024 11:15:04 Read function code(C00.08 PID Given amount)：0.0
05/03/2024 11:15:04 Read function code(C00.09 PID Feedback amount)：0.0
05/03/2024 11:15:04 Read function code(C00.10 Output Power)：0.0
05/03/2024 11:15:04 Read function code(C00.11 Bus voltage)：540.2
05/03/2024 11:15:04 Read function code(C00.12 Module temperature1)：23.4
05/03/2024 11:15:04 Read function code(C00.13 Module temperature2)：23.4
05/03/2024 11:15:04 Read function code(C00.14 Input terminal X connected state)：00000000
05/03/2024 11:15:04 Read function code(C00.15 Output terminal Y connected state)：00000000
05/03/2024 11:15:04 Read function code(C00.16 Analog AI1 input value)：7.547
05/03/2024 11:15:04 Read function code(C00.17 Analog AI2 input value)：0.000
05/03/2024 11:15:04 Read function code(C00.18 Keyboard potentiometer)：0.00
05/03/2024 11:15:04 Read function code(C00.19 Pulse signal PUL input value)：0.000
05/03/2024 11:15:04 Read function code(C00.20 Analog output AO1)：10.00
05/03/2024 11:15:04 Read function code(C00.21 Analog output AO2 (extended))：0.00
05/03/2024 11:15:04 Read function code(C00.22 Counter count value)：0
05/03/2024 11:15:04 Read function code(C00.23 Running time of this power-on)：0.0
05/03/2024 11:15:04 Read function code(C00.24 Accumulated running time of this machine)：0
05/03/2024 11:15:04 Read function code(C00.25 Inverter power rated power)：2.2
05/03/2024 11:15:04 Read function code(C00.26 Inverter rated voltage)：380
05/03/2024 11:15:04 Read function code(C00.27 Inverter rated current)：6.0
05/03/2024 11:15:04 Read function code(C00.28 Software version)：60.20
05/03/2024 11:15:04 Read function code(C00.29 PGFeedback frequency)：0.00
05/03/2024 11:15:04 Read function code(C00.30 Timer )：0
05/03/2024 11:15:04 Read function code(C00.31 PID output )：0.00
05/03/2024 11:15:04 Read function code(C00.32 Software subversion)：9.92
05/03/2024 11:15:04 Read function code(C00.33 Encoder angle)：0.00
05/03/2024 11:15:04 Read function code(C00.34 Z pulse error)：0
05/03/2024 11:15:05 Read function code(C00.35 Z pulse count)：0
05/03/2024 11:15:05 Read function code(C00.36 Fault warning code)：0:No failure
05/03/2024 11:15:05 Read function code(C00.37 Cumulative power consumption (low level))：0
05/03/2024 11:15:05 Read function code(C00.38 Accumulated electricity consumption (high　level))：0
05/03/2024 11:15:05 Read function code(C00.39 Power factor angle)：0.0
05/03/2024 11:15:05 Read function code(C00.40)：0
05/03/2024 11:15:05 Read function code(C00.41)：0
05/03/2024 11:15:05 Read function code(C00.42)：0
05/03/2024 11:15:05 Read function code(C00.43)：0
05/03/2024 11:15:05 Read function code(C00.44)：0
05/03/2024 11:15:05 Read function code(C00.45)：0
05/03/2024 11:15:05 Read function code(C00.46)：0
05/03/2024 11:15:05 Read function code(C00.47)：0
05/03/2024 11:15:05 Read function code(C00.48)：0
05/03/2024 11:15:05 Read function code(C00.49)：0
05/03/2024 11:15:05 Read function code(C00.50)：0
05/03/2024 11:15:05 Read function code(C00.51)：0
05/03/2024 11:15:05 Read function code(C00.52)：0
05/03/2024 11:15:05 Read function code(C00.53)：0
05/03/2024 11:15:05 Read function code(C00.54)：30000
05/03/2024 11:15:05 Read function code(C00.55)：0
05/03/2024 11:15:05 Read function code(C00.56)：0
05/03/2024 11:15:05 Read function code(C00.57)：55
05/03/2024 11:15:05 Read function code(C00.58)：65458
05/03/2024 11:15:05 Read function code(C00.59)：77
05/03/2024 11:15:05 Read function code(C00.60)：5336
05/03/2024 11:15:05 Read function code(C00.61)：0
05/03/2024 11:15:06 Read function code(C00.62)：0
05/03/2024 11:15:06 Read function code(C00.63)：0
05/03/2024 11:15:06 Read function code(C01.00 Fault type)：10
05/03/2024 11:15:06 Read function code(C01.01 Faults diagnostic information)：1002
05/03/2024 11:15:06 Read function code(C01.02 Faults operation frequency)：3.85
05/03/2024 11:15:06 Read function code(C01.03 Faults output voltage)：107.6
05/03/2024 11:15:06 Read function code(C01.04 Faults output current)：1.5
05/03/2024 11:15:06 Read function code(C01.05 Faults bus voltage)：820.5
05/03/2024 11:15:06 Read function code(C01.06 Faults module temperature)：27.9
05/03/2024 11:15:06 Read function code(C01.07 Faulty inverter status)：1320
05/03/2024 11:15:06 Read function code(C01.08 Fault input terminal status)：00000000
05/03/2024 11:15:06 Read function code(C01.09 Fault output terminal status)：10000000
05/03/2024 11:15:06 Read function code(C01.10 Last time fault type)：13
05/03/2024 11:15:06 Read function code(C01.11 Faults diagnostic information)：1300
05/03/2024 11:15:06 Read function code(C01.12 Last time fault operation frequency)：0.50
05/03/2024 11:15:06 Read function code(C01.13 Previous failure output voltage)：47.9
05/03/2024 11:15:06 Read function code(C01.14 Previous failure output current)：2.0
05/03/2024 11:15:06 Read function code(C01.15 Previous failure bus voltage)：318.8
05/03/2024 11:15:06 Read function code(C01.16 Previous failure module temperature)：27.9
05/03/2024 11:15:06 Read function code(C01.17 Last time faulty inverter status)：2330
05/03/2024 11:15:06 Read function code(C01.18 Last time fault input terminal status)：10000000
05/03/2024 11:15:06 Read function code(C01.19 Last time fault output terminal status)：10000000
05/03/2024 11:15:06 Read function code(C01.20 The first two times fault type)：0
05/03/2024 11:15:06 Read function code(C01.21 Faults diagnostic information)：0
05/03/2024 11:15:06 Read function code(C01.22 The first three times fault type)：0
05/03/2024 11:15:06 Read function code(C01.23 Faults diagnostic information)：0
05/03/2024 11:15:06 Read function code(F00.00 Parameter access level )：0:Standard parameter 
05/03/2024 11:15:07 Read function code(F00.01 Purpose selection)：0:Universal 
05/03/2024 11:15:07 Read function code(F00.02 Motor selection)：0
05/03/2024 11:15:07 Read function code(F00.03 Initialization)：0:Not initialized 
05/03/2024 11:15:07 Read function code(F00.04 Keyboard parameter copy)：0:No function 
05/03/2024 11:15:07 Read function code(F00.05 User password)：0000
05/03/2024 11:15:07 Read function code(F00.06 LCD keyboard language selection)：0
05/03/2024 11:15:07 Read function code(F00.07 Free parameters 1)：0
05/03/2024 11:15:07 Read function code(F00.08 Free parameters 2)：0
05/03/2024 11:15:07 Read function code(F00.09 Reserved)：0
05/03/2024 11:15:07 Read function code(F00.10 Common parameters 1Address setting)：0100
05/03/2024 11:15:07 Read function code(F00.11 Common parameters 2Address setting)：0101
05/03/2024 11:15:07 Read function code(F00.12 Common parameters 3Address setting)：0102
05/03/2024 11:15:07 Read function code(F00.13 Common parameters 4Address setting)：0710
05/03/2024 11:15:07 Read function code(F00.14 Common parameters 5Address setting)：0122
05/03/2024 11:15:07 Read function code(F00.15 Common parameters 6Address setting)：0123
05/03/2024 11:15:07 Read function code(F00.16 Common parameters 7Address setting)：0110
05/03/2024 11:15:07 Read function code(F00.17 Common parameters 8Address setting)：0112
05/03/2024 11:15:07 Read function code(F00.18 Common parameters 9Address setting)：0140
05/03/2024 11:15:07 Read function code(F00.19 Common parameters 10Address setting)：0730
05/03/2024 11:15:07 Read function code(F00.20 Common parameters 11Address setting)：0201
05/03/2024 11:15:07 Read function code(F00.21 Common parameters 12Address setting)：0202
05/03/2024 11:15:07 Read function code(F00.22 Common parameters 13Address setting)：0203
05/03/2024 11:15:07 Read function code(F00.23 Common parameters 14Address setting)：0204
05/03/2024 11:15:07 Read function code(F00.24 Common parameters 15Address setting)：0205
05/03/2024 11:15:07 Read function code(F00.25 Common parameters 16Address setting)：0206
05/03/2024 11:15:07 Read function code(F00.26 Common parameters 17Address setting)：0207
05/03/2024 11:15:08 Read function code(F00.27 Common parameters 18Address setting)：1201
05/03/2024 11:15:08 Read function code(F00.28 Common parameters 19Address setting)：1202
05/03/2024 11:15:08 Read function code(F00.29 Common parameters 20Address setting)：1203
05/03/2024 11:15:08 Read function code(F00.30 Common parameters 21Address setting)：0700
05/03/2024 11:15:08 Read function code(F00.31 Common parameters 22Address setting)：0705
05/03/2024 11:15:08 Read function code(F00.32 Common parameters 23Address setting)：0502
05/03/2024 11:15:08 Read function code(F00.33 Common parameters 24Address setting)：0503
05/03/2024 11:15:08 Read function code(F00.34 Common parameters 25Address setting)：0504
05/03/2024 11:15:08 Read function code(F00.35 Common parameters 26Address setting)：0601
05/03/2024 11:15:08 Read function code(F00.36 Common parameters 27Address setting)：0600
05/03/2024 11:15:08 Read function code(F00.37 Common parameters 28Address setting)：0621
05/03/2024 11:15:08 Read function code(F00.38 Common parameters 29Address setting)：0622
05/03/2024 11:15:08 Read function code(F00.39 Common parameters 30Address setting)：0400
05/03/2024 11:15:08 Read function code(F00.40 Single board debugging options)：0000
05/03/2024 11:15:08 Read function code(F00.41 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.42 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.43 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.44 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.45 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.46 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.47 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.48 Reserved)：0
05/03/2024 11:15:08 Read function code(F00.49 Reserved)：0
05/03/2024 11:15:08 Read function code(F01.00 Motor 1 way to control )：1:AM Open loop vector 
05/03/2024 11:15:08 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:15:08 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:15:08 Read function code(F01.03 Frequency given source channel A gain)：1.0
05/03/2024 11:15:09 Read function code(F01.04 Frequency given source channel B)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:15:09 Read function code(F01.05 Frequency given source channel B  gain)：1.0
05/03/2024 11:15:09 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:15:09 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:15:09 Read function code(F01.08 Run command bundle )：1111
05/03/2024 11:15:09 Read function code(F01.09 Keyboard numbers  Setting  frequency )：1.00
05/03/2024 11:15:09 Read function code(F01.10 Maximum frequency )：1.00
05/03/2024 11:15:09 Read function code(F01.11 Upper frequency source selection)：1:Reserved
05/03/2024 11:15:09 Read function code(F01.12 Digital setting of upper limit frequency)：1.00
05/03/2024 11:15:09 Read function code(F01.13 Lower limit frequency )：1.00
05/03/2024 11:15:09 Read function code(F01.14 Frequency Instruction Resolution)：1:0.1Hz
05/03/2024 11:15:09 Read function code(F01.15 Reserved)：0
05/03/2024 11:15:09 Read function code(F01.16 Reserved)：0
05/03/2024 11:15:09 Read function code(F01.17 Reserved)：0
05/03/2024 11:15:09 Read function code(F01.18 Reserved)：0
05/03/2024 11:15:09 Read function code(F01.19 Reserved)：0
05/03/2024 11:15:09 Read function code(F01.20 Base frequency of acceleration and deceleration time )：1:Fixed frequency 50Hz
05/03/2024 11:15:09 Read function code(F01.21 Acceleration time unit)：1:0.1S
05/03/2024 11:15:09 Read function code(F01.22 Acceleration time 1)：1.00
05/03/2024 11:15:09 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:15:09 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:15:09 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:15:09 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:15:09 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:15:09 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:15:10 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:15:10 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:15:10 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:15:10 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:15:10 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:15:10 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:15:10 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:15:10 Read function code(F01.36 Reserved)：0
05/03/2024 11:15:10 Read function code(F01.37 Reserved)：0
05/03/2024 11:15:10 Read function code(F01.38 Reserved)：0
05/03/2024 11:15:10 Read function code(F01.39 Reserved)：0
05/03/2024 11:15:10 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:15:10 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:15:10 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:15:10 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:15:10 Read function code(F01.44 Reserved)：15
05/03/2024 11:15:10 Read function code(F01.45 Reserved)：50
05/03/2024 11:15:10 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:15:10 Read function code(F01.47 Reserved)：0
05/03/2024 11:15:10 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:15:10 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:15:10 Read function code(F02.00 Motor  type )：0:Asynchronous motor （AM）
05/03/2024 11:15:10 Read function code(F02.01 Motor poles)：4
05/03/2024 11:15:10 Read function code(F02.02 Motor rated power)：2.2
05/03/2024 11:15:10 Read function code(F02.03 Motor rated frequency )：50.00
05/03/2024 11:15:11 Read function code(F02.04 Motor rated speed)：1500
05/03/2024 11:15:11 Read function code(F02.05 Motor rated voltage )：380
05/03/2024 11:15:11 Read function code(F02.06 Motor rated current )：5.0
05/03/2024 11:15:11 Read function code(F02.07 Motor parameter self tuning selection)：0:No operation 
05/03/2024 11:15:11 Read function code(F02.08 Self-learning sign )：0000
05/03/2024 11:15:11 Read function code(F02.09 Reserved)：0
05/03/2024 11:15:11 Read function code(F02.10 Asynchronous motor  No-load current )：1.9
05/03/2024 11:15:11 Read function code(F02.11 Asynchronous motor  Stator resistance )：3201
05/03/2024 11:15:11 Read function code(F02.12 Asynchronous motor  Rotor resistance )：2631
05/03/2024 11:15:11 Read function code(F02.13 Asynchronous motor  Stator leakage inductance )：1257
05/03/2024 11:15:11 Read function code(F02.14 Asynchronous motor  Stator inductance)：3518
05/03/2024 11:15:11 Read function code(F02.15 Stator resistance per unit value )：7.29
05/03/2024 11:15:11 Read function code(F02.16 Rotor resistance per unit value )：5.99
05/03/2024 11:15:11 Read function code(F02.17 Stator leakage inductance per unit value)：50.00
05/03/2024 11:15:11 Read function code(F02.18 Stator inductance per unit value )：900.0
05/03/2024 11:15:11 Read function code(F02.19 Actual value unit selection )：1200
05/03/2024 11:15:11 Read function code(F02.20 Synchronous motor stator resistance )：1315
05/03/2024 11:15:11 Read function code(F02.21 Synchronous machine d-axis inductance )：13.96
05/03/2024 11:15:11 Read function code(F02.22 Synchronous machine q-axis inductance )：13.96
05/03/2024 11:15:11 Read function code(F02.23 Synchronous Back EMF)：285
05/03/2024 11:15:11 Read function code(F02.24 Synchronous machine encoder installation angle )：0.0
05/03/2024 11:15:11 Read function code(F02.25 Synchronous motor Stator resistance per unit value )：2.99
05/03/2024 11:15:11 Read function code(F02.26 Synchronous machine d-axis inductance per-unit value )：99.97
05/03/2024 11:15:11 Read function code(F02.27 Synchronous machine q-axis inductance per-unit value )：99.97
05/03/2024 11:15:11 Read function code(F02.28 Synchronous  Motor Pulse width coefficient)：4050
05/03/2024 11:15:12 Read function code(F02.29 Actual value unit selection )：0220
05/03/2024 11:15:12 Read function code(F02.30 Speed feedback or encoder type)：0:Ordinary ABZ encoder +AC300PG01 card +EX_B
05/03/2024 11:15:12 Read function code(F02.31 Encoder direction)：0:Same direction 
05/03/2024 11:15:12 Read function code(F02.32 ABZ encoder Z pulse detection selection)：1:Turn on forward detection
05/03/2024 11:15:12 Read function code(F02.33 ABZ Encoder line number )：1024
05/03/2024 11:15:12 Read function code(F02.34 Number of poles of resolver )：2
05/03/2024 11:15:12 Read function code(F02.35 Encoder transmission ratio numerator )：1
05/03/2024 11:15:12 Read function code(F02.36 Encoder transmission ratio denominator )：1
05/03/2024 11:15:12 Read function code(F02.37 Encoder speed measurement filter time )：1.0
05/03/2024 11:15:12 Read function code(F02.38 Encoder disconnection Check out time )：0.050
05/03/2024 11:15:12 Read function code(F02.39 Reserved)：1
05/03/2024 11:15:12 Read function code(F02.40 Reserved)：0
05/03/2024 11:15:12 Read function code(F02.41 Reserved)：0
05/03/2024 11:15:12 Read function code(F02.42 Reserved)：1
05/03/2024 11:15:12 Read function code(F02.43 Reserved)：1024
05/03/2024 11:15:12 Read function code(F02.44 Reserved)：1.0
05/03/2024 11:15:12 Read function code(F02.45 Reserved)：0010
05/03/2024 11:15:12 Read function code(F02.46 Reserved)：4
05/03/2024 11:15:12 Read function code(F02.47 Z Pulse tolerance)：0
05/03/2024 11:15:12 Read function code(F02.48 Z Pulse learning current )：0
05/03/2024 11:15:12 Read function code(F02.49 Encoder debug register)：0000
05/03/2024 11:15:12 Read function code(F02.50 Motor Online learning function selection)：0:Invalid 
05/03/2024 11:15:12 Read function code(F02.51 Stator resistance start learning coefficient 1)：0
05/03/2024 11:15:12 Read function code(F02.52 Stator resistance start learning coefficient 2)：0.00
05/03/2024 11:15:12 Read function code(F02.53 Stator resistance start learning coefficient 3)：0
05/03/2024 11:15:12 Read function code(F02.54 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.55 ASR Learning frequency )：60.0
05/03/2024 11:15:13 Read function code(F02.56 ASR Learning acceleration and deceleration time )：1.00
05/03/2024 11:15:13 Read function code(F02.57 ASR Learning acceleration and deceleration times )：4
05/03/2024 11:15:13 Read function code(F02.58 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.59 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.60 Synchronous motor magnetic pole search function )：0010
05/03/2024 11:15:13 Read function code(F02.61 Magnetic pole search current setting value )：0.0
05/03/2024 11:15:13 Read function code(F02.62 Magnetic pole search current feedback value )：0.0
05/03/2024 11:15:13 Read function code(F02.63 PM Motor inductance learning frequency )：300.00
05/03/2024 11:15:13 Read function code(F02.64 PM Motor inductance learning current )：0
05/03/2024 11:15:13 Read function code(F02.65 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.66 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.67 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.68 Reserved)：300
05/03/2024 11:15:13 Read function code(F02.69 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.70 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.71 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.72 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.73 Reserved)：1024
05/03/2024 11:15:13 Read function code(F02.74 Reserved)：1024
05/03/2024 11:15:13 Read function code(F02.75 Reserved)：90.0
05/03/2024 11:15:13 Read function code(F02.76 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.77 Reserved)：0.00
05/03/2024 11:15:13 Read function code(F02.78 Reserved)：3
05/03/2024 11:15:13 Read function code(F02.79 Reserved)：0
05/03/2024 11:15:13 Read function code(F02.80 _LQCoef0)：100.0
05/03/2024 11:15:14 Read function code(F02.81)：100.0
05/03/2024 11:15:14 Read function code(F02.82)：100.0
05/03/2024 11:15:14 Read function code(F02.83)：100.0
05/03/2024 11:15:14 Read function code(F02.84)：100.0
05/03/2024 11:15:14 Read function code(F02.85)：100.0
05/03/2024 11:15:14 Read function code(F02.86)：100.0
05/03/2024 11:15:14 Read function code(F02.87)：100.0
05/03/2024 11:15:14 Read function code(F02.88)：100.0
05/03/2024 11:15:14 Read function code(F02.89)：100.0
05/03/2024 11:15:14 Read function code(F02.90)：100.0
05/03/2024 11:15:14 Read function code(F02.91)：100.0
05/03/2024 11:15:14 Read function code(F02.92)：100.0
05/03/2024 11:15:14 Read function code(F02.93)：100.0
05/03/2024 11:15:14 Read function code(F02.94)：100.0
05/03/2024 11:15:14 Read function code(F02.95)：100.0
05/03/2024 11:15:14 Read function code(F02.96)：100.0
05/03/2024 11:15:14 Read function code(F02.97)：100.0
05/03/2024 11:15:14 Read function code(F02.98)：100.0
05/03/2024 11:15:14 Read function code(F02.99)：100.0
05/03/2024 11:15:14 Read function code(F03.00 ASR Speed ​​rigidity level )：32
05/03/2024 11:15:14 Read function code(F03.01 ASR Speed ​​rigid mode )：0000
05/03/2024 11:15:14 Read function code(F03.02 ASR (Speed ​​loop) Proportional gain 1)：10.00
05/03/2024 11:15:14 Read function code(F03.03 ASR (Speed ​​loop) Integration time 1)：0.100
05/03/2024 11:15:14 Read function code(F03.04 ASR Filter time 1)：0.0
05/03/2024 11:15:14 Read function code(F03.05 ASR Switching frequency 1)：0.00
05/03/2024 11:15:15 Read function code(F03.06 ASR (Speed ​​loop) Proportional gain 2)：10.00
05/03/2024 11:15:15 Read function code(F03.07 ASR (Speed ​​loop) Integration time 2)：0.100
05/03/2024 11:15:15 Read function code(F03.08 ASR Filter time 2)：0.0
05/03/2024 11:15:15 Read function code(F03.09 ASR Switching frequency 2)：0.00
05/03/2024 11:15:15 Read function code(F03.10 Current loop D axis proportional gain )：1.000
05/03/2024 11:15:15 Read function code(F03.11 Current loop D axis integral gain )：1.000
05/03/2024 11:15:15 Read function code(F03.12 Current loop Q axis proportional gain )：1.000
05/03/2024 11:15:15 Read function code(F03.13 Current loop Q axis integral gain )：1.000
05/03/2024 11:15:15 Read function code(F03.14 Current loop optimized configuration )：0000
05/03/2024 11:15:15 Read function code(F03.15 Motor torque limit )：250.0
05/03/2024 11:15:15 Read function code(F03.16 Torque limit in power generation state )：250.0
05/03/2024 11:15:15 Read function code(F03.17 Regenerative torque limit value at low speed )：0.0
05/03/2024 11:15:15 Read function code(F03.18 Torque limit action frequency range at low speed )：6.00
05/03/2024 11:15:15 Read function code(F03.19 Torque limit selection )：0000
05/03/2024 11:15:15 Read function code(F03.20 Synchronous motor pulls in current at low frequency )：20.0
05/03/2024 11:15:15 Read function code(F03.21 Synchronous motor draws current at high frequency )：10.0
05/03/2024 11:15:15 Read function code(F03.22 Synchronous motor pull-in current frequency )：10.0
05/03/2024 11:15:15 Read function code(F03.23 Slip compensation )：100.0
05/03/2024 11:15:15 Read function code(F03.24 Starting torque initial value )：0.0
05/03/2024 11:15:15 Read function code(F03.25 Flux control gain )：0.0
05/03/2024 11:15:15 Read function code(F03.26 Flux control integral gain )：0.0
05/03/2024 11:15:15 Read function code(F03.27 Reserved)：0
05/03/2024 11:15:15 Read function code(F03.28 Reserved)：0
05/03/2024 11:15:16 Read function code(F03.29 Reserved)：0
05/03/2024 11:15:16 Read function code(F03.30 Field weakening feedforward coefficient )：10.0
05/03/2024 11:15:16 Read function code(F03.31 Field weakening control gain )：10.0
05/03/2024 11:15:16 Read function code(F03.32 Upper limit of field weakening current )：60.0
05/03/2024 11:15:16 Read function code(F03.33 Field weakening voltage coefficient )：97.0
05/03/2024 11:15:16 Read function code(F03.34 Shaft power limit )：250.0
05/03/2024 11:15:16 Read function code(F03.35 Overexcitation braking gain )：100.0
05/03/2024 11:15:16 Read function code(F03.36 Overexcitation braking limit )：100.0
05/03/2024 11:15:16 Read function code(F03.37 Energy saving operation)：0:Shut down 
05/03/2024 11:15:16 Read function code(F03.38 Energy-saving operation lower limit of excitation )：50.0
05/03/2024 11:15:16 Read function code(F03.39 Energy-saving operation filter coefficient )：0.010
05/03/2024 11:15:16 Read function code(F03.40 Torque/speed control )：0:Speed control 
05/03/2024 11:15:16 Read function code(F03.41 Torque reference channel selection )：0000
05/03/2024 11:15:16 Read function code(F03.42 Torque  Keyboard numbers  Setting )：0.0
05/03/2024 11:15:16 Read function code(F03.43 Torque input lower limit )：0.00
05/03/2024 11:15:16 Read function code(F03.44 Lower limit corresponding setting )：0.00
05/03/2024 11:15:16 Read function code(F03.45 Torque input upper limit )：100.00
05/03/2024 11:15:16 Read function code(F03.46 Upper limit corresponding setting )：100.00
05/03/2024 11:15:16 Read function code(F03.47 Torque filter time )：0.100
05/03/2024 11:15:16 Read function code(F03.48 Speed limit selection)：0:Frequency  instruction 
05/03/2024 11:15:16 Read function code(F03.49 Reserved)：0.0
05/03/2024 11:15:16 Read function code(F03.50 Reserved)：0.0
05/03/2024 11:15:16 Read function code(F03.51 Speed limit mode)：0:Mode 0,same for forward and reverse 
05/03/2024 11:15:16 Read function code(F03.52 Output torque Upper limit )：150.0
05/03/2024 11:15:17 Read function code(F03.53 Output torque lower limit)：0.0
05/03/2024 11:15:17 Read function code(F03.54 Selection of Positive Speed Limit for Torque Control)：0:Function code F03.56 Setting 
05/03/2024 11:15:17 Read function code(F03.55 Selection of reverse speed limit for torque control)：0:Function code F03.57 Setting 
05/03/2024 11:15:17 Read function code(F03.56 Maximum speed limit for torque control forward rotation )：100.0
05/03/2024 11:15:17 Read function code(F03.57 Torque control reverse Maximum speed limit )：100.0
05/03/2024 11:15:17 Read function code(F03.58 Reserved)：1.00
05/03/2024 11:15:17 Read function code(F03.59 Reserved)：100.0
05/03/2024 11:15:17 Read function code(F03.60 High frequency injection selection )：0
05/03/2024 11:15:17 Read function code(F03.61 High frequency injection voltage )：10.0
05/03/2024 11:15:17 Read function code(F03.62 High frequency cutoff frequency )：10.0
05/03/2024 11:15:17 Read function code(F03.63 Reserved)：0
05/03/2024 11:15:17 Read function code(F03.64 Reserved)：0
05/03/2024 11:15:17 Read function code(F03.65 High frequency injection estimated gain 1)：0.500
05/03/2024 11:15:17 Read function code(F03.66 High frequency injection estimated gain 2)：0.100
05/03/2024 11:15:17 Read function code(F03.67 High frequency injection configuration )：0
05/03/2024 11:15:17 Read function code(F03.68 High frequency injection carrier )：0
05/03/2024 11:15:17 Read function code(F03.69 Reserved)：0
05/03/2024 11:15:17 Read function code(F03.70 Position compensation control )：50.0
05/03/2024 11:15:17 Read function code(F03.71 Compensation gain )：0.00
05/03/2024 11:15:17 Read function code(F03.72 Compensation limit )：0.000
05/03/2024 11:15:17 Read function code(F03.73 Compensation range )：10.0
05/03/2024 11:15:17 Read function code(F03.74 Reserved)：10.0
05/03/2024 11:15:17 Read function code(F03.75 Software speed tracking phase lock gain 1)：1.00
05/03/2024 11:15:18 Read function code(F03.76 Software speed tracking phase lock gain 2)：5.00
05/03/2024 11:15:18 Read function code(F03.77 Reserved)：2
05/03/2024 11:15:18 Read function code(F03.78 Reserved)：0
05/03/2024 11:15:18 Read function code(F03.79 Reserved)：200
05/03/2024 11:15:18 Read function code(F03.80 Gain of SYNCHRONOUS motor MTPA )：100.0
05/03/2024 11:15:18 Read function code(F03.81 MTPA Filter time )：1.0
05/03/2024 11:15:18 Read function code(F03.82 Motor  Salient rate adjustment )：500
05/03/2024 11:15:18 Read function code(F03.83 Out of step detection time of motor )：0.000
05/03/2024 11:15:18 Read function code(F03.84 Reserved)：0
05/03/2024 11:15:18 Read function code(F03.85 Open loop estimation gain 1)：1.000
05/03/2024 11:15:18 Read function code(F03.86 Open loop estimation gain 2)：1.000
05/03/2024 11:15:18 Read function code(F03.87 Power generation gain )：30.0
05/03/2024 11:15:18 Read function code(F03.88 Phase lock gain 1)：3.000
05/03/2024 11:15:18 Read function code(F03.89 Phase lock gain 2)：1.000
05/03/2024 11:15:18 Read function code(F03.90 Reserved)：60.0
05/03/2024 11:15:18 Read function code(F03.91 Reserved)：0.0
05/03/2024 11:15:18 Read function code(F03.92 Direct vector mode optimization )：0000
05/03/2024 11:15:18 Read function code(F03.93 Direct vector minimum frequency )：1.0
05/03/2024 11:15:18 Read function code(F03.94 Minimum frequency of magnetic flux closed loop )：10.0
05/03/2024 11:15:18 Read function code(F03.95 Direct vector estimation gain )：1000
05/03/2024 11:15:18 Read function code(F04.00 Linear VF curve selection )：0:Straight line VF curve 
05/03/2024 11:15:18 Read function code(F04.01 Torque increase )：3.0
05/03/2024 11:15:18 Read function code(F04.02 Torque boost cut-off frequency )：100.0
05/03/2024 11:15:19 Read function code(F04.03 Slip compensation  gain )：0.0
05/03/2024 11:15:19 Read function code(F04.04 Slip compensation  limiting )：100.0
05/03/2024 11:15:19 Read function code(F04.05 Slip compensation  Filter time )：0.200
05/03/2024 11:15:19 Read function code(F04.06 Oscillation suppression gain )：100.0
05/03/2024 11:15:19 Read function code(F04.07 Oscillation suppression filter time )：1.0
05/03/2024 11:15:19 Read function code(F04.08 Output voltage percentage )：100.0
05/03/2024 11:15:19 Read function code(F04.09 Reserved)：0.00
05/03/2024 11:15:19 Read function code(F04.10 Self-set voltage V1)：3.0
05/03/2024 11:15:19 Read function code(F04.11 Self-setting frequency F1)：1.00
05/03/2024 11:15:19 Read function code(F04.12 Self-set voltage V2)：28.0
05/03/2024 11:15:19 Read function code(F04.13 Self-setting frequency F2)：10.00
05/03/2024 11:15:19 Read function code(F04.14 Self-set voltage V3)：55.0
05/03/2024 11:15:19 Read function code(F04.15 Self-setting frequency F3)：25.00
05/03/2024 11:15:19 Read function code(F04.16 Self-set voltage V4)：78.0
05/03/2024 11:15:19 Read function code(F04.17 Self-setting frequency F4)：37.50
05/03/2024 11:15:19 Read function code(F04.18 Self-set voltage V5)：100.0
05/03/2024 11:15:19 Read function code(F04.19 Self-setting frequency F5)：50.00
05/03/2024 11:15:19 Read function code(F04.20 V/F Voltage frequency separation  voltage given)：0000
05/03/2024 11:15:19 Read function code(F04.21 Voltage frequency separation output voltage digital  Setting )：0.00
05/03/2024 11:15:19 Read function code(F04.22 Voltage frequency separation  voltage  acceleration time )：10.00
05/03/2024 11:15:19 Read function code(F04.23 Voltage frequency separation  voltage  deceleration time )：10.00
05/03/2024 11:15:19 Read function code(F04.24 Voltage-frequency separation shutdown mode)：0:Output voltage、Output frequency Acceleration and deceleration do not affect each other 
05/03/2024 11:15:19 Read function code(F04.25 Voltage frequency separation  Setting  voltage )：0.00
05/03/2024 11:15:19 Read function code(F04.26 Voltage frequency separation min output voltage)：0
05/03/2024 11:15:19 Read function code(F04.27 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.28 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.29 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.30 Automatic energy saving control )：0:Shut down 
05/03/2024 11:15:20 Read function code(F04.31 Lower limit of energy saving frequency )：15.00
05/03/2024 11:15:20 Read function code(F04.32 Energy-saving step-down voltage lower limit )：50.0
05/03/2024 11:15:20 Read function code(F04.33 Energy-saving step-down voltage regulation rate )：0.010
05/03/2024 11:15:20 Read function code(F04.34 Energy-saving step-down voltage recovery rate )：0.200
05/03/2024 11:15:20 Read function code(F04.35 VF Overexcitation gain )：64
05/03/2024 11:15:20 Read function code(F04.36 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.37 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.38 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.39 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.40 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.41 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.42 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.43 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.44 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.45 Stabilizer proportional gain )：10.0
05/03/2024 11:15:20 Read function code(F04.46 Stabilizer filter coefficient )：0.0
05/03/2024 11:15:20 Read function code(F04.47 Stabilizer output limit )：5.0
05/03/2024 11:15:20 Read function code(F04.48 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.49 Reserved)：0
05/03/2024 11:15:20 Read function code(F04.50 Low-frequency pull-in current )：100.0
05/03/2024 11:15:20 Read function code(F04.51 Low frequency pull-in current frequency )：10.0
05/03/2024 11:15:20 Read function code(F04.52 High frequency pull current )：0.0
05/03/2024 11:15:21 Read function code(F04.53 High frequency pull current  frequency )：20.0
05/03/2024 11:15:21 Read function code(F04.54 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.55 D Shaft current gain )：0.500
05/03/2024 11:15:21 Read function code(F04.56 Q Shaft current gain )：0.500
05/03/2024 11:15:21 Read function code(F04.57 D Shaft feedforward gain )：0.000
05/03/2024 11:15:21 Read function code(F04.58 Q Shaft feedforward gain )：1.000
05/03/2024 11:15:21 Read function code(F04.59 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.60 Flux Control Setting  )：300
05/03/2024 11:15:21 Read function code(F04.61 Flux control proportional gain )：1000
05/03/2024 11:15:21 Read function code(F04.62 Flux control integral gain )：1000
05/03/2024 11:15:21 Read function code(F04.63 Flux controller frequency )：5.0
05/03/2024 11:15:21 Read function code(F04.64 Flux controller time )：7.0
05/03/2024 11:15:21 Read function code(F04.65 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.66 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.67 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.68 Reserved)：0
05/03/2024 11:15:21 Read function code(F04.69 Reserved)：0
05/03/2024 11:15:21 Read function code(F05.00 Multi-function input terminal 1(X1))：1:Forward running 
05/03/2024 11:15:21 Read function code(F05.01 Multi-function input terminal 2(X2))：4:Forward jog
05/03/2024 11:15:21 Read function code(F05.02 Multi-function input terminal 3(X3))：4:Forward jog
05/03/2024 11:15:21 Read function code(F05.03 Multi-function input terminal4(X4))：5:Reverse jog
05/03/2024 11:15:21 Read function code(F05.04 Multi-function input terminal5(X5))：6:Free stop 
05/03/2024 11:15:21 Read function code(F05.05 Multi-function input terminal6(X6))：0:No function 
05/03/2024 11:15:21 Read function code(F05.06 Multi-function input terminal7(X7))：0:No function 
05/03/2024 11:15:21 Read function code(F05.07 Multi-function input terminal8(X8))：0:No function 
05/03/2024 11:15:22 Read function code(F05.08 Multi-function input terminal9(X9))：0:No function 
05/03/2024 11:15:22 Read function code(F05.09 Multi-function input terminal10(X10))：0:No function 
05/03/2024 11:15:22 Read function code(F05.10 X1 Effective detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.11 X1 Invalid detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.12 X2 Effective detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.13 X2 Invalid detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.14 X3 Effective detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.15 X3 Invalid detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.16 X4 Effective detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.17 X4 Invalid detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.18 X5 Effective detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.19 X5 Invalid detection delay )：0.010
05/03/2024 11:15:22 Read function code(F05.20 Terminal control  operation mode )：0:Two-wire system 1
05/03/2024 11:15:22 Read function code(F05.21 Reserved)：0000
05/03/2024 11:15:22 Read function code(F05.22 X1～X4 Terminal feature selection )：0000
05/03/2024 11:15:22 Read function code(F05.23 X5～X8 Terminal feature selection )：0000
05/03/2024 11:15:22 Read function code(F05.24 X9～X10 Terminal feature selection )：0000
05/03/2024 11:15:22 Read function code(F05.25 Terminal UP / DW control selection)：0:Frequency power down storage 
05/03/2024 11:15:22 Read function code(F05.26 Terminal UP/DW control Frequency increase and decrease rate )：0.50
05/03/2024 11:15:22 Read function code(F05.27 Emergency stop  deceleration time )：1.00
05/03/2024 11:15:22 Read function code(F05.28 Reserved)：0
05/03/2024 11:15:22 Read function code(F05.29 Reserved)：0
05/03/2024 11:15:22 Read function code(F05.30 PUL port signal source )：0:X5(Max is 5.000KHz)
05/03/2024 11:15:22 Read function code(F05.31 PUL Enter the minimum frequency )：0.000
05/03/2024 11:15:22 Read function code(F05.32 PUL Minimum frequency correspondence  Setting )：0.00
05/03/2024 11:15:23 Read function code(F05.33 PUL input  Maximum frequency )：5.000
05/03/2024 11:15:23 Read function code(F05.34 PUL Maximum frequency  correspond  Setting )：100.00
05/03/2024 11:15:23 Read function code(F05.35 PUL Filter time )：0.100
05/03/2024 11:15:23 Read function code(F05.36 PUL Cut-off frequency )：0.010
05/03/2024 11:15:23 Read function code(F05.37 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.38 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.39 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.40 AI input signal type selection mode)：0:DIP switch 
05/03/2024 11:15:23 Read function code(F05.41 AI1 input signal type)：0:Voltage 0~10.00V
05/03/2024 11:15:23 Read function code(F05.42 AI2 input signal type)：0:Voltage 0~10.00V
05/03/2024 11:15:23 Read function code(F05.43 Analog input curve selection)：0000
05/03/2024 11:15:23 Read function code(F05.44 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.45 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.46 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.47 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.48 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.49 Reserved)：0
05/03/2024 11:15:23 Read function code(F05.50 AI1 lower limit)：0.0
05/03/2024 11:15:23 Read function code(F05.51 AI1 lower limit corresponding setting)：0.00
05/03/2024 11:15:23 Read function code(F05.52 AI1 upper limit)：100.0
05/03/2024 11:15:23 Read function code(F05.53 AI1 upper limit corresponding setting)：100.00
05/03/2024 11:15:23 Read function code(F05.54 AI1 filter time)：0.100
05/03/2024 11:15:23 Read function code(F05.55 AI2 lower limit)：0.0
05/03/2024 11:15:23 Read function code(F05.56 AI2 lower limit corresponding setting)：0.00
05/03/2024 11:15:23 Read function code(F05.57 AI2 upper limit value)：100.0
05/03/2024 11:15:24 Read function code(F05.58 AI2 upper limit corresponding setting)：100.00
05/03/2024 11:15:24 Read function code(F05.59 AI2 filter time )：0.100
05/03/2024 11:15:24 Read function code(F05.60 Curve 1 lower limit )：0.0
05/03/2024 11:15:24 Read function code(F05.61 Curve 1 lower limit corresponding setting)：0.00
05/03/2024 11:15:24 Read function code(F05.62 Curve 1 turning point 1 input voltage)：30.0
05/03/2024 11:15:24 Read function code(F05.63 Curve 1 turning point 1 correspond setting)：30.00
05/03/2024 11:15:24 Read function code(F05.64 Curve 1 turning point 2 input voltage)：60.0
05/03/2024 11:15:24 Read function code(F05.65 Curve 1 turning point 2 correspond setting)：60.00
05/03/2024 11:15:24 Read function code(F05.66 Curve 1 upper limit value)：100.0
05/03/2024 11:15:24 Read function code(F05.67 Curve 1 upper limit corresponding setting)：100.00
05/03/2024 11:15:24 Read function code(F05.68 Reserved)：0
05/03/2024 11:15:24 Read function code(F05.69 Reserved)：0
05/03/2024 11:15:24 Read function code(F05.70 Curve 2 lower limit value)：0.0
05/03/2024 11:15:24 Read function code(F05.71 Curve 2 lower limit corresponding setting)：0.00
05/03/2024 11:15:24 Read function code(F05.72 Curve 2 turning point 1 input voltage)：30.0
05/03/2024 11:15:24 Read function code(F05.73 Curve 2 turning point 1 correspond setting)：30.00
05/03/2024 11:15:24 Read function code(F05.74 Curve 2 turning point 2 input voltage)：60.0
05/03/2024 11:15:24 Read function code(F05.75 Curve 2 turning point 2 correspond setting)：60.00
05/03/2024 11:15:24 Read function code(F05.76 Curve 2 upper limit value)：100.0
05/03/2024 11:15:24 Read function code(F05.77 Curve 2 upper limit corresponding setting)：100.00
05/03/2024 11:15:24 Read function code(F05.78 Reserved)：0
05/03/2024 11:15:24 Read function code(F05.79 Reserved)：0
05/03/2024 11:15:24 Read function code(F05.80 AI as digital input terminal feature selection)：0000
05/03/2024 11:15:24 Read function code(F05.81 AI1 terminal Feature selection (as X))：0:No function
05/03/2024 11:15:24 Read function code(F05.82 AI1 High voltage level  Setting)：70.00
05/03/2024 11:15:24 Read function code(F05.83 AI1 Low voltage level  Setting)：30.00
05/03/2024 11:15:24 Read function code(F05.84 AI2 terminal  Feature selection (as X))：0:No function
05/03/2024 11:15:24 Read function code(F05.85 AI2 High voltage level  Setting )：70.00
05/03/2024 11:15:24 Read function code(F05.86 AI2 Low voltage level  Setting)：30.00
05/03/2024 11:15:24 Read function code(F05.87 Reserved)：1.00
05/03/2024 11:15:24 Read function code(F05.88 Reserved)：2.00
05/03/2024 11:15:24 Read function code(F05.89 Reserved)：0
05/03/2024 11:15:24 Read function code(F06.00 AO Output signal selection)：0:0～10V
05/03/2024 11:15:25 Read function code(F06.01 AO1 Output selection)：0:Given frequency
05/03/2024 11:15:25 Read function code(F06.02 AO1 Output gain )：100.0
05/03/2024 11:15:25 Read function code(F06.03 AO1 Output Signal offset)：0.0
05/03/2024 11:15:25 Read function code(F06.04 AO1 Output filter)：0.010
05/03/2024 11:15:25 Read function code(F06.05 AO1FM frequency Output lower limit)：0.20
05/03/2024 11:15:25 Read function code(F06.06 AO1FM frequency Output upper limit)：50.00
05/03/2024 11:15:25 Read function code(F06.07 AO Fixed frequency change ratio Output)：0
05/03/2024 11:15:25 Read function code(F06.08 AO Constant frequency duty cycle )：0
05/03/2024 11:15:25 Read function code(F06.09 Reserved)：0
05/03/2024 11:15:25 Read function code(F06.10 Extension AO Output  Way to choose)：0:0～10V
05/03/2024 11:15:25 Read function code(F06.11 Extension AO Output selection)：1:Output frequency
05/03/2024 11:15:25 Read function code(F06.12 Extended AO output gain)：100.0
05/03/2024 11:15:25 Read function code(F06.13 Expansion AO output signal offset)：0.0
05/03/2024 11:15:25 Read function code(F06.14 Extended AO output filter)：0.010
05/03/2024 11:15:25 Read function code(F06.15 Extend the lower limit of AOFM frequency output)：0.20
05/03/2024 11:15:25 Read function code(F06.16 Extend the upper limit of AOFM frequency output)：50.00
05/03/2024 11:15:25 Read function code(F06.17 Reserved)：0
05/03/2024 11:15:25 Read function code(F06.18 Reserved)：0
05/03/2024 11:15:25 Read function code(F06.19 Reserved)：0
05/03/2024 11:15:25 Read function code(F06.20 Output terminal polarity selection)：0000
05/03/2024 11:15:25 Read function code(F06.21 Output terminal Y)：1:The inverter is running
05/03/2024 11:15:25 Read function code(F06.22 Relay 1 output)：4:Fault trip alarm 1 (alarm during fault self-recovery)
05/03/2024 11:15:25 Read function code(F06.23 Extend the Y1 terminal)：0:No output
05/03/2024 11:15:25 Read function code(F06.24 Extended relay output 2)：0:No output
05/03/2024 11:15:25 Read function code(F06.25 Y output ON delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.26 Relay 1 output ON delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.27 Extend Y1 output ON delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.28 Extend relay 2 output ON delay time )：0.010
05/03/2024 11:15:25 Read function code(F06.29 Y output OFF delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.30 Relay 1 output OFF delay time )：0.010
05/03/2024 11:15:25 Read function code(F06.31 Extend Y1 output OFF delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.32 Extend relay 2 output OFF delay time)：0.010
05/03/2024 11:15:25 Read function code(F06.33 Y terminal second function selection)：0
05/03/2024 11:15:25 Read function code(F06.34 Y terminal logic function selection)：0
05/03/2024 11:15:26 Read function code(F06.35 Y terminal delay time )：0
05/03/2024 11:15:26 Read function code(F06.36 Relay 1 second function selection)：0
05/03/2024 11:15:26 Read function code(F06.37 Relay 1 logical function selection)：0
05/03/2024 11:15:26 Read function code(F06.38 Relay 1 delay time)：0
05/03/2024 11:15:26 Read function code(F06.39 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.40 Frequency detection value 1)：2.00
05/03/2024 11:15:26 Read function code(F06.41 Frequency detection amplitude 1)：1.00
05/03/2024 11:15:26 Read function code(F06.42 Frequency detection value 2)：2.00
05/03/2024 11:15:26 Read function code(F06.43 Frequency detection amplitude 2)：1.00
05/03/2024 11:15:26 Read function code(F06.44 Given frequency arrives Check out the amplitude)：2.00
05/03/2024 11:15:26 Read function code(F06.45 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.46 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.47 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.48 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.49 Reserved)：0
05/03/2024 11:15:26 Read function code(F06.50 Comparator 1 monitors the selection)：0001
05/03/2024 11:15:26 Read function code(F06.51 Comparator 1 upper limit)：30.00
05/03/2024 11:15:26 Read function code(F06.52 Comparator 1 lower limit )：0.00
05/03/2024 11:15:26 Read function code(F06.53 Comparator 1 bias)：0.00
05/03/2024 11:15:26 Read function code(F06.54 Action selection when sending CP1)：0:Forced stop 
05/03/2024 11:15:26 Read function code(F06.55 Comparator 2 monitors the selection)：0002
05/03/2024 11:15:26 Read function code(F06.56 Comparator 2 upper limit )：3.0
05/03/2024 11:15:26 Read function code(F06.57 Comparator 2 lower limit)：0.0
05/03/2024 11:15:26 Read function code(F06.58 Comparator 2 bias)：0.0
05/03/2024 11:15:26 Read function code(F06.59 Action selection when sending CP2)：0:Forced stop 
05/03/2024 11:15:26 Read function code(F06.60 Virtual vX1 terminal function selection)：0:No function
05/03/2024 11:15:26 Read function code(F06.61 Virtual vX2 terminal function selection)：0:No function
05/03/2024 11:15:26 Read function code(F06.62 Virtual vX3 terminal function selection)：0:No function
05/03/2024 11:15:26 Read function code(F06.63 Virtual vX4 terminal function selection)：0:No function
05/03/2024 11:15:26 Read function code(F06.64 vX Terminal valid status source)：0000
05/03/2024 11:15:26 Read function code(F06.65 Virtual vX terminal function code Setting Valid state)：0000
05/03/2024 11:15:26 Read function code(F06.66 Virtual vY1 Output selection)：0:No output
05/03/2024 11:15:26 Read function code(F06.67 Virtual vY2 Output selection)：0:No output
05/03/2024 11:15:27 Read function code(F06.68 Virtual vY3 Output selection)：0:No output
05/03/2024 11:15:27 Read function code(F06.69 Virtual vY4 output selection)：0:No output
05/03/2024 11:15:27 Read function code(F06.70 vY1 Output ON Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.71 vY2 Output ON Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.72 vY3 Output ON Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.73 vY4 Output ON Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.74 vY1 Output OFF Delay time )：0.010
05/03/2024 11:15:27 Read function code(F06.75 vY2 Output OFF Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.76 vY3 Output OFF Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.77 vY4 Output OFF Delay time)：0.010
05/03/2024 11:15:27 Read function code(F06.78 Reserved)：0
05/03/2024 11:15:27 Read function code(F06.79 Reserved)：0
05/03/2024 11:15:27 Read function code(F07.00 Startup operation mode )：0:Started by the boot frequency 
05/03/2024 11:15:27 Read function code(F07.01 Start pre-excitation time )：0.00
05/03/2024 11:15:27 Read function code(F07.02 Start frequency )：0.00
05/03/2024 11:15:27 Read function code(F07.03 Enable protection selection )：0111
05/03/2024 11:15:27 Read function code(F07.04 Reserved)：0000
05/03/2024 11:15:27 Read function code(F07.05 Rotation direction selection)：0000
05/03/2024 11:15:27 Read function code(F07.06 Start action selection after power failure)：0:Invalid
05/03/2024 11:15:27 Read function code(F07.07 Blackout restart waiting time)：0.50
05/03/2024 11:15:27 Read function code(F07.08 Reserved)：0
05/03/2024 11:15:27 Read function code(F07.09 Reserved)：0
05/03/2024 11:15:27 Read function code(F07.10 Stop way )：0:Decelerate to stop
05/03/2024 11:15:27 Read function code(F07.11 Stop check out frequency)：0.05
05/03/2024 11:15:27 Read function code(F07.12 Stop restart limit time )：0.010
05/03/2024 11:15:27 Read function code(F07.13 Reserved)：0
05/03/2024 11:15:27 Read function code(F07.14 Reserved)：0
05/03/2024 11:15:27 Read function code(F07.15 Insufficient lower frequency action selection )：2:Operation at the lowest output frequency
05/03/2024 11:15:27 Read function code(F07.16 Zero velocity moment retention factor)：60.0
05/03/2024 11:15:27 Read function code(F07.17 Zero velocity moment holding time)：0.0
05/03/2024 11:15:27 Read function code(F07.18 Positive and negative dead zone time)：0.0
05/03/2024 11:15:27 Read function code(F07.19 Reserved)：0.00
05/03/2024 11:15:28 Read function code(F07.20 Braking current before starting)：60.0
05/03/2024 11:15:28 Read function code(F07.21 Braking time before starting)：0.0
05/03/2024 11:15:28 Read function code(F07.22 Dc brake start frequency)：0.10
05/03/2024 11:15:28 Read function code(F07.23 Dc brake current )：60.0
05/03/2024 11:15:28 Read function code(F07.24 Dc braking time when stop )：0.0
05/03/2024 11:15:28 Read function code(F07.25 Speed tracking mode)：0000
05/03/2024 11:15:28 Read function code(F07.26 Speed tracking )：0.50
05/03/2024 11:15:28 Read function code(F07.27 Speed tracking stop delay)：1.00
05/03/2024 11:15:28 Read function code(F07.28 Speed tracking current )：120.0
05/03/2024 11:15:28 Read function code(F07.29 Short circuit braking time)：0.00
05/03/2024 11:15:28 Read function code(F07.30 Jog operating frequency setting)：50.00
05/03/2024 11:15:28 Read function code(F07.31 Jog acceleration time)：10.00
05/03/2024 11:15:28 Read function code(F07.32 Jog deceleration time)：10.00
05/03/2024 11:15:28 Read function code(F07.33 Jog S curve choose)：1
05/03/2024 11:15:28 Read function code(F07.34 Inching deceleration mode selection)：0:Same as F07.10 
05/03/2024 11:15:28 Read function code(F07.35 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.36 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.37 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.38 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.39 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.40 Maintain frequency at startup)：0.05
05/03/2024 11:15:28 Read function code(F07.41 Frequency duration at startup)：0.00
05/03/2024 11:15:28 Read function code(F07.42 Maintain frequency during downtime )：0.05
05/03/2024 11:15:28 Read function code(F07.43 Maintain frequency during downtime )：0.00
05/03/2024 11:15:28 Read function code(F07.44 Hopping frequency 1)：0.00
05/03/2024 11:15:28 Read function code(F07.45 Jump frequency amplitude 1)：0.00
05/03/2024 11:15:28 Read function code(F07.46 Hopping frequency 2)：0.00
05/03/2024 11:15:28 Read function code(F07.47 Jump frequency amplitude 2)：0.00
05/03/2024 11:15:28 Read function code(F07.48 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.49 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.50 Reserved)：0
05/03/2024 11:15:28 Read function code(F07.51 Reserved)：0
05/03/2024 11:15:29 Read function code(F07.52 Reserved)：0
05/03/2024 11:15:29 Read function code(F07.53 Reserved)：0
05/03/2024 11:15:29 Read function code(F07.54 Reserved)：0
05/03/2024 11:15:29 Read function code(F07.55 Reserved)：0
05/03/2024 11:15:29 Read function code(F08.00 Counter input source)：0:Ordinary X terminal 
05/03/2024 11:15:29 Read function code(F08.01 Count input frequency division)：0
05/03/2024 11:15:29 Read function code(F08.02 Counter maximum)：1000
05/03/2024 11:15:29 Read function code(F08.03 Counter setting value)：500
05/03/2024 11:15:29 Read function code(F08.04 Pulse per meter )：10.0
05/03/2024 11:15:29 Read function code(F08.05 Setting length)：1000
05/03/2024 11:15:29 Read function code(F08.06 Actual length)：0
05/03/2024 11:15:29 Read function code(F08.07 Timer Unit of time)：0:Second
05/03/2024 11:15:29 Read function code(F08.08 Timer Setting value)：0
05/03/2024 11:15:29 Read function code(F08.09 Reserved)：0
05/03/2024 11:15:29 Read function code(F08.10 Reserved)：0.50
05/03/2024 11:15:29 Read function code(F08.11 Reserved)：0.00
05/03/2024 11:15:29 Read function code(F08.12 Reserved)：4.50
05/03/2024 11:15:29 Read function code(F08.13 Reserved)：100.00
05/03/2024 11:15:29 Read function code(F08.14 Reserved)：0000
05/03/2024 11:15:29 Read function code(F08.15 Reserved)：0001
05/03/2024 11:15:29 Read function code(F08.16 Reserved)：0002
05/03/2024 11:15:29 Read function code(F08.17 Reserved)：0011
05/03/2024 11:15:29 Read function code(F08.18 Reserved)：0002
05/03/2024 11:15:29 Read function code(F08.19 Reserved)：0004
05/03/2024 11:15:29 Read function code(F08.20 Zero servo gain)：0010
05/03/2024 11:15:29 Read function code(F08.21 Zero servo end amplitude)：0012
05/03/2024 11:15:29 Read function code(F08.22 Reserved)：0000
05/03/2024 11:15:29 Read function code(F08.23 Reserved)：0
05/03/2024 11:15:29 Read function code(F08.24 Reserved)：100.0
05/03/2024 11:15:29 Read function code(F08.25 Reserved)：100.0
05/03/2024 11:15:29 Read function code(F08.26 Reserved)：0
05/03/2024 11:15:29 Read function code(F08.27 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.28 Reserved)：1
05/03/2024 11:15:30 Read function code(F08.29 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.30 Pendulum frequency control)：0:The pendulum control is invalid
05/03/2024 11:15:30 Read function code(F08.31 Swing frequency and amplitude control)：0000
05/03/2024 11:15:30 Read function code(F08.32 Pendulum preset frequency)：0.00
05/03/2024 11:15:30 Read function code(F08.33 Pendulum preset frequency  Waiting time)：0.0
05/03/2024 11:15:30 Read function code(F08.34 Frequency and amplitude)：10.0
05/03/2024 11:15:30 Read function code(F08.35 Jump frequency)：10.0
05/03/2024 11:15:30 Read function code(F08.36 Pendulum frequency cycle)：5.00
05/03/2024 11:15:30 Read function code(F08.37 Delta wave rise time)：5.00
05/03/2024 11:15:30 Read function code(F08.38 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.39 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.40 Droop mode controls selection )：0:Invalid
05/03/2024 11:15:30 Read function code(F08.41 Droop control output torque filter coefficient)：8192
05/03/2024 11:15:30 Read function code(F08.42 Droop control gain 1)：100
05/03/2024 11:15:30 Read function code(F08.43 Droop control gain 2)：8193
05/03/2024 11:15:30 Read function code(F08.44 Droop control gain  Switch torque points)：100
05/03/2024 11:15:30 Read function code(F08.45 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.46 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.47 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.48 Reserved)：0
05/03/2024 11:15:30 Read function code(F08.49 Reserved)：0
05/03/2024 11:15:30 Read function code(F10.00 Overcurrent suppression function)：0:Suppression works all the time
05/03/2024 11:15:30 Read function code(F10.01 Overcurrent suppression point )：160.0
05/03/2024 11:15:30 Read function code(F10.02 Overcurrent suppression gain)：100.0
05/03/2024 11:15:30 Read function code(F10.03 Current protection setting 1)：0001
05/03/2024 11:15:30 Read function code(F10.04 Current protection setting 2)：0001
05/03/2024 11:15:30 Read function code(F10.05 Current imbalances  Judgment threshold)：160
05/03/2024 11:15:30 Read function code(F10.06 Current imbalances  Filter time)：2.0
05/03/2024 11:15:30 Read function code(F10.07 Reserved)：0
05/03/2024 11:15:30 Read function code(F10.08 Reserved)：0
05/03/2024 11:15:30 Read function code(F10.09 Inverter overload)：0.0
05/03/2024 11:15:31 Read function code(F10.10 Bus over-voltage hardware protection)：0:Close
05/03/2024 11:15:31 Read function code(F10.11 Bus over-voltage  Inhibition function)：0011
05/03/2024 11:15:31 Read function code(F10.12 Bus overpressure suppression point)：750
05/03/2024 11:15:31 Read function code(F10.13 Overvoltage suppression gain of the bus)：100.0
05/03/2024 11:15:31 Read function code(F10.14 Energy consumption braking  Enable)：2:At the same time Enable energy consumption braking and overvoltage  Inhibition function
05/03/2024 11:15:31 Read function code(F10.15 Energy saving brake operating voltage)：740
05/03/2024 11:15:31 Read function code(F10.16 Bus undervoltage Inhibition function )：0:Disable
05/03/2024 11:15:31 Read function code(F10.17 Bus undervoltage suppression point)：430
05/03/2024 11:15:31 Read function code(F10.18 Bus undervoltage suppressed gain)：100.0
05/03/2024 11:15:31 Read function code(F10.19 Bus undervoltage protection point )：320
05/03/2024 11:15:31 Read function code(F10.20 Input and output phase loss protection selection)：0021
05/03/2024 11:15:31 Read function code(F10.21 Input phase loss threshold)：15.0
05/03/2024 11:15:31 Read function code(F10.22 Choice of ground short circuit protection)：0111
05/03/2024 11:15:31 Read function code(F10.23 Fan ON/OFF controls selection )：1:ON/OFF control according to the running instructions
05/03/2024 11:15:31 Read function code(F10.24 Fan control  Delay time )：30.00
05/03/2024 11:15:31 Read function code(F10.25 Frequency converter overheating oH1Warning Check out level)：80.0
05/03/2024 11:15:31 Read function code(F10.26 Motor Overheating protection Options (extended))：0061
05/03/2024 11:15:31 Read function code(F10.27 Motor Overheat protection level )：110.0
05/03/2024 11:15:31 Read function code(F10.28 Motor Overheat alarm level )：90.0
05/03/2024 11:15:31 Read function code(F10.29 Reserved)：0
05/03/2024 11:15:31 Read function code(F10.30 Reserved)：100.0
05/03/2024 11:15:31 Read function code(F10.31 Reserved)：0
05/03/2024 11:15:31 Read function code(F10.32 Load warning check out Settings)：0000
05/03/2024 11:15:31 Read function code(F10.33 Load warning check out level 1)：130.0
05/03/2024 11:15:31 Read function code(F10.34 Load warning check out time 1)：5.0
05/03/2024 11:15:31 Read function code(F10.35 Load warning check out level 2)：30.0
05/03/2024 11:15:31 Read function code(F10.36 Load warning check out time 2)：5.0
05/03/2024 11:15:31 Read function code(F10.37 Reserved)：90.0
05/03/2024 11:15:31 Read function code(F10.38 Reserved)：110.0
05/03/2024 11:15:31 Read function code(F10.39 Reserved)：-35.0
05/03/2024 11:15:31 Read function code(F10.40 Speed ​​deviation is too large protection action)：0000
05/03/2024 11:15:32 Read function code(F10.41 Speed ​​deviation is too large detection threshold)：10.0
05/03/2024 11:15:32 Read function code(F10.42 Speed ​​deviation is too large check out time)：2.0
05/03/2024 11:15:32 Read function code(F10.43 Rapid protective action)：0002
05/03/2024 11:15:32 Read function code(F10.44 Rapid detection of thresholds)：110.0
05/03/2024 11:15:32 Read function code(F10.45 Rapid detection time )：0.100
05/03/2024 11:15:32 Read function code(F10.46 Reserved)：0
05/03/2024 11:15:32 Read function code(F10.47 Reserved)：0
05/03/2024 11:15:32 Read function code(F10.48 Reserved)：0
05/03/2024 11:15:32 Read function code(F10.49 Reserved)：0
05/03/2024 11:15:32 Read function code(F10.50 Faults Number of self-recovery)：0
05/03/2024 11:15:32 Read function code(F10.51 Faults Self recovery interval)：1.0
05/03/2024 11:15:32 Read function code(F10.52 Faults Retry the valid selection group 1)：0
05/03/2024 11:15:32 Read function code(F10.53 Faults Retry the valid selection group 2)：0
05/03/2024 11:15:32 Read function code(F10.54 Reserved)：0
05/03/2024 11:15:32 Read function code(F10.55 Motor overload model)：0:General Motor 
05/03/2024 11:15:32 Read function code(F10.56 Motor Insulation class)：3:Insulation class F
05/03/2024 11:15:32 Read function code(F10.57 Motor work schedule)：0
05/03/2024 11:15:32 Read function code(F10.58 Motor overload The initial threshold)：105.0
05/03/2024 11:15:32 Read function code(F10.59 Motor overload protection curve coefficient)：100.0
05/03/2024 11:15:32 Read function code(F11.00 Key lock selection )：0:Don't lock
05/03/2024 11:15:32 Read function code(F11.01 Key lock password )：0
05/03/2024 11:15:32 Read function code(F11.02 Keyboard multikey selection)：0:Invalid
05/03/2024 11:15:32 Read function code(F11.03 Keyboard STOP key Settings )：0:Not Keyboard control mode is invalid
05/03/2024 11:15:32 Read function code(F11.04 Keyboard up and down key selection)：0011
05/03/2024 11:15:32 Read function code(F11.05 The up and down key modifies the parameter number  Setting)：0109
05/03/2024 11:15:32 Read function code(F11.06 Keyboard command key selection)：0000
05/03/2024 11:15:32 Read function code(F11.07 Reserved)：0
05/03/2024 11:15:32 Read function code(F11.08 Keyboard knobs change dimensions )：0
05/03/2024 11:15:32 Read function code(F11.09 Reserved)：0001
05/03/2024 11:15:32 Read function code(F11.10 The status interface moves left and right  Feature selection )：0011
05/03/2024 11:15:32 Read function code(F11.11 The first line of the keyboard loops out the parameters 1)：0000
05/03/2024 11:15:33 Read function code(F11.12 The first line of the keyboard loops out the parameters 2)：0001
05/03/2024 11:15:33 Read function code(F11.13 The first line of the keyboard loops out the parameters 3)：0002
05/03/2024 11:15:33 Read function code(F11.14 The first line of the keyboard loops out the parameters 4)：0011
05/03/2024 11:15:33 Read function code(F11.15 The second line of the keyboard loops out the parameters 1)：0002
05/03/2024 11:15:33 Read function code(F11.16 The second line of the keyboard loops out the parameters 2)：0004
05/03/2024 11:15:33 Read function code(F11.17 The second line of the keyboard loops out the parameters 3)：0010
05/03/2024 11:15:33 Read function code(F11.18 The second line of the keyboard loops out the parameters 4)：0012
05/03/2024 11:15:33 Read function code(F11.19 Reserved)：0001
05/03/2024 11:15:33 Read function code(F11.20 Keyboard display item Settings)：0002
05/03/2024 11:15:33 Read function code(F11.21 Speed display coefficient )：100.0
05/03/2024 11:15:33 Read function code(F11.22 Power display coefficient )：100.0
05/03/2024 11:15:33 Read function code(F11.23 Monitor parameter display selection)：0000
05/03/2024 11:15:33 Read function code(F11.24 Monitoring parameters Filter option )：0002
05/03/2024 11:15:33 Read function code(F11.25 Motor Display selection when self-learning)：0:Show self-learning process status
05/03/2024 11:15:33 Read function code(F11.26 EEPROM Faults Output choose)：0:Report Faults E.EEP
05/03/2024 11:15:33 Read function code(F11.27 Faults Self-restoring display selection )：1:Display
05/03/2024 11:15:33 Read function code(F11.28 Reserved)：0
05/03/2024 11:15:33 Read function code(F11.29 Reserved)：0
05/03/2024 11:15:33 Read function code(F11.30 AC10 serial port function selection)：0:RS485
05/03/2024 11:15:33 Read function code(F11.31 Keyboard potentiometer The lower voltage)：0.50
05/03/2024 11:15:33 Read function code(F11.32 Keyboard potentiometer Lower bound corresponding value )：0.00
05/03/2024 11:15:33 Read function code(F11.33 Keyboard potentiometer Ceiling voltage)：2.80
05/03/2024 11:15:33 Read function code(F11.34 Keyboard potentiometer Upper bound corresponding value)：100.00
05/03/2024 11:15:33 Read function code(F11.35 Reserved)：1
05/03/2024 11:15:33 Read function code(F11.36 Reserved)：0
05/03/2024 11:15:33 Read function code(F11.37 Reserved)：0
05/03/2024 11:15:33 Read function code(F11.38 Reserved)：0
05/03/2024 11:15:33 Read function code(F11.39 Reserved)：0
05/03/2024 11:15:33 Read function code(F12.00 Master-slave choice )：0:Slave
05/03/2024 11:15:33 Read function code(F12.01 485 Communication address)：1
05/03/2024 11:15:33 Read function code(F12.02 Communication Baud rate selection )：3:9600 bps
05/03/2024 11:15:33 Read function code(F12.03 Modbus data format)：0
05/03/2024 11:15:34 Read function code(F12.04 Modbus Transmission response processing)：0:Write operations respond
05/03/2024 11:15:34 Read function code(F12.05 Modbus Communication response delay )：0
05/03/2024 11:15:34 Read function code(F12.06 Modbus communication timeout failure time)：1.0
05/03/2024 11:15:34 Read function code(F12.07 Modbus communication fault action mode selection)：0:Timeout failure is not detected 
05/03/2024 11:15:34 Read function code(F12.08 Receive data (address 0x3000) with zero offset )：0.00
05/03/2024 11:15:34 Read function code(F12.09 Receive data (address 0x3000) gain )：100.0
05/03/2024 11:15:34 Read function code(F12.10 Host loop sends parameter selection)：0031
05/03/2024 11:15:34 Read function code(F12.11 Frequency given custom address Settings)：0000
05/03/2024 11:15:34 Read function code(F12.12 Command given custom Address setting)：0000
05/03/2024 11:15:34 Read function code(F12.13 Set the command value to forward run command)：0001
05/03/2024 11:15:34 Read function code(F12.14 Command to reverse the value of the run command)：0002
05/03/2024 11:15:34 Read function code(F12.15 The command is set to the stop command value)：0005
05/03/2024 11:15:34 Read function code(F12.16 Command set to reset command value)：0007
05/03/2024 11:15:34 Read function code(F12.17 Reserved)：0
05/03/2024 11:15:34 Read function code(F12.18 Reserved)：0
05/03/2024 11:15:34 Read function code(F12.19 Host send command)：0:Send run command 
05/03/2024 11:15:34 Read function code(F12.20 RJ45 Interface communication mode selection )：0:Two-line keyboard communication 
05/03/2024 11:15:34 Read function code(F12.21 Modbus communication address)：1
05/03/2024 11:15:34 Read function code(F12.22 Communication Baud rate selection)：3:9600 bps
05/03/2024 11:15:34 Read function code(F12.23 Modbus data format )：0
05/03/2024 11:15:34 Read function code(F12.24 Modbus Transmission response processing)：0:Write operations respond 
05/03/2024 11:15:34 Read function code(F12.25 Modbus communication response delay)：0
05/03/2024 11:15:34 Read function code(F12.26 Modbus communication timeout failure time )：1.0
05/03/2024 11:15:34 Read function code(F12.27 Modbus communication fault action mode selection)：0:Timeout failure is not detected 
05/03/2024 11:15:34 Read function code(F12.28 Send data selection from slave machine)：0
05/03/2024 11:15:34 Read function code(F12.29 Host send selection )：0031
05/03/2024 11:15:35 Read function code(F12.30 DP card address)：1
05/03/2024 11:15:35 Read function code(F12.31 Baud rate )：0
05/03/2024 11:15:35 Read function code(F12.32 DP host and slave Communication disconnect processing)：0:Timeout failure is not detected
05/03/2024 11:15:35 Read function code(F12.33 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.34 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.35 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.36 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.37 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.38 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.39 Reserved)：0
05/03/2024 11:15:35 Read function code(F12.40 CAN mode selection )：0
05/03/2024 11:15:35 Read function code(F12.41 Communication address )：1
05/03/2024 11:15:35 Read function code(F12.42 Communication Baud rate selection)：3
05/03/2024 11:15:35 Read function code(F12.43 Communication disconnect processing)：0:Timeout failure is not detected
05/03/2024 11:15:35 Read function code(F12.44 Communication protocol )：0:VEICHI PDO
05/03/2024 11:15:35 Read function code(F12.45 The function code sets the PDO mapping variable)：0
05/03/2024 11:15:35 Read function code(F12.46 CAN host loop sends parameter selection)：0C31
05/03/2024 11:15:35 Read function code(F12.47 CAN host receives parameter selection)：0000
05/03/2024 11:15:35 Read function code(F12.48 Number of slave nodes )：1
05/03/2024 11:15:35 Read function code(F12.49 CAN-Inverter Periodic communication time)：0
05/03/2024 11:15:35 Read function code(F12.50 Extension port communication disconnect processing)：0000
05/03/2024 11:15:35 Read function code(F12.51 EX-A parameter update for expansion port )：0
05/03/2024 11:15:35 Read function code(F12.52 EX-B parameter update for expansion port)：0
05/03/2024 11:15:35 Read function code(F12.53 EX-A expansion port monitoring frame address group 1)：0001
05/03/2024 11:15:35 Read function code(F12.54 EX-A expansion port monitoring frame address group 2)：0002
05/03/2024 11:15:35 Read function code(F12.55 EX-A expansion port monitoring frame address group 3)：0007
05/03/2024 11:15:35 Read function code(F12.56 EX-A expansion port monitoring frame address group 4)：0011
05/03/2024 11:15:35 Read function code(F12.57 EX-B expansion port monitoring frame address group 1)：0001
05/03/2024 11:15:35 Read function code(F12.58 EX-B expansion port monitoring frame address group 2)：0002
05/03/2024 11:15:36 Read function code(F12.59 EX-B expansion port monitoring frame address group 3)：0007
05/03/2024 11:15:36 Read function code(F12.60 EX-B expansion port monitoring frame address group 4)：0011
05/03/2024 11:15:36 Read function code(F12.61 Reserved)：65535
05/03/2024 11:15:36 Read function code(F12.62 Reserved)：0
05/03/2024 11:15:36 Read function code(F12.63 Reserved)：0
05/03/2024 11:15:36 Read function code(F12.64 Reserved)：0
05/03/2024 11:15:36 Read function code(F12.65 Reserved)：0
05/03/2024 11:15:36 Read function code(F13.00 The PID controller is given the signal source)：0:Keyboard numbers PID given
05/03/2024 11:15:36 Read function code(F13.01 Keyboard numbers PID given/feedback)：50.0
05/03/2024 11:15:36 Read function code(F13.02 PID given  Change time)：1.00
05/03/2024 11:15:36 Read function code(F13.03 PID controller feedback signal source)：2:AI1
05/03/2024 11:15:36 Read function code(F13.04 Feedback signal Filter time)：0.010
05/03/2024 11:15:36 Read function code(F13.05 Feedback gain )：1.00
05/03/2024 11:15:36 Read function code(F13.06 Given and feedback range)：100.0
05/03/2024 11:15:36 Read function code(F13.07 PID control selection )：0100
05/03/2024 11:15:36 Read function code(F13.08 PID Preset the Output )：100.0
05/03/2024 11:15:36 Read function code(F13.09 PID preset Output running time)：0.0
05/03/2024 11:15:36 Read function code(F13.10 Limit of PID control deviation)：0.0
05/03/2024 11:15:36 Read function code(F13.11 The proportional gain P1)：0.100
05/03/2024 11:15:36 Read function code(F13.12 Integration time I1)：1.0
05/03/2024 11:15:36 Read function code(F13.13 Differential gain D1)：0.000
05/03/2024 11:15:36 Read function code(F13.14 The proportional gain P2)：0.100
05/03/2024 11:15:36 Read function code(F13.15 Integration time I2)：1.0
05/03/2024 11:15:36 Read function code(F13.16 Differential gain D2)：0.000
05/03/2024 11:15:36 Read function code(F13.17 PID parameter switching conditions )：0:Don't switch
05/03/2024 11:15:36 Read function code(F13.18 Switch deviation low value)：20.0
05/03/2024 11:15:36 Read function code(F13.19 Switch bias high value)：80.0
05/03/2024 11:15:36 Read function code(F13.20 Reserved)：0.010
05/03/2024 11:15:36 Read function code(F13.21 Differential limiting)：5.0
05/03/2024 11:15:36 Read function code(F13.22 PID output upper limit)：100.0
05/03/2024 11:15:36 Read function code(F13.23 PID output lower limit)：0.0
05/03/2024 11:15:37 Read function code(F13.24 PID output filter time)：0.000
05/03/2024 11:15:37 Read function code(F13.25 Feedback line break action selection)：0:Continue PID running without reporting Faults 
05/03/2024 11:15:37 Read function code(F13.26 Feedback disconnection detection time)：1.0
05/03/2024 11:15:37 Read function code(F13.27 Disconnected  Alarm upper limit)：100.0
05/03/2024 11:15:37 Read function code(F13.28 Disconnected  Alarm lower limit )：0.0
05/03/2024 11:15:37 Read function code(F13.29 Sleep to choose)：0:Invalid
05/03/2024 11:15:37 Read function code(F13.30 Frequency of sleep )：10.00
05/03/2024 11:15:37 Read function code(F13.31 Sleep latency )：60.0
05/03/2024 11:15:37 Read function code(F13.32 Wake up the deviation)：5.0
05/03/2024 11:15:37 Read function code(F13.33 Wake up time delay )：1.0
05/03/2024 11:15:37 Read function code(F13.34 Reserved)：0
05/03/2024 11:15:37 Read function code(F11.35保留)：0
05/03/2024 11:15:37 Read function code(F14.00 PLC multistage speed 1)：10.00
05/03/2024 11:15:37 Read function code(F14.01 PLC multistage speed 2)：20.00
05/03/2024 11:15:37 Read function code(F14.02 PLC multistage speed 3)：30.00
05/03/2024 11:15:37 Read function code(F14.03 PLC multistage speed 4)：40.00
05/03/2024 11:15:37 Read function code(F14.04 PLC multistage speed 5)：50.00
05/03/2024 11:15:37 Read function code(F14.05 PLC multistage speed 6)：40.00
05/03/2024 11:15:37 Read function code(F14.06 PLC multistage speed 7)：30.00
05/03/2024 11:15:37 Read function code(F14.07 PLC multistage speed 8)：20.00
05/03/2024 11:15:37 Read function code(F14.08 PLC multistage speed 9)：10.00
05/03/2024 11:15:37 Read function code(F14.09 PLC multistage speed 10)：20.00
05/03/2024 11:15:37 Read function code(F14.10 PLC multistage speed 11)：30.00
05/03/2024 11:15:37 Read function code(F14.11 PLC multistage speed 12)：40.00
05/03/2024 11:15:37 Read function code(F14.12 PLC multistage speed 13)：50.00
05/03/2024 11:15:37 Read function code(F14.13 PLC multistage speed 14)：40.00
05/03/2024 11:15:37 Read function code(F14.14 PLC multistage speed 15)：30.00
05/03/2024 11:15:37 Read function code(F14.15 PLC operation mode selection )：0000
05/03/2024 11:15:37 Read function code(F14.16 PLC stage 1 running time)：10.0
05/03/2024 11:15:37 Read function code(F14.17 PLC stage 2 running time)：10.0
05/03/2024 11:15:37 Read function code(F14.18 PLC stage 3 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.19 PLC stage 4 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.20 PLC stage 5 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.21 PLC stage 6 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.22 PLC stage 7 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.23 PLC stage 8 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.24 PLC stage 9 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.25 PLC stage 10 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.26 PLC stage 11 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.27 PLC stage 12 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.28 PLC stage 13 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.29 PLC stage 14 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.30 PLC stage 15 running time)：10.0
05/03/2024 11:15:38 Read function code(F14.31 PLC stage 1 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.32 PLC stage 2 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.33 PLC stage 3 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.34 PLC stage 4 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.35 PLC stage 5 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.36 PLC stage 6 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.37 PLC stage 7 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.38 PLC stage 8 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.39 PLC stage 9 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.40 PLC stage 10 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.41 PLC stage 11 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.42 PLC stage 12 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.43 PLC stage 13 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.44 PLC stage 14 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.45 PLC stage 15 Direction and  Acceleration and deceleration time)：0000
05/03/2024 11:15:38 Read function code(F14.46 Reserved)：0
05/03/2024 11:15:39 Read function code(F14.47 Reserved)：0
05/03/2024 11:15:39 Read function code(F14.48 Reserved)：0
05/03/2024 11:15:39 Read function code(F14.49 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.00)：1
05/03/2024 11:15:39 Read function code(F16.01 Winding mode Settings)：0:Winding
05/03/2024 11:15:39 Read function code(F16.02 Mechanical transmission ratio)：1.00
05/03/2024 11:15:39 Read function code(F16.03 Tension  Setting choose)：0000
05/03/2024 11:15:39 Read function code(F16.04 Recogniton digital Setting)：0.0
05/03/2024 11:15:39 Read function code(F16.05 Max tension)：100.0
05/03/2024 11:15:39 Read function code(F16.06 Tension taper coefficient)：0.0
05/03/2024 11:15:39 Read function code(F16.07 Taper compensation correction)：0
05/03/2024 11:15:39 Read function code(F16.08 Zero velocity threshold)：1.00
05/03/2024 11:15:39 Read function code(F16.09 Zero velocity tension gain)：100.0
05/03/2024 11:15:39 Read function code(F16.10 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.11 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.12 Static friction compensation )：0.0
05/03/2024 11:15:39 Read function code(F16.13 Static friction compensation delay time)：2.0
05/03/2024 11:15:39 Read function code(F16.14 Static friction compensation  Cut-off frequency)：2.00
05/03/2024 11:15:39 Read function code(F16.15 Initial coefficient of sliding friction compensation)：0.0
05/03/2024 11:15:39 Read function code(F16.16 Sliding friction compensation termination factor)：0.0
05/03/2024 11:15:39 Read function code(F16.17 Reserved)：50
05/03/2024 11:15:39 Read function code(F16.18 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.19 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.20 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.21 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.22 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.23 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.24 Reserved)：0
05/03/2024 11:15:39 Read function code(F16.25 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.26 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.27 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.28 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.29 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.30 Fault detection selection)：0000
05/03/2024 11:15:40 Read function code(F16.31 Cut-off detection threshold)：100.0
05/03/2024 11:15:40 Read function code(F16.32 Delay of breakage detection)：2.0
05/03/2024 11:15:40 Read function code(F16.33 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.34 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.35 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.36 Predrive feature selection)：0:Predrive invalid
05/03/2024 11:15:40 Read function code(F16.37 Predrive frequency gain )：105.0
05/03/2024 11:15:40 Read function code(F16.38 Predrive torque gain)：105.0
05/03/2024 11:15:40 Read function code(F16.39 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.40 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.41 Reserved)：0
05/03/2024 11:15:40 Read function code(F16.42 Stop brake frequency)：2.00
05/03/2024 11:15:40 Read function code(F16.43 Stop lock time)：0.0
05/03/2024 11:15:40 Read function code(F16.44 Selection of coil diameter calculation method)：0:The initial volume diameter is not calculated
05/03/2024 11:15:40 Read function code(F16.45 The largest diameter)：500
05/03/2024 11:15:40 Read function code(F16.46 Scrolls diameter)：100
05/03/2024 11:15:40 Read function code(F16.47 Initial volume diameter source selection)：0:Terminal choice F16.48~F16.50
05/03/2024 11:15:40 Read function code(F16.48 The initial diameter 1)：100
05/03/2024 11:15:40 Read function code(F16.49 The initial diameter 2)：100
05/03/2024 11:15:40 Read function code(F16.50 The initial diameter 3)：100
05/03/2024 11:15:40 Read function code(F16.51 Roll diameter reset choose)：0
05/03/2024 11:15:40 Read function code(F16.52 Reserved)：0000
05/03/2024 11:15:40 Read function code(F16.53)：1
05/03/2024 11:15:40 Read function code(F16.54 Limiting the rate of change of coil diameter )：10.00
05/03/2024 11:15:41 Read function code(F16.55 Limit of coil diameter variation direction)：0
05/03/2024 11:15:41 Read function code(F16.56 Linear velocity input)：0:Terminal choice F16.60/F16.61
05/03/2024 11:15:41 Read function code(F16.57 Maximum linear velocity)：1000.0
05/03/2024 11:15:41 Read function code(F16.58 Linear velocity digital Setting)：20.0
05/03/2024 11:15:41 Read function code(F16.59 The coil diameter calculates the minimum linear velocity)：2.0
05/03/2024 11:15:41 Read function code(F16.60 Linear velocity Setting value 1)：20.0
05/03/2024 11:15:41 Read function code(F16.61 Linear velocity Setting value 2)：20.0
05/03/2024 11:15:41 Read function code(F16.62 Reserved)：0.0
05/03/2024 11:15:41 Read function code(F16.63 The coil diameter calculates the lowest frequency)：1.00
05/03/2024 11:15:41 Read function code(F16.64 Reserved)：0000
05/03/2024 11:15:41 Read function code(F16.65 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.66 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.67 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.68 Number of pulses per turn of the winding roll )：1
05/03/2024 11:15:41 Read function code(F16.69 Each layer laps)：1
05/03/2024 11:15:41 Read function code(F16.70 Digital setting of material thickness)：0.01
05/03/2024 11:15:41 Read function code(F16.71 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.72 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.73 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.74 Reserved)：0
05/03/2024 11:15:41 Read function code(F16.75 Tension PID Enable)：0:Disable
05/03/2024 11:15:41 Read function code(F16.76 Tension PID output reference source)：0:Take a given tension as a reference source
05/03/2024 11:15:41 Read function code(F16.77 Maximum output ratio of tension PID)：10.0
05/03/2024 11:15:41 Read function code(F16.78 Tension PID feedback signal source)：2:AI1 feedback
05/03/2024 11:15:41 Read function code(F16.79 Tension PID Keyboard numbers  feedback  Setting)：50.0
05/03/2024 11:15:41 Read function code(F16.80 Tension PID feedback )：1.00
05/03/2024 11:15:41 Read function code(F16.81 The proportional gain P)：0.500
05/03/2024 11:15:41 Read function code(F16.82 Integration time T)：0.5
05/03/2024 11:15:41 Read function code(Communication Given frequency)：0.00
05/03/2024 11:15:41 Read function code(Communication command Setting)：0:No command
05/03/2024 11:15:41 Read function code(Inverter status)：10000000
05/03/2024 11:15:41 Read function code(Frequency converter fault code)：0
05/03/2024 11:15:42 Read function code(Communications given  Upper limit frequency )：0.00
05/03/2024 11:15:42 Read function code(Communication Given torque)：0.0
05/03/2024 11:15:42 Read function code(Torque control is forward Maximum Frequency limitation )：0.0
05/03/2024 11:15:42 Read function code(Torque control reverse Maximum Frequency limit)：0.0
05/03/2024 11:15:42 Read function code(Communications given PID Setting )：0.0
05/03/2024 11:15:42 Read function code(Communications given PID feedback)：0.0
05/03/2024 11:15:42 Read function code(Voltage and frequency separation voltage setting)：0.0
05/03/2024 11:15:42 Read function code(Tension Setting)：0.0
05/03/2024 11:15:42 Read function code(Coil diameter Setting)：0.0
05/03/2024 11:15:42 Read function code(Linear velocity  Setting )：0.0
05/03/2024 11:15:42 Read function code(Acceleration time 1)：1.00
05/03/2024 11:15:42 Read function code(Deceleration time 1)：6.00
05/03/2024 11:15:42 Read function code(Faults Warning、 alarm numbers )：0
05/03/2024 11:15:42 Read function code(Torque current component)：0.00
05/03/2024 11:15:42 Read function code(Torque filter time )：0.100
05/03/2024 11:15:42 Read function code(Reserved)：0.0
05/03/2024 11:15:42 Read function code(Reserved)：0.0
05/03/2024 11:15:42 Read function code(Reserved)：0.0
05/03/2024 11:15:42 Read function code(Reserved)：0.0
05/03/2024 11:15:42 Read function code(Reserved)：0.0
05/03/2024 11:15:42 Read function code(Terminal  Output )：0.0
05/03/2024 11:15:42 Read function code(AO1 Output)：0.00
05/03/2024 11:15:42 Read function code(AO2 Output )：0.00
05/03/2024 11:15:42 Read function code(CAN Communication Given frequency)：0.00
05/03/2024 11:15:42 Read function code(CAN Communication start command )：0
05/03/2024 11:15:43 Export function code to file(C:\Users\VEDA0060\Desktop\123.data)Success
05/03/2024 11:16:00 Set function code(F01.00 Motor 1 way to control )：1-->0:AM VF control 
05/03/2024 11:16:01 Set function code(F01.01 Run command channel)：1-->0:Keyboard control (External keyboard first)
05/03/2024 11:16:01 Set function code(F01.02 Frequency given source channel A)：1-->0:Keyboard numbers Given frequency
05/03/2024 11:16:02 Set function code(F01.03 Frequency given source channel A gain)：1.0-->0.0
05/03/2024 11:16:02 Set function code(F01.04 Frequency given source channel B)：1-->0:Keyboard numbers Given frequency
05/03/2024 11:16:02 Set function code(F01.05 Frequency given source channel B  gain)：1.0-->0.0
05/03/2024 11:16:03 Set function code(F01.06 Frequency channel B reference source)：1-->0:Take the maximum output frequency as the reference source 
05/03/2024 11:16:03 Set function code(F01.07 Frequency given source selection)：1-->0:Channel A
05/03/2024 11:16:03 Set function code(F01.08 Run command bundle )：1111-->0000
05/03/2024 11:16:03 Set function code(F01.09 Keyboard numbers  Setting  frequency )：1.00-->0.00
05/03/2024 11:16:04 Set function code(F01.11 Upper frequency source selection)：1-->0:Upper limit frequency digital given
05/03/2024 11:16:05 Set function code(F01.13 Lower limit frequency )：1.00-->0.00
05/03/2024 11:16:05 Set function code(F01.14 Frequency Instruction Resolution)：1-->0:0.01Hz
05/03/2024 11:16:05 Set function code(F01.20 Base frequency of acceleration and deceleration time )：1-->0:Maximum frequency 
05/03/2024 11:16:05 Set function code(F01.21 Acceleration time unit)：1-->0:1S
05/03/2024 11:16:08 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:16:08 Read function code(F01.01 Run command channel)：0:Keyboard control (External keyboard first)
05/03/2024 11:16:08 Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
05/03/2024 11:16:08 Read function code(F01.03 Frequency given source channel A gain)：0.0
05/03/2024 11:16:08 Read function code(F01.04 Frequency given source channel B)：0:Keyboard numbers Given frequency
05/03/2024 11:16:08 Read function code(F01.05 Frequency given source channel B  gain)：0.0
05/03/2024 11:16:08 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 11:16:08 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 11:16:08 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:16:08 Read function code(F01.09 Keyboard numbers  Setting  frequency )：0.00
05/03/2024 11:16:08 Read function code(F01.10 Maximum frequency )：1.00
05/03/2024 11:16:08 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:16:08 Read function code(F01.12 Digital setting of upper limit frequency)：1.00
05/03/2024 11:16:08 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:16:08 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:16:08 Read function code(F01.15 Reserved)：0
05/03/2024 11:16:08 Read function code(F01.16 Reserved)：0
05/03/2024 11:16:08 Read function code(F01.17 Reserved)：0
05/03/2024 11:16:08 Read function code(F01.18 Reserved)：0
05/03/2024 11:16:08 Read function code(F01.19 Reserved)：0
05/03/2024 11:16:08 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:16:09 Read function code(F01.21 Acceleration time unit)：0:1S
05/03/2024 11:16:09 Read function code(F01.22 Acceleration time 1)：1.00
05/03/2024 11:16:09 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:16:09 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:16:09 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:16:09 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:16:09 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:16:09 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:16:09 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:16:09 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:16:09 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:16:09 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:16:09 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:16:09 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:16:09 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:16:09 Read function code(F01.36 Reserved)：0
05/03/2024 11:16:09 Read function code(F01.37 Reserved)：0
05/03/2024 11:16:09 Read function code(F01.38 Reserved)：0
05/03/2024 11:16:09 Read function code(F01.39 Reserved)：0
05/03/2024 11:16:09 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:16:09 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:16:09 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:16:09 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:16:09 Read function code(F01.44 Reserved)：15
05/03/2024 11:16:09 Read function code(F01.45 Reserved)：50
05/03/2024 11:16:09 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:16:09 Read function code(F01.47 Reserved)：0
05/03/2024 11:16:09 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:16:09 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:16:28 Start the batch write function operation
05/03/2024 11:16:28 Batch setting function code(F00.00 Parameter access level )0
05/03/2024 11:16:28 Batch setting function code(F00.01 Purpose selection)0
05/03/2024 11:16:28 Batch setting function code(F00.02 Motor selection)0
05/03/2024 11:16:28 Batch setting function code(F00.03 Initialization)0
05/03/2024 11:16:28 Batch setting function code(F00.04 Keyboard parameter copy)0
05/03/2024 11:16:28 Batch setting function code(F00.05 User password)0000
05/03/2024 11:16:29 Batch setting function code(F00.06 LCD keyboard language selection)0
05/03/2024 11:16:29 Batch setting function code(F00.07 Free parameters 1)0
05/03/2024 11:16:29 Batch setting function code(F00.08 Free parameters 2)0
05/03/2024 11:16:29 Batch setting function code(F00.09 Reserved)0
05/03/2024 11:16:29 Batch setting function code(F00.10 Common parameters 1Address setting)0100
05/03/2024 11:16:29 Batch setting function code(F00.11 Common parameters 2Address setting)0101
05/03/2024 11:16:29 Batch setting function code(F00.12 Common parameters 3Address setting)0102
05/03/2024 11:16:29 Batch setting function code(F00.13 Common parameters 4Address setting)0710
05/03/2024 11:16:29 Batch setting function code(F00.14 Common parameters 5Address setting)0122
05/03/2024 11:16:29 Batch setting function code(F00.15 Common parameters 6Address setting)0123
05/03/2024 11:16:29 Batch setting function code(F00.16 Common parameters 7Address setting)0110
05/03/2024 11:16:29 Batch setting function code(F00.17 Common parameters 8Address setting)0112
05/03/2024 11:16:29 Batch setting function code(F00.18 Common parameters 9Address setting)0140
05/03/2024 11:16:29 Batch setting function code(F00.19 Common parameters 10Address setting)0730
05/03/2024 11:16:29 Batch setting function code(F00.20 Common parameters 11Address setting)0201
05/03/2024 11:16:29 Batch setting function code(F00.21 Common parameters 12Address setting)0202
05/03/2024 11:16:30 Batch setting function code(F00.22 Common parameters 13Address setting)0203
05/03/2024 11:16:30 Batch setting function code(F00.23 Common parameters 14Address setting)0204
05/03/2024 11:16:30 Batch setting function code(F00.24 Common parameters 15Address setting)0205
05/03/2024 11:16:30 Batch setting function code(F00.25 Common parameters 16Address setting)0206
05/03/2024 11:16:30 Batch setting function code(F00.26 Common parameters 17Address setting)0207
05/03/2024 11:16:30 Batch setting function code(F00.27 Common parameters 18Address setting)1201
05/03/2024 11:16:30 Batch setting function code(F00.28 Common parameters 19Address setting)1202
05/03/2024 11:16:30 Batch setting function code(F00.29 Common parameters 20Address setting)1203
05/03/2024 11:16:30 Batch setting function code(F00.30 Common parameters 21Address setting)0700
05/03/2024 11:16:30 Batch setting function code(F00.31 Common parameters 22Address setting)0705
05/03/2024 11:16:30 Batch setting function code(F00.32 Common parameters 23Address setting)0502
05/03/2024 11:16:30 Batch setting function code(F00.33 Common parameters 24Address setting)0503
05/03/2024 11:16:30 Batch setting function code(F00.34 Common parameters 25Address setting)0504
05/03/2024 11:16:30 Batch setting function code(F00.35 Common parameters 26Address setting)0601
05/03/2024 11:16:30 Batch setting function code(F00.36 Common parameters 27Address setting)0600
05/03/2024 11:16:30 Batch setting function code(F00.37 Common parameters 28Address setting)0621
05/03/2024 11:16:31 Batch setting function code(F00.38 Common parameters 29Address setting)0622
05/03/2024 11:16:31 Batch setting function code(F00.39 Common parameters 30Address setting)0400
05/03/2024 11:16:31 Batch setting function code(F00.40 Single board debugging options)0000
05/03/2024 11:16:31 Batch setting function code(F00.41 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.42 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.43 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.44 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.45 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.46 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.47 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.48 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F00.49 Reserved)0
05/03/2024 11:16:31 Batch setting function code(F01.00 Motor 1 way to control )1
05/03/2024 11:16:31 Batch setting function code(F01.01 Run command channel)1
05/03/2024 11:16:31 Batch setting function code(F01.02 Frequency given source channel A)1
05/03/2024 11:16:31 Batch setting function code(F01.03 Frequency given source channel A gain)1.0
05/03/2024 11:16:32 Batch setting function code(F01.04 Frequency given source channel B)1
05/03/2024 11:16:32 Batch setting function code(F01.05 Frequency given source channel B  gain)1.0
05/03/2024 11:16:32 Batch setting function code(F01.06 Frequency channel B reference source)1
05/03/2024 11:16:32 Batch setting function code(F01.07 Frequency given source selection)1
05/03/2024 11:16:32 Batch setting function code(F01.08 Run command bundle )1111
05/03/2024 11:16:32 Batch setting function code(F01.09 Keyboard numbers  Setting  frequency )1.00
05/03/2024 11:16:32 Batch setting function code(F01.10 Maximum frequency )1.00
05/03/2024 11:16:32 Batch setting function code(F01.11 Upper frequency source selection)1
05/03/2024 11:16:32 Batch setting function code(F01.12 Digital setting of upper limit frequency)1.00
05/03/2024 11:16:32 Batch setting function code(F01.13 Lower limit frequency )1.00
05/03/2024 11:16:32 Batch setting function code(F01.14 Frequency Instruction Resolution)1
05/03/2024 11:16:32 Batch setting function code(F01.15 Reserved)0
05/03/2024 11:16:32 Batch setting function code(F01.16 Reserved)0
05/03/2024 11:16:32 Batch setting function code(F01.17 Reserved)0
05/03/2024 11:16:32 Batch setting function code(F01.18 Reserved)0
05/03/2024 11:16:32 Batch setting function code(F01.19 Reserved)0
05/03/2024 11:16:33 Batch setting function code(F01.20 Base frequency of acceleration and deceleration time )1
05/03/2024 11:16:33 Batch setting function code(F01.21 Acceleration time unit)1
05/03/2024 11:16:33 Batch setting function code(F01.22 Acceleration time 1)1.00
05/03/2024 11:16:33 Batch setting function code(F01.23 Deceleration time 1)6.00
05/03/2024 11:16:33 Batch setting function code(F01.24 Acceleration time 2)10.00
05/03/2024 11:16:33 Batch setting function code(F01.25 Deceleration time 2)10.00
05/03/2024 11:16:33 Batch setting function code(F01.26 Acceleration time 3)10.00
05/03/2024 11:16:33 Batch setting function code(F01.27 Deceleration time 3)10.00
05/03/2024 11:16:33 Batch setting function code(F01.28 Acceleration time 4)10.00
05/03/2024 11:16:33 Batch setting function code(F01.29 Deceleration time 4)10.00
05/03/2024 11:16:33 Batch setting function code(F01.30 S Curve acceleration and deceleration selection )1
05/03/2024 11:16:33 Batch setting function code(F01.31 Acceleration start S-curve time )0.20
05/03/2024 11:16:33 Batch setting function code(F01.32 Acceleration end S curve time )0.20
05/03/2024 11:16:33 Batch setting function code(F01.33 S-curve time to start deceleration )0.20
05/03/2024 11:16:33 Batch setting function code(F01.34 S-curve time at the end of deceleration)0.20
05/03/2024 11:16:34 Batch setting function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )0.00
05/03/2024 11:16:34 Batch setting function code(F01.36 Reserved)0
05/03/2024 11:16:34 Batch setting function code(F01.37 Reserved)0
05/03/2024 11:16:34 Batch setting function code(F01.38 Reserved)0
05/03/2024 11:16:34 Batch setting function code(F01.39 Reserved)0
05/03/2024 11:16:34 Batch setting function code(F01.40 PWM Carrier frequency )4.0
05/03/2024 11:16:34 Batch setting function code(F01.41 PWM Control mode )1111
05/03/2024 11:16:34 Batch setting function code(F01.42 PWM way to control 1)9101
05/03/2024 11:16:34 Batch setting function code(F01.43 Dead zone compensation gain )306
05/03/2024 11:16:34 Batch setting function code(F01.44 Reserved)15
05/03/2024 11:16:34 Batch setting function code(F01.45 Reserved)50
05/03/2024 11:16:34 Batch setting function code(F01.46 Random carrier depth )0
05/03/2024 11:16:34 Batch setting function code(F01.48 Reserved)0.00
05/03/2024 11:16:34 Batch setting function code(F01.49 Reserved)6.0
05/03/2024 11:16:34 Batch setting function code(F02.01 Motor poles)4
05/03/2024 11:16:34 Batch setting function code(F02.02 Motor rated power)2.2
05/03/2024 11:16:35 Function code(F02.03 Motor rated frequency )Communication failed(code:0x86)
05/03/2024 11:16:35 Batch setting function code(F02.04 Motor rated speed)1500
05/03/2024 11:16:35 Batch setting function code(F02.05 Motor rated voltage )380
05/03/2024 11:16:35 Batch setting function code(F02.06 Motor rated current )5.0
05/03/2024 11:16:35 Batch setting function code(F02.07 Motor parameter self tuning selection)0
05/03/2024 11:16:35 Batch setting function code(F02.09 Reserved)0
05/03/2024 11:16:35 Batch setting function code(F02.10 Asynchronous motor  No-load current )1.9
05/03/2024 11:16:35 Batch setting function code(F02.11 Asynchronous motor  Stator resistance )3201
05/03/2024 11:16:35 Batch setting function code(F02.12 Asynchronous motor  Rotor resistance )2631
05/03/2024 11:16:35 Batch setting function code(F02.13 Asynchronous motor  Stator leakage inductance )1257
05/03/2024 11:16:35 Batch setting function code(F02.14 Asynchronous motor  Stator inductance)3518
05/03/2024 11:16:35 Batch setting function code(F02.20 Synchronous motor stator resistance )1315
05/03/2024 11:16:35 Batch setting function code(F02.21 Synchronous machine d-axis inductance )13.96
05/03/2024 11:16:35 Batch setting function code(F02.22 Synchronous machine q-axis inductance )13.96
05/03/2024 11:16:35 Batch setting function code(F02.23 Synchronous Back EMF)285
05/03/2024 11:16:35 Batch setting function code(F02.24 Synchronous machine encoder installation angle )0.0
05/03/2024 11:16:36 Batch setting function code(F02.28 Synchronous  Motor Pulse width coefficient)4050
05/03/2024 11:16:36 Batch setting function code(F02.30 Speed feedback or encoder type)0
05/03/2024 11:16:36 Batch setting function code(F02.31 Encoder direction)0
05/03/2024 11:16:36 Batch setting function code(F02.32 ABZ encoder Z pulse detection selection)1
05/03/2024 11:16:36 Batch setting function code(F02.33 ABZ Encoder line number )1024
05/03/2024 11:16:36 Batch setting function code(F02.34 Number of poles of resolver )2
05/03/2024 11:16:36 Batch setting function code(F02.35 Encoder transmission ratio numerator )1
05/03/2024 11:16:36 Batch setting function code(F02.36 Encoder transmission ratio denominator )1
05/03/2024 11:16:36 Batch setting function code(F02.37 Encoder speed measurement filter time )1.0
05/03/2024 11:16:36 Batch setting function code(F02.38 Encoder disconnection Check out time )0.050
05/03/2024 11:16:36 Batch setting function code(F02.39 Reserved)1
05/03/2024 11:16:36 Batch setting function code(F02.40 Reserved)0
05/03/2024 11:16:36 Batch setting function code(F02.41 Reserved)0
05/03/2024 11:16:36 Batch setting function code(F02.42 Reserved)1
05/03/2024 11:16:36 Batch setting function code(F02.43 Reserved)1024
05/03/2024 11:16:36 Batch setting function code(F02.44 Reserved)1.0
05/03/2024 11:16:36 Batch setting function code(F02.45 Reserved)0010
05/03/2024 11:16:37 Batch setting function code(F02.46 Reserved)4
05/03/2024 11:16:37 Batch setting function code(F02.47 Z Pulse tolerance)0
05/03/2024 11:16:37 Batch setting function code(F02.48 Z Pulse learning current )0
05/03/2024 11:16:37 Batch setting function code(F02.49 Encoder debug register)0000
05/03/2024 11:16:37 Batch setting function code(F02.50 Motor Online learning function selection)0
05/03/2024 11:16:37 Batch setting function code(F02.51 Stator resistance start learning coefficient 1)0
05/03/2024 11:16:37 Batch setting function code(F02.52 Stator resistance start learning coefficient 2)0.00
05/03/2024 11:16:37 Batch setting function code(F02.53 Stator resistance start learning coefficient 3)0
05/03/2024 11:16:37 Batch setting function code(F02.54 Reserved)0
05/03/2024 11:16:37 Batch setting function code(F02.55 ASR Learning frequency )60.0
05/03/2024 11:16:37 Batch setting function code(F02.56 ASR Learning acceleration and deceleration time )1.00
05/03/2024 11:16:37 Batch setting function code(F02.57 ASR Learning acceleration and deceleration times )4
05/03/2024 11:16:37 Batch setting function code(F02.58 Reserved)0
05/03/2024 11:16:37 Batch setting function code(F02.59 Reserved)0
05/03/2024 11:16:37 Batch setting function code(F02.60 Synchronous motor magnetic pole search function )0010
05/03/2024 11:16:37 Batch setting function code(F02.61 Magnetic pole search current setting value )0.0
05/03/2024 11:16:38 Batch setting function code(F02.62 Magnetic pole search current feedback value )0.0
05/03/2024 11:16:38 Batch setting function code(F02.63 PM Motor inductance learning frequency )300.00
05/03/2024 11:16:38 Batch setting function code(F02.64 PM Motor inductance learning current )0
05/03/2024 11:16:38 Batch setting function code(F02.65 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.66 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.67 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.68 Reserved)300
05/03/2024 11:16:38 Batch setting function code(F02.69 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.70 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.71 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.72 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.73 Reserved)1024
05/03/2024 11:16:38 Batch setting function code(F02.74 Reserved)1024
05/03/2024 11:16:38 Batch setting function code(F02.75 Reserved)90.0
05/03/2024 11:16:38 Batch setting function code(F02.76 Reserved)0
05/03/2024 11:16:38 Batch setting function code(F02.77 Reserved)0.00
05/03/2024 11:16:39 Batch setting function code(F02.78 Reserved)3
05/03/2024 11:16:39 Batch setting function code(F02.79 Reserved)0
05/03/2024 11:16:39 Batch setting function code(F02.80 _LQCoef0)100.0
05/03/2024 11:16:39 Batch setting function code(F02.81)100.0
05/03/2024 11:16:39 Batch setting function code(F02.82)100.0
05/03/2024 11:16:39 Batch setting function code(F02.83)100.0
05/03/2024 11:16:39 Batch setting function code(F02.84)100.0
05/03/2024 11:16:39 Batch setting function code(F02.85)100.0
05/03/2024 11:16:39 Batch setting function code(F02.86)100.0
05/03/2024 11:16:39 Batch setting function code(F02.87)100.0
05/03/2024 11:16:39 Batch setting function code(F02.88)100.0
05/03/2024 11:16:39 Batch setting function code(F02.89)100.0
05/03/2024 11:16:39 Batch setting function code(F02.90)100.0
05/03/2024 11:16:39 Batch setting function code(F02.91)100.0
05/03/2024 11:16:39 Batch setting function code(F02.92)100.0
05/03/2024 11:16:39 Batch setting function code(F02.93)100.0
05/03/2024 11:16:40 Batch setting function code(F02.94)100.0
05/03/2024 11:16:40 Batch setting function code(F02.95)100.0
05/03/2024 11:16:40 Batch setting function code(F02.96)100.0
05/03/2024 11:16:40 Batch setting function code(F02.97)100.0
05/03/2024 11:16:40 Batch setting function code(F02.98)100.0
05/03/2024 11:16:40 Batch setting function code(F02.99)100.0
05/03/2024 11:16:40 Batch setting function code(F03.00 ASR Speed ​​rigidity level )32
05/03/2024 11:16:40 Batch setting function code(F03.01 ASR Speed ​​rigid mode )0000
05/03/2024 11:16:40 Batch setting function code(F03.02 ASR (Speed ​​loop) Proportional gain 1)10.00
05/03/2024 11:16:40 Batch setting function code(F03.03 ASR (Speed ​​loop) Integration time 1)0.100
05/03/2024 11:16:40 Batch setting function code(F03.04 ASR Filter time 1)0.0
05/03/2024 11:16:40 Batch setting function code(F03.05 ASR Switching frequency 1)0.00
05/03/2024 11:16:40 Batch setting function code(F03.06 ASR (Speed ​​loop) Proportional gain 2)10.00
05/03/2024 11:16:40 Batch setting function code(F03.07 ASR (Speed ​​loop) Integration time 2)0.100
05/03/2024 11:16:40 Batch setting function code(F03.08 ASR Filter time 2)0.0
05/03/2024 11:16:41 Batch setting function code(F03.09 ASR Switching frequency 2)0.00
05/03/2024 11:16:41 Batch setting function code(F03.10 Current loop D axis proportional gain )1.000
05/03/2024 11:16:41 Batch setting function code(F03.11 Current loop D axis integral gain )1.000
05/03/2024 11:16:41 Batch setting function code(F03.12 Current loop Q axis proportional gain )1.000
05/03/2024 11:16:41 Batch setting function code(F03.13 Current loop Q axis integral gain )1.000
05/03/2024 11:16:41 Batch setting function code(F03.14 Current loop optimized configuration )0000
05/03/2024 11:16:41 Batch setting function code(F03.15 Motor torque limit )250.0
05/03/2024 11:16:41 Batch setting function code(F03.16 Torque limit in power generation state )250.0
05/03/2024 11:16:41 Batch setting function code(F03.17 Regenerative torque limit value at low speed )0.0
05/03/2024 11:16:41 Batch setting function code(F03.18 Torque limit action frequency range at low speed )6.00
05/03/2024 11:16:41 Batch setting function code(F03.19 Torque limit selection )0000
05/03/2024 11:16:41 Batch setting function code(F03.20 Synchronous motor pulls in current at low frequency )20.0
05/03/2024 11:16:41 Batch setting function code(F03.21 Synchronous motor draws current at high frequency )10.0
05/03/2024 11:16:41 Batch setting function code(F03.22 Synchronous motor pull-in current frequency )10.0
05/03/2024 11:16:41 Batch setting function code(F03.23 Slip compensation )100.0
05/03/2024 11:16:41 Batch setting function code(F03.24 Starting torque initial value )0.0
05/03/2024 11:16:42 Batch setting function code(F03.25 Flux control gain )0.0
05/03/2024 11:16:42 Batch setting function code(F03.26 Flux control integral gain )0.0
05/03/2024 11:16:42 Batch setting function code(F03.27 Reserved)0
05/03/2024 11:16:42 Batch setting function code(F03.28 Reserved)0
05/03/2024 11:16:42 Batch setting function code(F03.29 Reserved)0
05/03/2024 11:16:42 Batch setting function code(F03.30 Field weakening feedforward coefficient )10.0
05/03/2024 11:16:42 Batch setting function code(F03.31 Field weakening control gain )10.0
05/03/2024 11:16:42 Batch setting function code(F03.32 Upper limit of field weakening current )60.0
05/03/2024 11:16:42 Batch setting function code(F03.33 Field weakening voltage coefficient )97.0
05/03/2024 11:16:42 Batch setting function code(F03.34 Shaft power limit )250.0
05/03/2024 11:16:42 Batch setting function code(F03.35 Overexcitation braking gain )100.0
05/03/2024 11:16:42 Batch setting function code(F03.36 Overexcitation braking limit )100.0
05/03/2024 11:16:42 Batch setting function code(F03.37 Energy saving operation)0
05/03/2024 11:16:42 Batch setting function code(F03.38 Energy-saving operation lower limit of excitation )50.0
05/03/2024 11:16:42 Batch setting function code(F03.39 Energy-saving operation filter coefficient )0.010
05/03/2024 11:16:42 Batch setting function code(F03.40 Torque/speed control )0
05/03/2024 11:16:43 Batch setting function code(F03.41 Torque reference channel selection )0000
05/03/2024 11:16:43 Batch setting function code(F03.42 Torque  Keyboard numbers  Setting )0.0
05/03/2024 11:16:43 Batch setting function code(F03.43 Torque input lower limit )0.00
05/03/2024 11:16:43 Batch setting function code(F03.44 Lower limit corresponding setting )0.00
05/03/2024 11:16:43 Batch setting function code(F03.45 Torque input upper limit )100.00
05/03/2024 11:16:43 Batch setting function code(F03.46 Upper limit corresponding setting )100.00
05/03/2024 11:16:43 Batch setting function code(F03.47 Torque filter time )0.100
05/03/2024 11:16:43 Batch setting function code(F03.48 Speed limit selection)0
05/03/2024 11:16:43 Batch setting function code(F03.49 Reserved)0.0
05/03/2024 11:16:43 Batch setting function code(F03.50 Reserved)0.0
05/03/2024 11:16:43 Batch setting function code(F03.51 Speed limit mode)0
05/03/2024 11:16:43 Batch setting function code(F03.52 Output torque Upper limit )150.0
05/03/2024 11:16:43 Batch setting function code(F03.53 Output torque lower limit)0.0
05/03/2024 11:16:43 Batch setting function code(F03.54 Selection of Positive Speed Limit for Torque Control)0
05/03/2024 11:16:43 Batch setting function code(F03.55 Selection of reverse speed limit for torque control)0
05/03/2024 11:16:43 Batch setting function code(F03.56 Maximum speed limit for torque control forward rotation )100.0
05/03/2024 11:16:44 Batch setting function code(F03.57 Torque control reverse Maximum speed limit )100.0
05/03/2024 11:16:44 Batch setting function code(F03.58 Reserved)1.00
05/03/2024 11:16:44 Batch setting function code(F03.59 Reserved)100.0
05/03/2024 11:16:44 Batch setting function code(F03.60 High frequency injection selection )0
05/03/2024 11:16:44 Batch setting function code(F03.61 High frequency injection voltage )10.0
05/03/2024 11:16:44 Batch setting function code(F03.62 High frequency cutoff frequency )10.0
05/03/2024 11:16:44 Batch setting function code(F03.63 Reserved)0
05/03/2024 11:16:44 Batch setting function code(F03.64 Reserved)0
05/03/2024 11:16:44 Batch setting function code(F03.65 High frequency injection estimated gain 1)0.500
05/03/2024 11:16:44 Batch setting function code(F03.66 High frequency injection estimated gain 2)0.100
05/03/2024 11:16:44 Batch setting function code(F03.67 High frequency injection configuration )0
05/03/2024 11:16:44 Batch setting function code(F03.68 High frequency injection carrier )0
05/03/2024 11:16:44 Batch setting function code(F03.69 Reserved)0
05/03/2024 11:16:44 Batch setting function code(F03.70 Position compensation control )50.0
05/03/2024 11:16:44 Batch setting function code(F03.71 Compensation gain )0.00
05/03/2024 11:16:44 Batch setting function code(F03.72 Compensation limit )0.000
05/03/2024 11:16:45 Batch setting function code(F03.73 Compensation range )10.0
05/03/2024 11:16:45 Batch setting function code(F03.74 Reserved)10.0
05/03/2024 11:16:45 Batch setting function code(F03.75 Software speed tracking phase lock gain 1)1.00
05/03/2024 11:16:45 Batch setting function code(F03.76 Software speed tracking phase lock gain 2)5.00
05/03/2024 11:16:45 Batch setting function code(F03.77 Reserved)2
05/03/2024 11:16:45 Batch setting function code(F03.78 Reserved)0
05/03/2024 11:16:45 Batch setting function code(F03.79 Reserved)200
05/03/2024 11:16:45 Batch setting function code(F03.80 Gain of SYNCHRONOUS motor MTPA )100.0
05/03/2024 11:16:45 Batch setting function code(F03.81 MTPA Filter time )1.0
05/03/2024 11:16:45 Batch setting function code(F03.82 Motor  Salient rate adjustment )500
05/03/2024 11:16:45 Batch setting function code(F03.83 Out of step detection time of motor )0.000
05/03/2024 11:16:45 Batch setting function code(F03.84 Reserved)0
05/03/2024 11:16:45 Batch setting function code(F03.85 Open loop estimation gain 1)1.000
05/03/2024 11:16:45 Batch setting function code(F03.86 Open loop estimation gain 2)1.000
05/03/2024 11:16:45 Batch setting function code(F03.87 Power generation gain )30.0
05/03/2024 11:16:45 Batch setting function code(F03.88 Phase lock gain 1)3.000
05/03/2024 11:16:46 Batch setting function code(F03.89 Phase lock gain 2)1.000
05/03/2024 11:16:46 Batch setting function code(F03.90 Reserved)60.0
05/03/2024 11:16:46 Batch setting function code(F03.91 Reserved)0.0
05/03/2024 11:16:46 Batch setting function code(F03.92 Direct vector mode optimization )0000
05/03/2024 11:16:46 Batch setting function code(F03.93 Direct vector minimum frequency )1.0
05/03/2024 11:16:46 Batch setting function code(F03.94 Minimum frequency of magnetic flux closed loop )10.0
05/03/2024 11:16:46 Batch setting function code(F03.95 Direct vector estimation gain )1000
05/03/2024 11:16:46 Batch setting function code(F04.00 Linear VF curve selection )0
05/03/2024 11:16:46 Batch setting function code(F04.01 Torque increase )3.0
05/03/2024 11:16:46 Batch setting function code(F04.02 Torque boost cut-off frequency )100.0
05/03/2024 11:16:46 Batch setting function code(F04.03 Slip compensation  gain )0.0
05/03/2024 11:16:46 Batch setting function code(F04.04 Slip compensation  limiting )100.0
05/03/2024 11:16:46 Batch setting function code(F04.05 Slip compensation  Filter time )0.200
05/03/2024 11:16:46 Batch setting function code(F04.06 Oscillation suppression gain )100.0
05/03/2024 11:16:46 Batch setting function code(F04.07 Oscillation suppression filter time )1.0
05/03/2024 11:16:46 Batch setting function code(F04.08 Output voltage percentage )100.0
05/03/2024 11:16:47 Batch setting function code(F04.09 Reserved)0.00
05/03/2024 11:16:47 Batch setting function code(F04.10 Self-set voltage V1)3.0
05/03/2024 11:16:47 Batch setting function code(F04.11 Self-setting frequency F1)1.00
05/03/2024 11:16:47 Batch setting function code(F04.12 Self-set voltage V2)28.0
05/03/2024 11:16:47 Function code(F04.13 Self-setting frequency F2)Communication failed(code:0x86)
05/03/2024 11:16:47 Batch setting function code(F04.14 Self-set voltage V3)55.0
05/03/2024 11:16:47 Function code(F04.15 Self-setting frequency F3)Communication failed(code:0x86)
05/03/2024 11:16:47 Batch setting function code(F04.16 Self-set voltage V4)78.0
05/03/2024 11:16:47 Function code(F04.17 Self-setting frequency F4)Communication failed(code:0x86)
05/03/2024 11:16:47 Batch setting function code(F04.18 Self-set voltage V5)100.0
05/03/2024 11:16:47 Function code(F04.19 Self-setting frequency F5)Communication failed(code:0x86)
05/03/2024 11:16:47 Batch setting function code(F04.20 V/F Voltage frequency separation  voltage given)0000
05/03/2024 11:16:47 Batch setting function code(F04.21 Voltage frequency separation output voltage digital  Setting )0.00
05/03/2024 11:16:47 Batch setting function code(F04.22 Voltage frequency separation  voltage  acceleration time )10.00
05/03/2024 11:16:47 Batch setting function code(F04.23 Voltage frequency separation  voltage  deceleration time )10.00
05/03/2024 11:16:47 Batch setting function code(F04.24 Voltage-frequency separation shutdown mode)0
05/03/2024 11:16:48 Batch setting function code(F04.25 Voltage frequency separation  Setting  voltage )0.00
05/03/2024 11:16:48 Batch setting function code(F04.26 Voltage frequency separation min output voltage)0
05/03/2024 11:16:48 Batch setting function code(F04.27 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.28 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.29 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.30 Automatic energy saving control )0
05/03/2024 11:16:48 Function code(F04.31 Lower limit of energy saving frequency )Communication failed(code:0x86)
05/03/2024 11:16:48 Batch setting function code(F04.32 Energy-saving step-down voltage lower limit )50.0
05/03/2024 11:16:48 Batch setting function code(F04.33 Energy-saving step-down voltage regulation rate )0.010
05/03/2024 11:16:48 Batch setting function code(F04.34 Energy-saving step-down voltage recovery rate )0.200
05/03/2024 11:16:48 Batch setting function code(F04.35 VF Overexcitation gain )64
05/03/2024 11:16:48 Batch setting function code(F04.36 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.37 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.38 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.39 Reserved)0
05/03/2024 11:16:48 Batch setting function code(F04.40 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.41 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.42 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.43 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.44 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.45 Stabilizer proportional gain )10.0
05/03/2024 11:16:49 Batch setting function code(F04.46 Stabilizer filter coefficient )0.0
05/03/2024 11:16:49 Batch setting function code(F04.47 Stabilizer output limit )5.0
05/03/2024 11:16:49 Batch setting function code(F04.48 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.49 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.50 Low-frequency pull-in current )100.0
05/03/2024 11:16:49 Batch setting function code(F04.51 Low frequency pull-in current frequency )10.0
05/03/2024 11:16:49 Batch setting function code(F04.52 High frequency pull current )0.0
05/03/2024 11:16:49 Batch setting function code(F04.53 High frequency pull current  frequency )20.0
05/03/2024 11:16:49 Batch setting function code(F04.54 Reserved)0
05/03/2024 11:16:49 Batch setting function code(F04.55 D Shaft current gain )0.500
05/03/2024 11:16:49 Batch setting function code(F04.56 Q Shaft current gain )0.500
05/03/2024 11:16:50 Batch setting function code(F04.57 D Shaft feedforward gain )0.000
05/03/2024 11:16:50 Batch setting function code(F04.58 Q Shaft feedforward gain )1.000
05/03/2024 11:16:50 Batch setting function code(F04.59 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F04.60 Flux Control Setting  )300
05/03/2024 11:16:50 Batch setting function code(F04.61 Flux control proportional gain )1000
05/03/2024 11:16:50 Batch setting function code(F04.62 Flux control integral gain )1000
05/03/2024 11:16:50 Batch setting function code(F04.63 Flux controller frequency )5.0
05/03/2024 11:16:50 Batch setting function code(F04.64 Flux controller time )7.0
05/03/2024 11:16:50 Batch setting function code(F04.65 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F04.66 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F04.67 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F04.68 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F04.69 Reserved)0
05/03/2024 11:16:50 Batch setting function code(F05.00 Multi-function input terminal 1(X1))1
05/03/2024 11:16:50 Batch setting function code(F05.01 Multi-function input terminal 2(X2))4
05/03/2024 11:16:51 Batch setting function code(F05.02 Multi-function input terminal 3(X3))4
05/03/2024 11:16:51 Batch setting function code(F05.03 Multi-function input terminal4(X4))5
05/03/2024 11:16:51 Batch setting function code(F05.04 Multi-function input terminal5(X5))6
05/03/2024 11:16:51 Batch setting function code(F05.05 Multi-function input terminal6(X6))0
05/03/2024 11:16:51 Batch setting function code(F05.06 Multi-function input terminal7(X7))0
05/03/2024 11:16:51 Batch setting function code(F05.07 Multi-function input terminal8(X8))0
05/03/2024 11:16:51 Batch setting function code(F05.08 Multi-function input terminal9(X9))0
05/03/2024 11:16:51 Batch setting function code(F05.09 Multi-function input terminal10(X10))0
05/03/2024 11:16:51 Batch setting function code(F05.10 X1 Effective detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.11 X1 Invalid detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.12 X2 Effective detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.13 X2 Invalid detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.14 X3 Effective detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.15 X3 Invalid detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.16 X4 Effective detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.17 X4 Invalid detection delay )0.010
05/03/2024 11:16:51 Batch setting function code(F05.18 X5 Effective detection delay )0.010
05/03/2024 11:16:52 Batch setting function code(F05.19 X5 Invalid detection delay )0.010
05/03/2024 11:16:52 Batch setting function code(F05.20 Terminal control  operation mode )0
05/03/2024 11:16:52 Batch setting function code(F05.21 Reserved)0000
05/03/2024 11:16:52 Batch setting function code(F05.22 X1～X4 Terminal feature selection )0000
05/03/2024 11:16:52 Batch setting function code(F05.23 X5～X8 Terminal feature selection )0000
05/03/2024 11:16:52 Batch setting function code(F05.24 X9～X10 Terminal feature selection )0000
05/03/2024 11:16:52 Batch setting function code(F05.25 Terminal UP / DW control selection)0
05/03/2024 11:16:52 Batch setting function code(F05.26 Terminal UP/DW control Frequency increase and decrease rate )0.50
05/03/2024 11:16:52 Batch setting function code(F05.27 Emergency stop  deceleration time )1.00
05/03/2024 11:16:52 Batch setting function code(F05.28 Reserved)0
05/03/2024 11:16:52 Batch setting function code(F05.29 Reserved)0
05/03/2024 11:16:52 Batch setting function code(F05.30 PUL port signal source )0
05/03/2024 11:16:52 Batch setting function code(F05.31 PUL Enter the minimum frequency )0.000
05/03/2024 11:16:52 Batch setting function code(F05.32 PUL Minimum frequency correspondence  Setting )0.00
05/03/2024 11:16:52 Batch setting function code(F05.33 PUL input  Maximum frequency )5.000
05/03/2024 11:16:53 Batch setting function code(F05.34 PUL Maximum frequency  correspond  Setting )100.00
05/03/2024 11:16:53 Batch setting function code(F05.35 PUL Filter time )0.100
05/03/2024 11:16:53 Batch setting function code(F05.36 PUL Cut-off frequency )0.010
05/03/2024 11:16:53 Batch setting function code(F05.37 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.38 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.39 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.40 AI input signal type selection mode)0
05/03/2024 11:16:53 Batch setting function code(F05.41 AI1 input signal type)0
05/03/2024 11:16:53 Batch setting function code(F05.42 AI2 input signal type)0
05/03/2024 11:16:53 Batch setting function code(F05.43 Analog input curve selection)0000
05/03/2024 11:16:53 Batch setting function code(F05.44 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.45 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.46 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.47 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.48 Reserved)0
05/03/2024 11:16:53 Batch setting function code(F05.49 Reserved)0
05/03/2024 11:16:54 Batch setting function code(F05.50 AI1 lower limit)0.0
05/03/2024 11:16:54 Batch setting function code(F05.51 AI1 lower limit corresponding setting)0.00
05/03/2024 11:16:54 Batch setting function code(F05.52 AI1 upper limit)100.0
05/03/2024 11:16:54 Batch setting function code(F05.53 AI1 upper limit corresponding setting)100.00
05/03/2024 11:16:54 Batch setting function code(F05.54 AI1 filter time)0.100
05/03/2024 11:16:54 Batch setting function code(F05.55 AI2 lower limit)0.0
05/03/2024 11:16:54 Batch setting function code(F05.56 AI2 lower limit corresponding setting)0.00
05/03/2024 11:16:54 Batch setting function code(F05.57 AI2 upper limit value)100.0
05/03/2024 11:16:54 Batch setting function code(F05.58 AI2 upper limit corresponding setting)100.00
05/03/2024 11:16:54 Batch setting function code(F05.59 AI2 filter time )0.100
05/03/2024 11:16:54 Batch setting function code(F05.60 Curve 1 lower limit )0.0
05/03/2024 11:16:54 Batch setting function code(F05.61 Curve 1 lower limit corresponding setting)0.00
05/03/2024 11:16:54 Batch setting function code(F05.62 Curve 1 turning point 1 input voltage)30.0
05/03/2024 11:16:54 Batch setting function code(F05.63 Curve 1 turning point 1 correspond setting)30.00
05/03/2024 11:16:54 Batch setting function code(F05.64 Curve 1 turning point 2 input voltage)60.0
05/03/2024 11:16:54 Batch setting function code(F05.65 Curve 1 turning point 2 correspond setting)60.00
05/03/2024 11:16:55 Batch setting function code(F05.66 Curve 1 upper limit value)100.0
05/03/2024 11:16:55 Batch setting function code(F05.67 Curve 1 upper limit corresponding setting)100.00
05/03/2024 11:16:55 Batch setting function code(F05.68 Reserved)0
05/03/2024 11:16:55 Batch setting function code(F05.69 Reserved)0
05/03/2024 11:16:55 Batch setting function code(F05.70 Curve 2 lower limit value)0.0
05/03/2024 11:16:55 Batch setting function code(F05.71 Curve 2 lower limit corresponding setting)0.00
05/03/2024 11:16:55 Batch setting function code(F05.72 Curve 2 turning point 1 input voltage)30.0
05/03/2024 11:16:55 Batch setting function code(F05.73 Curve 2 turning point 1 correspond setting)30.00
05/03/2024 11:16:55 Batch setting function code(F05.74 Curve 2 turning point 2 input voltage)60.0
05/03/2024 11:16:55 Batch setting function code(F05.75 Curve 2 turning point 2 correspond setting)60.00
05/03/2024 11:16:55 Batch setting function code(F05.76 Curve 2 upper limit value)100.0
05/03/2024 11:16:55 Batch setting function code(F05.77 Curve 2 upper limit corresponding setting)100.00
05/03/2024 11:16:55 Batch setting function code(F05.78 Reserved)0
05/03/2024 11:16:55 Batch setting function code(F05.79 Reserved)0
05/03/2024 11:16:55 Batch setting function code(F05.80 AI as digital input terminal feature selection)0000
05/03/2024 11:16:55 Batch setting function code(F05.81 AI1 terminal Feature selection (as X))0
05/03/2024 11:16:56 Batch setting function code(F05.82 AI1 High voltage level  Setting)70.00
05/03/2024 11:16:56 Batch setting function code(F05.83 AI1 Low voltage level  Setting)30.00
05/03/2024 11:16:56 Batch setting function code(F05.84 AI2 terminal  Feature selection (as X))0
05/03/2024 11:16:56 Batch setting function code(F05.85 AI2 High voltage level  Setting )70.00
05/03/2024 11:16:56 Batch setting function code(F05.86 AI2 Low voltage level  Setting)30.00
05/03/2024 11:16:56 Batch setting function code(F05.87 Reserved)1.00
05/03/2024 11:16:56 Batch setting function code(F05.88 Reserved)2.00
05/03/2024 11:16:56 Batch setting function code(F05.89 Reserved)0
05/03/2024 11:16:56 Batch setting function code(F06.00 AO Output signal selection)0
05/03/2024 11:16:56 Batch setting function code(F06.01 AO1 Output selection)0
05/03/2024 11:16:56 Batch setting function code(F06.02 AO1 Output gain )100.0
05/03/2024 11:16:56 Batch setting function code(F06.03 AO1 Output Signal offset)0.0
05/03/2024 11:16:56 Batch setting function code(F06.04 AO1 Output filter)0.010
05/03/2024 11:16:56 Batch setting function code(F06.05 AO1FM frequency Output lower limit)0.20
05/03/2024 11:16:56 Batch setting function code(F06.06 AO1FM frequency Output upper limit)50.00
05/03/2024 11:16:56 Batch setting function code(F06.07 AO Fixed frequency change ratio Output)0
05/03/2024 11:16:57 Batch setting function code(F06.08 AO Constant frequency duty cycle )0
05/03/2024 11:16:57 Batch setting function code(F06.09 Reserved)0
05/03/2024 11:16:57 Batch setting function code(F06.10 Extension AO Output  Way to choose)0
05/03/2024 11:16:57 Batch setting function code(F06.11 Extension AO Output selection)1
05/03/2024 11:16:57 Batch setting function code(F06.12 Extended AO output gain)100.0
05/03/2024 11:16:57 Batch setting function code(F06.13 Expansion AO output signal offset)0.0
05/03/2024 11:16:57 Batch setting function code(F06.14 Extended AO output filter)0.010
05/03/2024 11:16:57 Batch setting function code(F06.15 Extend the lower limit of AOFM frequency output)0.20
05/03/2024 11:16:57 Batch setting function code(F06.16 Extend the upper limit of AOFM frequency output)50.00
05/03/2024 11:16:57 Batch setting function code(F06.17 Reserved)0
05/03/2024 11:16:57 Batch setting function code(F06.18 Reserved)0
05/03/2024 11:16:57 Batch setting function code(F06.19 Reserved)0
05/03/2024 11:16:57 Batch setting function code(F06.20 Output terminal polarity selection)0000
05/03/2024 11:16:57 Batch setting function code(F06.21 Output terminal Y)1
05/03/2024 11:16:57 Batch setting function code(F06.22 Relay 1 output)4
05/03/2024 11:16:57 Batch setting function code(F06.23 Extend the Y1 terminal)0
05/03/2024 11:16:58 Batch setting function code(F06.24 Extended relay output 2)0
05/03/2024 11:16:58 Batch setting function code(F06.25 Y output ON delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.26 Relay 1 output ON delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.27 Extend Y1 output ON delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.28 Extend relay 2 output ON delay time )0.010
05/03/2024 11:16:58 Batch setting function code(F06.29 Y output OFF delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.30 Relay 1 output OFF delay time )0.010
05/03/2024 11:16:58 Batch setting function code(F06.31 Extend Y1 output OFF delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.32 Extend relay 2 output OFF delay time)0.010
05/03/2024 11:16:58 Batch setting function code(F06.33 Y terminal second function selection)0
05/03/2024 11:16:58 Batch setting function code(F06.34 Y terminal logic function selection)0
05/03/2024 11:16:58 Batch setting function code(F06.35 Y terminal delay time )0
05/03/2024 11:16:58 Batch setting function code(F06.36 Relay 1 second function selection)0
05/03/2024 11:16:58 Batch setting function code(F06.37 Relay 1 logical function selection)0
05/03/2024 11:16:58 Batch setting function code(F06.38 Relay 1 delay time)0
05/03/2024 11:16:58 Batch setting function code(F06.39 Reserved)0
05/03/2024 11:16:59 Function code(F06.40 Frequency detection value 1)Communication failed(code:0x86)
05/03/2024 11:16:59 Batch setting function code(F06.41 Frequency detection amplitude 1)1.00
05/03/2024 11:16:59 Function code(F06.42 Frequency detection value 2)Communication failed(code:0x86)
05/03/2024 11:16:59 Batch setting function code(F06.43 Frequency detection amplitude 2)1.00
05/03/2024 11:16:59 Batch setting function code(F06.44 Given frequency arrives Check out the amplitude)2.00
05/03/2024 11:16:59 Batch setting function code(F06.45 Reserved)0
05/03/2024 11:16:59 Batch setting function code(F06.46 Reserved)0
05/03/2024 11:16:59 Batch setting function code(F06.47 Reserved)0
05/03/2024 11:16:59 Batch setting function code(F06.48 Reserved)0
05/03/2024 11:16:59 Batch setting function code(F06.49 Reserved)0
05/03/2024 11:16:59 Batch setting function code(F06.50 Comparator 1 monitors the selection)0001
05/03/2024 11:16:59 Batch setting function code(F06.51 Comparator 1 upper limit)30.00
05/03/2024 11:16:59 Batch setting function code(F06.52 Comparator 1 lower limit )0.00
05/03/2024 11:16:59 Batch setting function code(F06.53 Comparator 1 bias)0.00
05/03/2024 11:16:59 Batch setting function code(F06.54 Action selection when sending CP1)0
05/03/2024 11:17:00 Batch setting function code(F06.55 Comparator 2 monitors the selection)0002
05/03/2024 11:17:00 Batch setting function code(F06.56 Comparator 2 upper limit )3.0
05/03/2024 11:17:00 Batch setting function code(F06.57 Comparator 2 lower limit)0.0
05/03/2024 11:17:00 Batch setting function code(F06.58 Comparator 2 bias)0.0
05/03/2024 11:17:00 Batch setting function code(F06.59 Action selection when sending CP2)0
05/03/2024 11:17:00 Batch setting function code(F06.60 Virtual vX1 terminal function selection)0
05/03/2024 11:17:00 Batch setting function code(F06.61 Virtual vX2 terminal function selection)0
05/03/2024 11:17:00 Batch setting function code(F06.62 Virtual vX3 terminal function selection)0
05/03/2024 11:17:00 Batch setting function code(F06.63 Virtual vX4 terminal function selection)0
05/03/2024 11:17:00 Batch setting function code(F06.64 vX Terminal valid status source)0000
05/03/2024 11:17:00 Batch setting function code(F06.65 Virtual vX terminal function code Setting Valid state)0000
05/03/2024 11:17:00 Batch setting function code(F06.66 Virtual vY1 Output selection)0
05/03/2024 11:17:00 Batch setting function code(F06.67 Virtual vY2 Output selection)0
05/03/2024 11:17:00 Batch setting function code(F06.68 Virtual vY3 Output selection)0
05/03/2024 11:17:00 Batch setting function code(F06.69 Virtual vY4 output selection)0
05/03/2024 11:17:00 Batch setting function code(F06.70 vY1 Output ON Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.71 vY2 Output ON Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.72 vY3 Output ON Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.73 vY4 Output ON Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.74 vY1 Output OFF Delay time )0.010
05/03/2024 11:17:01 Batch setting function code(F06.75 vY2 Output OFF Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.76 vY3 Output OFF Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.77 vY4 Output OFF Delay time)0.010
05/03/2024 11:17:01 Batch setting function code(F06.78 Reserved)0
05/03/2024 11:17:01 Batch setting function code(F06.79 Reserved)0
05/03/2024 11:17:01 Batch setting function code(F07.00 Startup operation mode )0
05/03/2024 11:17:01 Batch setting function code(F07.01 Start pre-excitation time )0.00
05/03/2024 11:17:01 Batch setting function code(F07.02 Start frequency )0.00
05/03/2024 11:17:01 Batch setting function code(F07.03 Enable protection selection )0111
05/03/2024 11:17:01 Batch setting function code(F07.04 Reserved)0000
05/03/2024 11:17:01 Batch setting function code(F07.05 Rotation direction selection)0000
05/03/2024 11:17:01 Batch setting function code(F07.06 Start action selection after power failure)0
05/03/2024 11:17:02 Batch setting function code(F07.07 Blackout restart waiting time)0.50
05/03/2024 11:17:02 Batch setting function code(F07.08 Reserved)0
05/03/2024 11:17:02 Batch setting function code(F07.09 Reserved)0
05/03/2024 11:17:02 Batch setting function code(F07.10 Stop way )0
05/03/2024 11:17:02 Batch setting function code(F07.11 Stop check out frequency)0.05
05/03/2024 11:17:02 Batch setting function code(F07.12 Stop restart limit time )0.010
05/03/2024 11:17:02 Batch setting function code(F07.13 Reserved)0
05/03/2024 11:17:02 Batch setting function code(F07.14 Reserved)0
05/03/2024 11:17:02 Batch setting function code(F07.15 Insufficient lower frequency action selection )2
05/03/2024 11:17:02 Batch setting function code(F07.16 Zero velocity moment retention factor)60.0
05/03/2024 11:17:02 Batch setting function code(F07.17 Zero velocity moment holding time)0.0
05/03/2024 11:17:02 Batch setting function code(F07.18 Positive and negative dead zone time)0.0
05/03/2024 11:17:02 Batch setting function code(F07.19 Reserved)0.00
05/03/2024 11:17:02 Batch setting function code(F07.20 Braking current before starting)60.0
05/03/2024 11:17:02 Batch setting function code(F07.21 Braking time before starting)0.0
05/03/2024 11:17:02 Batch setting function code(F07.22 Dc brake start frequency)0.10
05/03/2024 11:17:03 Batch setting function code(F07.23 Dc brake current )60.0
05/03/2024 11:17:03 Batch setting function code(F07.24 Dc braking time when stop )0.0
05/03/2024 11:17:03 Batch setting function code(F07.25 Speed tracking mode)0000
05/03/2024 11:17:03 Batch setting function code(F07.26 Speed tracking )0.50
05/03/2024 11:17:03 Batch setting function code(F07.27 Speed tracking stop delay)1.00
05/03/2024 11:17:03 Batch setting function code(F07.28 Speed tracking current )120.0
05/03/2024 11:17:03 Batch setting function code(F07.29 Short circuit braking time)0.00
05/03/2024 11:17:03 Function code(F07.30 Jog operating frequency setting)Communication failed(code:0x86)
05/03/2024 11:17:03 Batch setting function code(F07.31 Jog acceleration time)10.00
05/03/2024 11:17:03 Batch setting function code(F07.32 Jog deceleration time)10.00
05/03/2024 11:17:03 Batch setting function code(F07.33 Jog S curve choose)1
05/03/2024 11:17:03 Batch setting function code(F07.34 Inching deceleration mode selection)0
05/03/2024 11:17:03 Batch setting function code(F07.35 Reserved)0
05/03/2024 11:17:03 Batch setting function code(F07.36 Reserved)0
05/03/2024 11:17:03 Batch setting function code(F07.37 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.38 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.39 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.40 Maintain frequency at startup)0.05
05/03/2024 11:17:04 Batch setting function code(F07.41 Frequency duration at startup)0.00
05/03/2024 11:17:04 Batch setting function code(F07.42 Maintain frequency during downtime )0.05
05/03/2024 11:17:04 Batch setting function code(F07.43 Maintain frequency during downtime )0.00
05/03/2024 11:17:04 Batch setting function code(F07.44 Hopping frequency 1)0.00
05/03/2024 11:17:04 Batch setting function code(F07.45 Jump frequency amplitude 1)0.00
05/03/2024 11:17:04 Batch setting function code(F07.46 Hopping frequency 2)0.00
05/03/2024 11:17:04 Batch setting function code(F07.47 Jump frequency amplitude 2)0.00
05/03/2024 11:17:04 Batch setting function code(F07.48 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.49 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.50 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.51 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.52 Reserved)0
05/03/2024 11:17:04 Batch setting function code(F07.53 Reserved)0
05/03/2024 11:17:05 Batch setting function code(F07.54 Reserved)0
05/03/2024 11:17:05 Batch setting function code(F07.55 Reserved)0
05/03/2024 11:17:05 Batch setting function code(F08.00 Counter input source)0
05/03/2024 11:17:05 Batch setting function code(F08.01 Count input frequency division)0
05/03/2024 11:17:05 Batch setting function code(F08.02 Counter maximum)1000
05/03/2024 11:17:05 Batch setting function code(F08.03 Counter setting value)500
05/03/2024 11:17:05 Batch setting function code(F08.04 Pulse per meter )10.0
05/03/2024 11:17:05 Batch setting function code(F08.05 Setting length)1000
05/03/2024 11:17:05 Batch setting function code(F08.06 Actual length)0
05/03/2024 11:17:05 Batch setting function code(F08.07 Timer Unit of time)0
05/03/2024 11:17:05 Batch setting function code(F08.08 Timer Setting value)0
05/03/2024 11:17:05 Batch setting function code(F08.09 Reserved)0
05/03/2024 11:17:05 Batch setting function code(F08.10 Reserved)0.50
05/03/2024 11:17:05 Batch setting function code(F08.11 Reserved)0.00
05/03/2024 11:17:05 Batch setting function code(F08.12 Reserved)4.50
05/03/2024 11:17:05 Batch setting function code(F08.13 Reserved)100.00
05/03/2024 11:17:06 Batch setting function code(F08.14 Reserved)0000
05/03/2024 11:17:06 Batch setting function code(F08.15 Reserved)0001
05/03/2024 11:17:06 Batch setting function code(F08.16 Reserved)0002
05/03/2024 11:17:06 Batch setting function code(F08.17 Reserved)0011
05/03/2024 11:17:06 Batch setting function code(F08.18 Reserved)0002
05/03/2024 11:17:06 Batch setting function code(F08.19 Reserved)0004
05/03/2024 11:17:06 Batch setting function code(F08.20 Zero servo gain)0010
05/03/2024 11:17:06 Batch setting function code(F08.21 Zero servo end amplitude)0012
05/03/2024 11:17:06 Batch setting function code(F08.22 Reserved)0000
05/03/2024 11:17:06 Batch setting function code(F08.23 Reserved)0
05/03/2024 11:17:06 Batch setting function code(F08.24 Reserved)100.0
05/03/2024 11:17:06 Batch setting function code(F08.25 Reserved)100.0
05/03/2024 11:17:06 Batch setting function code(F08.26 Reserved)0
05/03/2024 11:17:06 Batch setting function code(F08.27 Reserved)0
05/03/2024 11:17:06 Batch setting function code(F08.28 Reserved)1
05/03/2024 11:17:06 Batch setting function code(F08.29 Reserved)0
05/03/2024 11:17:07 Batch setting function code(F08.30 Pendulum frequency control)0
05/03/2024 11:17:07 Batch setting function code(F08.31 Swing frequency and amplitude control)0000
05/03/2024 11:17:07 Batch setting function code(F08.32 Pendulum preset frequency)0.00
05/03/2024 11:17:07 Batch setting function code(F08.33 Pendulum preset frequency  Waiting time)0.0
05/03/2024 11:17:07 Batch setting function code(F08.34 Frequency and amplitude)10.0
05/03/2024 11:17:07 Batch setting function code(F08.35 Jump frequency)10.0
05/03/2024 11:17:07 Batch setting function code(F08.36 Pendulum frequency cycle)5.00
05/03/2024 11:17:07 Batch setting function code(F08.37 Delta wave rise time)5.00
05/03/2024 11:17:07 Batch setting function code(F08.38 Reserved)0
05/03/2024 11:17:07 Batch setting function code(F08.39 Reserved)0
05/03/2024 11:17:07 Batch setting function code(F08.40 Droop mode controls selection )0
05/03/2024 11:17:07 Batch setting function code(F08.41 Droop control output torque filter coefficient)8192
05/03/2024 11:17:07 Batch setting function code(F08.42 Droop control gain 1)100
05/03/2024 11:17:07 Batch setting function code(F08.43 Droop control gain 2)8193
05/03/2024 11:17:07 Batch setting function code(F08.44 Droop control gain  Switch torque points)100
05/03/2024 11:17:08 Batch setting function code(F08.45 Reserved)0
05/03/2024 11:17:08 Batch setting function code(F08.46 Reserved)0
05/03/2024 11:17:08 Batch setting function code(F08.47 Reserved)0
05/03/2024 11:17:08 Batch setting function code(F08.48 Reserved)0
05/03/2024 11:17:08 Batch setting function code(F08.49 Reserved)0
05/03/2024 11:17:08 Batch setting function code(F09.00 Cumulative running time)10
05/03/2024 11:17:08 Batch setting function code(F09.01 Accumulative power time)10
05/03/2024 11:17:08 Batch setting function code(F09.02 Device maintenance alarm)0000
05/03/2024 11:17:08 Batch setting function code(F09.03 Cooling fan maintenance)0
05/03/2024 11:17:08 Batch setting function code(F09.04 Main Relay maintenance )0.0
05/03/2024 11:17:08 Batch setting function code(F09.05 Main Capacitor maintenance)0.1
05/03/2024 11:17:08 Batch setting function code(F09.06 IGBT maintenance  Setting)0.1
05/03/2024 11:17:08 Batch setting function code(F09.07)0.1
05/03/2024 11:17:08 Batch setting function code(F09.08)0
05/03/2024 11:17:08 Batch setting function code(F09.09)0
05/03/2024 11:17:08 Batch setting function code(F09.10)0
05/03/2024 11:17:09 Batch setting function code(F09.11 Customizing 1)0000
05/03/2024 11:17:09 Batch setting function code(F09.12 Setting value 1)0
05/03/2024 11:17:09 Batch setting function code(F09.13 Customizing 2)0000
05/03/2024 11:17:09 Batch setting function code(F09.14 Setting value 2)0
05/03/2024 11:17:09 Batch setting function code(F09.15 Customizing 3)0000
05/03/2024 11:17:09 Batch setting function code(F09.16 Setting value 3)0
05/03/2024 11:17:09 Batch setting function code(F09.17 Customizing 4)0000
05/03/2024 11:17:09 Batch setting function code(F09.18 Setting value 4)0
05/03/2024 11:17:09 Batch setting function code(F09.19 Customizing 5)0000
05/03/2024 11:17:09 Batch setting function code(F09.20 Setting value 5)0
05/03/2024 11:17:09 Batch setting function code(F09.21 Customizing 6)0000
05/03/2024 11:17:09 Batch setting function code(F09.22 Setting value 6)0
05/03/2024 11:17:09 Batch setting function code(F09.23 Customizing 7)0000
05/03/2024 11:17:09 Batch setting function code(F09.24 Setting value 7)0
05/03/2024 11:17:09 Batch setting function code(F09.25 Customizing 8)0000
05/03/2024 11:17:09 Batch setting function code(F09.26 Setting value 8)0
05/03/2024 11:17:10 Batch setting function code(F09.27 Customizing 9)0000
05/03/2024 11:17:10 Batch setting function code(F09.28 Setting value 9)0
05/03/2024 11:17:10 Batch setting function code(F09.29 Customizing 10)0000
05/03/2024 11:17:10 Batch setting function code(F09.30 Setting value 10)0
05/03/2024 11:17:10 Batch setting function code(F09.31 Customizing 11)0000
05/03/2024 11:17:10 Batch setting function code(F09.32 Setting value 11)0
05/03/2024 11:17:10 Batch setting function code(F09.33 Customizing 12)0000
05/03/2024 11:17:10 Batch setting function code(F09.34 Setting value 12)0
05/03/2024 11:17:10 Batch setting function code(F09.35 Customizing 13)0000
05/03/2024 11:17:10 Batch setting function code(F09.36 Setting value 13)0
05/03/2024 11:17:10 Batch setting function code(F09.37 Customizing 14)0000
05/03/2024 11:17:10 Batch setting function code(F09.38 Setting value 14)0
05/03/2024 11:17:10 Batch setting function code(F09.39 Customizing 15)0000
05/03/2024 11:17:10 Batch setting function code(F09.40 Setting value 15)0
05/03/2024 11:17:10 Batch setting function code(F09.41 Customizing 16)0000
05/03/2024 11:17:10 Batch setting function code(F09.42 Setting value 16)0
05/03/2024 11:17:11 Batch setting function code(F09.43 Customizing 17)0000
05/03/2024 11:17:11 Batch setting function code(F09.44 Setting value 17)0
05/03/2024 11:17:11 Batch setting function code(F09.45 Customizing 18)0000
05/03/2024 11:17:11 Batch setting function code(F09.46 Setting value 18)0
05/03/2024 11:17:11 Batch setting function code(F09.47 Customizing 19)0000
05/03/2024 11:17:11 Batch setting function code(F09.48 Setting value 19)0
05/03/2024 11:17:11 Batch setting function code(F09.49 Customizing 20)0000
05/03/2024 11:17:11 Batch setting function code(F09.50 Setting value 20)0
05/03/2024 11:17:11 Batch setting function code(F10.00 Overcurrent suppression function)0
05/03/2024 11:17:11 Batch setting function code(F10.01 Overcurrent suppression point )160.0
05/03/2024 11:17:11 Batch setting function code(F10.02 Overcurrent suppression gain)100.0
05/03/2024 11:17:11 Batch setting function code(F10.03 Current protection setting 1)0001
05/03/2024 11:17:11 Batch setting function code(F10.04 Current protection setting 2)0001
05/03/2024 11:17:11 Batch setting function code(F10.05 Current imbalances  Judgment threshold)160
05/03/2024 11:17:11 Batch setting function code(F10.06 Current imbalances  Filter time)2.0
05/03/2024 11:17:12 Batch setting function code(F10.07 Reserved)0
05/03/2024 11:17:12 Batch setting function code(F10.08 Reserved)0
05/03/2024 11:17:12 Batch setting function code(F10.09 Inverter overload)0.0
05/03/2024 11:17:12 Batch setting function code(F10.10 Bus over-voltage hardware protection)0
05/03/2024 11:17:12 Batch setting function code(F10.11 Bus over-voltage  Inhibition function)0011
05/03/2024 11:17:12 Batch setting function code(F10.12 Bus overpressure suppression point)750
05/03/2024 11:17:12 Batch setting function code(F10.13 Overvoltage suppression gain of the bus)100.0
05/03/2024 11:17:12 Batch setting function code(F10.14 Energy consumption braking  Enable)2
05/03/2024 11:17:12 Batch setting function code(F10.15 Energy saving brake operating voltage)740
05/03/2024 11:17:12 Batch setting function code(F10.16 Bus undervoltage Inhibition function )0
05/03/2024 11:17:12 Batch setting function code(F10.17 Bus undervoltage suppression point)430
05/03/2024 11:17:12 Batch setting function code(F10.18 Bus undervoltage suppressed gain)100.0
05/03/2024 11:17:12 Batch setting function code(F10.19 Bus undervoltage protection point )320
05/03/2024 11:17:12 Batch setting function code(F10.20 Input and output phase loss protection selection)0021
05/03/2024 11:17:12 Batch setting function code(F10.21 Input phase loss threshold)15.0
05/03/2024 11:17:12 Batch setting function code(F10.22 Choice of ground short circuit protection)0111
05/03/2024 11:17:13 Batch setting function code(F10.23 Fan ON/OFF controls selection )1
05/03/2024 11:17:13 Batch setting function code(F10.24 Fan control  Delay time )30.00
05/03/2024 11:17:13 Batch setting function code(F10.25 Frequency converter overheating oH1Warning Check out level)80.0
05/03/2024 11:17:13 Batch setting function code(F10.26 Motor Overheating protection Options (extended))0061
05/03/2024 11:17:13 Batch setting function code(F10.27 Motor Overheat protection level )110.0
05/03/2024 11:17:13 Batch setting function code(F10.28 Motor Overheat alarm level )90.0
05/03/2024 11:17:13 Batch setting function code(F10.29 Reserved)0
05/03/2024 11:17:13 Batch setting function code(F10.30 Reserved)100.0
05/03/2024 11:17:13 Batch setting function code(F10.31 Reserved)0
05/03/2024 11:17:13 Batch setting function code(F10.32 Load warning check out Settings)0000
05/03/2024 11:17:13 Batch setting function code(F10.33 Load warning check out level 1)130.0
05/03/2024 11:17:13 Batch setting function code(F10.34 Load warning check out time 1)5.0
05/03/2024 11:17:13 Batch setting function code(F10.35 Load warning check out level 2)30.0
05/03/2024 11:17:13 Batch setting function code(F10.36 Load warning check out time 2)5.0
05/03/2024 11:17:13 Batch setting function code(F10.37 Reserved)90.0
05/03/2024 11:17:13 Batch setting function code(F10.38 Reserved)110.0
05/03/2024 11:17:14 Batch setting function code(F10.39 Reserved)-35.0
05/03/2024 11:17:14 Batch setting function code(F10.40 Speed ​​deviation is too large protection action)0000
05/03/2024 11:17:14 Batch setting function code(F10.41 Speed ​​deviation is too large detection threshold)10.0
05/03/2024 11:17:14 Batch setting function code(F10.42 Speed ​​deviation is too large check out time)2.0
05/03/2024 11:17:14 Batch setting function code(F10.43 Rapid protective action)0002
05/03/2024 11:17:14 Batch setting function code(F10.44 Rapid detection of thresholds)110.0
05/03/2024 11:17:14 Batch setting function code(F10.45 Rapid detection time )0.100
05/03/2024 11:17:14 Batch setting function code(F10.46 Reserved)0
05/03/2024 11:17:14 Batch setting function code(F10.47 Reserved)0
05/03/2024 11:17:14 Batch setting function code(F10.48 Reserved)0
05/03/2024 11:17:14 Batch setting function code(F10.49 Reserved)0
05/03/2024 11:17:14 Batch setting function code(F10.50 Faults Number of self-recovery)0
05/03/2024 11:17:14 Batch setting function code(F10.51 Faults Self recovery interval)1.0
05/03/2024 11:17:14 Batch setting function code(F10.53 Faults Retry the valid selection group 2)0
05/03/2024 11:17:14 Function code(F10.54 Reserved)Communication failed(code:0x86)
05/03/2024 11:17:15 Batch setting function code(F10.55 Motor overload model)0
05/03/2024 11:17:15 Batch setting function code(F10.56 Motor Insulation class)3
05/03/2024 11:17:15 Batch setting function code(F10.57 Motor work schedule)0
05/03/2024 11:17:15 Batch setting function code(F10.58 Motor overload The initial threshold)105.0
05/03/2024 11:17:15 Batch setting function code(F10.59 Motor overload protection curve coefficient)100.0
05/03/2024 11:17:15 Batch setting function code(F11.00 Key lock selection )0
05/03/2024 11:17:15 Batch setting function code(F11.01 Key lock password )0
05/03/2024 11:17:15 Batch setting function code(F11.02 Keyboard multikey selection)0
05/03/2024 11:17:15 Batch setting function code(F11.03 Keyboard STOP key Settings )0
05/03/2024 11:17:15 Batch setting function code(F11.04 Keyboard up and down key selection)0011
05/03/2024 11:17:15 Batch setting function code(F11.05 The up and down key modifies the parameter number  Setting)0109
05/03/2024 11:17:15 Batch setting function code(F11.06 Keyboard command key selection)0000
05/03/2024 11:17:15 Batch setting function code(F11.07 Reserved)0
05/03/2024 11:17:15 Batch setting function code(F11.08 Keyboard knobs change dimensions )0
05/03/2024 11:17:15 Batch setting function code(F11.10 The status interface moves left and right  Feature selection )0011
05/03/2024 11:17:15 Batch setting function code(F11.11 The first line of the keyboard loops out the parameters 1)0000
05/03/2024 11:17:16 Batch setting function code(F11.12 The first line of the keyboard loops out the parameters 2)0001
05/03/2024 11:17:16 Batch setting function code(F11.13 The first line of the keyboard loops out the parameters 3)0002
05/03/2024 11:17:16 Batch setting function code(F11.14 The first line of the keyboard loops out the parameters 4)0011
05/03/2024 11:17:16 Batch setting function code(F11.15 The second line of the keyboard loops out the parameters 1)0002
05/03/2024 11:17:16 Batch setting function code(F11.16 The second line of the keyboard loops out the parameters 2)0004
05/03/2024 11:17:16 Batch setting function code(F11.17 The second line of the keyboard loops out the parameters 3)0010
05/03/2024 11:17:16 Batch setting function code(F11.18 The second line of the keyboard loops out the parameters 4)0012
05/03/2024 11:17:16 Batch setting function code(F11.19 Reserved)0001
05/03/2024 11:17:16 Batch setting function code(F11.20 Keyboard display item Settings)0002
05/03/2024 11:17:16 Batch setting function code(F11.21 Speed display coefficient )100.0
05/03/2024 11:17:16 Batch setting function code(F11.22 Power display coefficient )100.0
05/03/2024 11:17:16 Batch setting function code(F11.23 Monitor parameter display selection)0000
05/03/2024 11:17:16 Batch setting function code(F11.24 Monitoring parameters Filter option )0002
05/03/2024 11:17:16 Batch setting function code(F11.25 Motor Display selection when self-learning)0
05/03/2024 11:17:16 Batch setting function code(F11.26 EEPROM Faults Output choose)0
05/03/2024 11:17:16 Batch setting function code(F11.27 Faults Self-restoring display selection )1
05/03/2024 11:17:17 Batch setting function code(F11.28 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F11.29 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F11.30 AC10 serial port function selection)0
05/03/2024 11:17:17 Batch setting function code(F11.31 Keyboard potentiometer The lower voltage)0.50
05/03/2024 11:17:17 Batch setting function code(F11.32 Keyboard potentiometer Lower bound corresponding value )0.00
05/03/2024 11:17:17 Batch setting function code(F11.33 Keyboard potentiometer Ceiling voltage)2.80
05/03/2024 11:17:17 Batch setting function code(F11.34 Keyboard potentiometer Upper bound corresponding value)100.00
05/03/2024 11:17:17 Batch setting function code(F11.35 Reserved)1
05/03/2024 11:17:17 Batch setting function code(F11.36 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F11.37 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F11.38 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F11.39 Reserved)0
05/03/2024 11:17:17 Batch setting function code(F12.00 Master-slave choice )0
05/03/2024 11:17:17 Batch setting function code(F12.01 485 Communication address)1
05/03/2024 11:17:17 Batch setting function code(F12.02 Communication Baud rate selection )3
05/03/2024 11:17:17 Batch setting function code(F12.03 Modbus data format)0
05/03/2024 11:17:18 Batch setting function code(F12.04 Modbus Transmission response processing)0
05/03/2024 11:17:18 Batch setting function code(F12.05 Modbus Communication response delay )0
05/03/2024 11:17:18 Batch setting function code(F12.06 Modbus communication timeout failure time)1.0
05/03/2024 11:17:18 Batch setting function code(F12.07 Modbus communication fault action mode selection)0
05/03/2024 11:17:18 Batch setting function code(F12.08 Receive data (address 0x3000) with zero offset )0.00
05/03/2024 11:17:18 Batch setting function code(F12.09 Receive data (address 0x3000) gain )100.0
05/03/2024 11:17:18 Batch setting function code(F12.10 Host loop sends parameter selection)0031
05/03/2024 11:17:18 Batch setting function code(F12.11 Frequency given custom address Settings)0000
05/03/2024 11:17:18 Batch setting function code(F12.12 Command given custom Address setting)0000
05/03/2024 11:17:18 Batch setting function code(F12.13 Set the command value to forward run command)0001
05/03/2024 11:17:18 Batch setting function code(F12.14 Command to reverse the value of the run command)0002
05/03/2024 11:17:18 Batch setting function code(F12.15 The command is set to the stop command value)0005
05/03/2024 11:17:18 Batch setting function code(F12.16 Command set to reset command value)0007
05/03/2024 11:17:18 Batch setting function code(F12.17 Reserved)0
05/03/2024 11:17:18 Batch setting function code(F12.18 Reserved)0
05/03/2024 11:17:18 Batch setting function code(F12.19 Host send command)0
05/03/2024 11:17:19 Batch setting function code(F12.20 RJ45 Interface communication mode selection )0
05/03/2024 11:17:19 Batch setting function code(F12.21 Modbus communication address)1
05/03/2024 11:17:19 Batch setting function code(F12.22 Communication Baud rate selection)3
05/03/2024 11:17:19 Batch setting function code(F12.23 Modbus data format )0
05/03/2024 11:17:19 Batch setting function code(F12.24 Modbus Transmission response processing)0
05/03/2024 11:17:19 Batch setting function code(F12.25 Modbus communication response delay)0
05/03/2024 11:17:19 Batch setting function code(F12.26 Modbus communication timeout failure time )1.0
05/03/2024 11:17:19 Batch setting function code(F12.27 Modbus communication fault action mode selection)0
05/03/2024 11:17:19 Batch setting function code(F12.28 Send data selection from slave machine)0
05/03/2024 11:17:19 Batch setting function code(F12.29 Host send selection )0031
05/03/2024 11:17:19 Batch setting function code(F12.30 DP card address)1
05/03/2024 11:17:19 Batch setting function code(F12.31 Baud rate )0
05/03/2024 11:17:19 Batch setting function code(F12.32 DP host and slave Communication disconnect processing)0
05/03/2024 11:17:19 Batch setting function code(F12.33 Reserved)0
05/03/2024 11:17:19 Batch setting function code(F12.34 Reserved)0
05/03/2024 11:17:19 Batch setting function code(F12.35 Reserved)0
05/03/2024 11:17:20 Batch setting function code(F12.36 Reserved)0
05/03/2024 11:17:20 Batch setting function code(F12.37 Reserved)0
05/03/2024 11:17:20 Batch setting function code(F12.38 Reserved)0
05/03/2024 11:17:20 Batch setting function code(F12.39 Reserved)0
05/03/2024 11:17:20 Batch setting function code(F12.40 CAN mode selection )0
05/03/2024 11:17:20 Batch setting function code(F12.41 Communication address )1
05/03/2024 11:17:20 Batch setting function code(F12.42 Communication Baud rate selection)3
05/03/2024 11:17:20 Batch setting function code(F12.43 Communication disconnect processing)0
05/03/2024 11:17:20 Batch setting function code(F12.44 Communication protocol )0
05/03/2024 11:17:20 Batch setting function code(F12.45 The function code sets the PDO mapping variable)0
05/03/2024 11:17:20 Batch setting function code(F12.46 CAN host loop sends parameter selection)0C31
05/03/2024 11:17:20 Batch setting function code(F12.47 CAN host receives parameter selection)0000
05/03/2024 11:17:20 Batch setting function code(F12.48 Number of slave nodes )1
05/03/2024 11:17:20 Batch setting function code(F12.49 CAN-Inverter Periodic communication time)0
05/03/2024 11:17:20 Batch setting function code(F12.50 Extension port communication disconnect processing)0000
05/03/2024 11:17:20 Batch setting function code(F12.51 EX-A parameter update for expansion port )0
05/03/2024 11:17:21 Batch setting function code(F12.52 EX-B parameter update for expansion port)0
05/03/2024 11:17:21 Batch setting function code(F12.53 EX-A expansion port monitoring frame address group 1)0001
05/03/2024 11:17:21 Batch setting function code(F12.54 EX-A expansion port monitoring frame address group 2)0002
05/03/2024 11:17:21 Batch setting function code(F12.55 EX-A expansion port monitoring frame address group 3)0007
05/03/2024 11:17:21 Batch setting function code(F12.56 EX-A expansion port monitoring frame address group 4)0011
05/03/2024 11:17:21 Batch setting function code(F12.57 EX-B expansion port monitoring frame address group 1)0001
05/03/2024 11:17:21 Batch setting function code(F12.58 EX-B expansion port monitoring frame address group 2)0002
05/03/2024 11:17:21 Batch setting function code(F12.59 EX-B expansion port monitoring frame address group 3)0007
05/03/2024 11:17:21 Batch setting function code(F12.60 EX-B expansion port monitoring frame address group 4)0011
05/03/2024 11:17:21 Batch setting function code(F12.61 Reserved)65535
05/03/2024 11:17:21 Batch setting function code(F12.62 Reserved)0
05/03/2024 11:17:21 Batch setting function code(F12.63 Reserved)0
05/03/2024 11:17:21 Batch setting function code(F12.64 Reserved)0
05/03/2024 11:17:21 Batch setting function code(F12.65 Reserved)0
05/03/2024 11:17:21 Batch setting function code(F13.00 The PID controller is given the signal source)0
05/03/2024 11:17:21 Batch setting function code(F13.01 Keyboard numbers PID given/feedback)50.0
05/03/2024 11:17:22 Batch setting function code(F13.02 PID given  Change time)1.00
05/03/2024 11:17:22 Batch setting function code(F13.03 PID controller feedback signal source)2
05/03/2024 11:17:22 Batch setting function code(F13.04 Feedback signal Filter time)0.010
05/03/2024 11:17:22 Batch setting function code(F13.05 Feedback gain )1.00
05/03/2024 11:17:22 Batch setting function code(F13.06 Given and feedback range)100.0
05/03/2024 11:17:22 Batch setting function code(F13.07 PID control selection )0100
05/03/2024 11:17:22 Batch setting function code(F13.08 PID Preset the Output )100.0
05/03/2024 11:17:22 Batch setting function code(F13.09 PID preset Output running time)0.0
05/03/2024 11:17:22 Batch setting function code(F13.10 Limit of PID control deviation)0.0
05/03/2024 11:17:22 Batch setting function code(F13.11 The proportional gain P1)0.100
05/03/2024 11:17:22 Batch setting function code(F13.12 Integration time I1)1.0
05/03/2024 11:17:22 Batch setting function code(F13.13 Differential gain D1)0.000
05/03/2024 11:17:22 Batch setting function code(F13.14 The proportional gain P2)0.100
05/03/2024 11:17:22 Batch setting function code(F13.15 Integration time I2)1.0
05/03/2024 11:17:22 Batch setting function code(F13.16 Differential gain D2)0.000
05/03/2024 11:17:22 Batch setting function code(F13.17 PID parameter switching conditions )0
05/03/2024 11:17:23 Batch setting function code(F13.18 Switch deviation low value)20.0
05/03/2024 11:17:23 Batch setting function code(F13.19 Switch bias high value)80.0
05/03/2024 11:17:23 Batch setting function code(F13.20 Reserved)0.010
05/03/2024 11:17:23 Batch setting function code(F13.21 Differential limiting)5.0
05/03/2024 11:17:23 Batch setting function code(F13.22 PID output upper limit)100.0
05/03/2024 11:17:23 Batch setting function code(F13.23 PID output lower limit)0.0
05/03/2024 11:17:23 Batch setting function code(F13.24 PID output filter time)0.000
05/03/2024 11:17:23 Batch setting function code(F13.25 Feedback line break action selection)0
05/03/2024 11:17:23 Batch setting function code(F13.26 Feedback disconnection detection time)1.0
05/03/2024 11:17:23 Batch setting function code(F13.27 Disconnected  Alarm upper limit)100.0
05/03/2024 11:17:23 Batch setting function code(F13.28 Disconnected  Alarm lower limit )0.0
05/03/2024 11:17:23 Batch setting function code(F13.29 Sleep to choose)0
05/03/2024 11:17:23 Function code(F13.30 Frequency of sleep )Communication failed(code:0x86)
05/03/2024 11:17:23 Batch setting function code(F13.31 Sleep latency )60.0
05/03/2024 11:17:23 Batch setting function code(F13.32 Wake up the deviation)5.0
05/03/2024 11:17:23 Batch setting function code(F13.33 Wake up time delay )1.0
05/03/2024 11:17:24 Batch setting function code(F13.34 Reserved)0
05/03/2024 11:17:24 Batch setting function code(F11.35保留)0
05/03/2024 11:17:24 Function code(F14.00 PLC multistage speed 1)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.01 PLC multistage speed 2)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.02 PLC multistage speed 3)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.03 PLC multistage speed 4)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.04 PLC multistage speed 5)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.05 PLC multistage speed 6)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.06 PLC multistage speed 7)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.07 PLC multistage speed 8)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.08 PLC multistage speed 9)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.09 PLC multistage speed 10)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.10 PLC multistage speed 11)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.11 PLC multistage speed 12)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.12 PLC multistage speed 13)Communication failed(code:0x86)
05/03/2024 11:17:24 Function code(F14.13 PLC multistage speed 14)Communication failed(code:0x86)
05/03/2024 11:17:25 Function code(F14.14 PLC multistage speed 15)Communication failed(code:0x86)
05/03/2024 11:17:25 Batch setting function code(F14.15 PLC operation mode selection )0000
05/03/2024 11:17:25 Batch setting function code(F14.16 PLC stage 1 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.17 PLC stage 2 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.18 PLC stage 3 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.19 PLC stage 4 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.20 PLC stage 5 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.21 PLC stage 6 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.22 PLC stage 7 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.23 PLC stage 8 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.24 PLC stage 9 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.25 PLC stage 10 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.26 PLC stage 11 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.27 PLC stage 12 running time)10.0
05/03/2024 11:17:25 Batch setting function code(F14.28 PLC stage 13 running time)10.0
05/03/2024 11:17:26 Batch setting function code(F14.29 PLC stage 14 running time)10.0
05/03/2024 11:17:26 Batch setting function code(F14.30 PLC stage 15 running time)10.0
05/03/2024 11:17:26 Batch setting function code(F14.31 PLC stage 1 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.32 PLC stage 2 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.33 PLC stage 3 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.34 PLC stage 4 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.35 PLC stage 5 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.36 PLC stage 6 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.37 PLC stage 7 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.38 PLC stage 8 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.39 PLC stage 9 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.40 PLC stage 10 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.41 PLC stage 11 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.42 PLC stage 12 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.43 PLC stage 13 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:26 Batch setting function code(F14.44 PLC stage 14 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:27 Batch setting function code(F14.45 PLC stage 15 Direction and  Acceleration and deceleration time)0000
05/03/2024 11:17:27 Batch setting function code(F14.46 Reserved)0
05/03/2024 11:17:27 Batch setting function code(F14.47 Reserved)0
05/03/2024 11:17:27 Batch setting function code(F14.48 Reserved)0
05/03/2024 11:17:27 Batch setting function code(F14.49 Reserved)0
05/03/2024 11:17:27 Batch setting function code(F16.00)1
05/03/2024 11:17:27 Batch setting function code(F16.01 Winding mode Settings)0
05/03/2024 11:17:27 Batch setting function code(F16.02 Mechanical transmission ratio)1.00
05/03/2024 11:17:27 Batch setting function code(F16.03 Tension  Setting choose)0000
05/03/2024 11:17:27 Batch setting function code(F16.04 Recogniton digital Setting)0.0
05/03/2024 11:17:27 Batch setting function code(F16.05 Max tension)100.0
05/03/2024 11:17:27 Batch setting function code(F16.06 Tension taper coefficient)0.0
05/03/2024 11:17:27 Batch setting function code(F16.07 Taper compensation correction)0
05/03/2024 11:17:27 Batch setting function code(F16.08 Zero velocity threshold)1.00
05/03/2024 11:17:27 Batch setting function code(F16.09 Zero velocity tension gain)100.0
05/03/2024 11:17:27 Batch setting function code(F16.10 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.11 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.12 Static friction compensation )0.0
05/03/2024 11:17:28 Batch setting function code(F16.13 Static friction compensation delay time)2.0
05/03/2024 11:17:28 Function code(F16.14 Static friction compensation  Cut-off frequency)Communication failed(code:0x86)
05/03/2024 11:17:28 Batch setting function code(F16.15 Initial coefficient of sliding friction compensation)0.0
05/03/2024 11:17:28 Batch setting function code(F16.16 Sliding friction compensation termination factor)0.0
05/03/2024 11:17:28 Batch setting function code(F16.17 Reserved)50
05/03/2024 11:17:28 Batch setting function code(F16.18 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.19 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.20 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.21 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.22 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.23 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.24 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.25 Reserved)0
05/03/2024 11:17:28 Batch setting function code(F16.26 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.27 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.28 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.29 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.30 Fault detection selection)0000
05/03/2024 11:17:29 Batch setting function code(F16.31 Cut-off detection threshold)100.0
05/03/2024 11:17:29 Batch setting function code(F16.32 Delay of breakage detection)2.0
05/03/2024 11:17:29 Batch setting function code(F16.33 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.34 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.35 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.36 Predrive feature selection)0
05/03/2024 11:17:29 Batch setting function code(F16.37 Predrive frequency gain )105.0
05/03/2024 11:17:29 Batch setting function code(F16.38 Predrive torque gain)105.0
05/03/2024 11:17:29 Batch setting function code(F16.39 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.40 Reserved)0
05/03/2024 11:17:29 Batch setting function code(F16.41 Reserved)0
05/03/2024 11:17:30 Function code(F16.42 Stop brake frequency)Communication failed(code:0x86)
05/03/2024 11:17:30 Batch setting function code(F16.43 Stop lock time)0.0
05/03/2024 11:17:30 Batch setting function code(F16.44 Selection of coil diameter calculation method)0
05/03/2024 11:17:30 Batch setting function code(F16.45 The largest diameter)500
05/03/2024 11:17:30 Batch setting function code(F16.46 Scrolls diameter)100
05/03/2024 11:17:30 Batch setting function code(F16.47 Initial volume diameter source selection)0
05/03/2024 11:17:30 Batch setting function code(F16.48 The initial diameter 1)100
05/03/2024 11:17:30 Batch setting function code(F16.49 The initial diameter 2)100
05/03/2024 11:17:30 Batch setting function code(F16.50 The initial diameter 3)100
05/03/2024 11:17:30 Batch setting function code(F16.51 Roll diameter reset choose)0
05/03/2024 11:17:30 Batch setting function code(F16.52 Reserved)0000
05/03/2024 11:17:30 Batch setting function code(F16.53)1
05/03/2024 11:17:30 Batch setting function code(F16.54 Limiting the rate of change of coil diameter )10.00
05/03/2024 11:17:30 Batch setting function code(F16.55 Limit of coil diameter variation direction)0
05/03/2024 11:17:30 Batch setting function code(F16.56 Linear velocity input)0
05/03/2024 11:17:30 Batch setting function code(F16.57 Maximum linear velocity)1000.0
05/03/2024 11:17:31 Batch setting function code(F16.58 Linear velocity digital Setting)20.0
05/03/2024 11:17:31 Batch setting function code(F16.59 The coil diameter calculates the minimum linear velocity)2.0
05/03/2024 11:17:31 Batch setting function code(F16.60 Linear velocity Setting value 1)20.0
05/03/2024 11:17:31 Batch setting function code(F16.61 Linear velocity Setting value 2)20.0
05/03/2024 11:17:31 Batch setting function code(F16.63 The coil diameter calculates the lowest frequency)1.00
05/03/2024 11:17:31 Batch setting function code(F16.64 Reserved)0000
05/03/2024 11:17:31 Batch setting function code(F16.65 Reserved)0
05/03/2024 11:17:31 Batch setting function code(F16.66 Reserved)0
05/03/2024 11:17:31 Batch setting function code(F16.67 Reserved)0
05/03/2024 11:17:31 Batch setting function code(F16.68 Number of pulses per turn of the winding roll )1
05/03/2024 11:17:31 Batch setting function code(F16.69 Each layer laps)1
05/03/2024 11:17:31 Batch setting function code(F16.70 Digital setting of material thickness)0.01
05/03/2024 11:17:31 Batch setting function code(F16.71 Reserved)0
05/03/2024 11:17:31 Batch setting function code(F16.72 Reserved)0
05/03/2024 11:17:31 Batch setting function code(F16.73 Reserved)0
05/03/2024 11:17:32 Batch setting function code(F16.74 Reserved)0
05/03/2024 11:17:32 Batch setting function code(F16.75 Tension PID Enable)0
05/03/2024 11:17:32 Batch setting function code(F16.76 Tension PID output reference source)0
05/03/2024 11:17:32 Batch setting function code(F16.77 Maximum output ratio of tension PID)10.0
05/03/2024 11:17:32 Batch setting function code(F16.78 Tension PID feedback signal source)2
05/03/2024 11:17:32 Batch setting function code(F16.79 Tension PID Keyboard numbers  feedback  Setting)50.0
05/03/2024 11:17:32 Batch setting function code(F16.80 Tension PID feedback )1.00
05/03/2024 11:17:32 Batch setting function code(F16.81 The proportional gain P)0.500
05/03/2024 11:17:32 Batch setting function code(F16.82 Integration time T)0.5
05/03/2024 11:17:32 Batch setting function code(F19.00)0
05/03/2024 11:17:32 Batch setting function code(F19.01)1
05/03/2024 11:17:32 Batch setting function code(F19.02)0
05/03/2024 11:17:32 Batch setting function code(F19.03)0
05/03/2024 11:17:32 Batch setting function code(F19.04)0
05/03/2024 11:17:32 Batch setting function code(F19.05)0
05/03/2024 11:17:32 Batch setting function code(F19.06)0
05/03/2024 11:17:33 Batch setting function code(F19.07)7
05/03/2024 11:17:33 Batch setting function code(F19.08)0
05/03/2024 11:17:33 Batch setting function code(F19.09)9
05/03/2024 11:17:33 Batch setting function code(F19.10)0
05/03/2024 11:17:33 Batch setting function code(F19.11)0
05/03/2024 11:17:33 Batch setting function code(F19.12)0
05/03/2024 11:17:33 Batch setting function code(F19.13)0
05/03/2024 11:17:33 Batch setting function code(F19.14)0
05/03/2024 11:17:33 Batch setting function code(F19.15)15
05/03/2024 11:17:33 Batch setting function code(F19.16)0
05/03/2024 11:17:33 Batch setting function code(F19.17)0
05/03/2024 11:17:33 Batch setting function code(F19.18)0
05/03/2024 11:17:33 Batch setting function code(F19.19)0
05/03/2024 11:17:33 Batch setting function code(F19.20)0
05/03/2024 11:17:33 Batch setting function code(F19.21)0
05/03/2024 11:17:33 Batch setting function code(F19.22)0
05/03/2024 11:17:34 Batch setting function code(F19.23)0
05/03/2024 11:17:34 Batch setting function code(F19.24)0
05/03/2024 11:17:34 Batch setting function code(F19.25)0
05/03/2024 11:17:34 Batch setting function code(F19.26)0
05/03/2024 11:17:34 Batch setting function code(F19.27)0
05/03/2024 11:17:34 Batch setting function code(F19.28)0
05/03/2024 11:17:34 Batch setting function code(F19.29)0
05/03/2024 11:17:34 Batch setting function code(F19.30)0
05/03/2024 11:17:34 Batch setting function code(F19.31)0
05/03/2024 11:17:34 Batch setting function code(F19.32)0
05/03/2024 11:17:34 Batch setting function code(F19.33)0
05/03/2024 11:17:34 Batch setting function code(F19.34)0
05/03/2024 11:17:34 Batch setting function code(F19.35)0
05/03/2024 11:17:34 Batch setting function code(F19.36)0
05/03/2024 11:17:34 Batch setting function code(F19.37)0
05/03/2024 11:17:34 Batch setting function code(F19.38)0
05/03/2024 11:17:35 Batch setting function code(F19.39)0
05/03/2024 11:17:35 Batch setting function code(F19.40)0
05/03/2024 11:17:35 Batch setting function code(F19.41)0
05/03/2024 11:17:35 Batch setting function code(F19.42)0
05/03/2024 11:17:35 Batch setting function code(F19.43)43
05/03/2024 11:17:35 Batch setting function code(F19.44)44
05/03/2024 11:17:35 Batch setting function code(F19.45)45
05/03/2024 11:17:35 Batch setting function code(F19.46)0
05/03/2024 11:17:35 Batch setting function code(F19.47)0
05/03/2024 11:17:35 Batch setting function code(F19.48)0
05/03/2024 11:17:35 Batch setting function code(F19.49)49
05/03/2024 11:17:35 Batch setting function code(F19.50)50
05/03/2024 11:17:35 Batch setting function code(F19.51)51
05/03/2024 11:17:35 Batch setting function code(F19.52)52
05/03/2024 11:17:35 Batch setting function code(F19.53)53
05/03/2024 11:17:36 Batch setting function code(F19.54)54
05/03/2024 11:17:36 Batch setting function code(F19.55)55
05/03/2024 11:17:36 Batch setting function code(F19.56)56
05/03/2024 11:17:36 Batch setting function code(F19.57)57
05/03/2024 11:17:36 Batch setting function code(F19.58)58
05/03/2024 11:17:36 Batch setting function code(F19.59)59
05/03/2024 11:17:36 Batch setting function code(F19.60)60
05/03/2024 11:17:36 Batch setting function code(F19.61)61
05/03/2024 11:17:36 Batch setting function code(F19.62)62
05/03/2024 11:17:36 Batch setting function code(F19.63)504
05/03/2024 11:17:36 Batch setting function code(F25.00 AI1 The measured voltage 1)0.515
05/03/2024 11:17:36 Batch setting function code(F25.01 AI1 Monitoring the voltage 1)0.500
05/03/2024 11:17:36 Batch setting function code(F25.02 AI1 The measured voltage 2)5.156
05/03/2024 11:17:36 Batch setting function code(F25.03 AI1 Monitoring the voltage 2)5.000
05/03/2024 11:17:36 Batch setting function code(F25.04 AI1 The measured voltage 3)9.796
05/03/2024 11:17:37 Batch setting function code(F25.05 AI1 Monitoring the voltage 3)9.500
05/03/2024 11:17:37 Batch setting function code(F25.06 AI1 The measured current 1)1.031
05/03/2024 11:17:37 Batch setting function code(F25.07 AI1 Monitor current 1)1.000
05/03/2024 11:17:37 Batch setting function code(F25.08 AI1 The measured current 2)10.312
05/03/2024 11:17:37 Batch setting function code(F25.09 AI1 The measured voltage 2)10.000
05/03/2024 11:17:37 Batch setting function code(F25.10 AI1 The measured current 3)19.593
05/03/2024 11:17:37 Batch setting function code(F25.11 AI1 Monitor current 3)19.000
05/03/2024 11:17:37 Batch setting function code(F25.12 AI2 The measured voltage 1)0.515
05/03/2024 11:17:37 Batch setting function code(F25.13 AI2 Monitoring the voltage 1)0.500
05/03/2024 11:17:37 Batch setting function code(F25.14 AI2 The measured voltage 2)5.156
05/03/2024 11:17:37 Batch setting function code(F25.15 AI2 Monitoring the voltage 2)5.000
05/03/2024 11:17:37 Batch setting function code(F25.16 AI2 The measured voltage 3)9.796
05/03/2024 11:17:37 Batch setting function code(F25.17 AI2 Monitoring the voltage 3)9.500
05/03/2024 11:17:37 Batch setting function code(F25.18 AI2 The measured current 1)1.031
05/03/2024 11:17:37 Batch setting function code(F25.19 AI2 Monitor current 1)1.000
05/03/2024 11:17:38 Batch setting function code(F25.20 AI2 The measured current 2)10.312
05/03/2024 11:17:38 Batch setting function code(F25.21 AI2 Monitor current 2)10.000
05/03/2024 11:17:38 Batch setting function code(F25.22 AI2 The measured current 3)19.593
05/03/2024 11:17:38 Batch setting function code(F25.23 AI2 Monitor current 3)19.000
05/03/2024 11:17:38 Batch setting function code(F25.24 AO1 The measured voltage 1)0.501
05/03/2024 11:17:38 Batch setting function code(F25.25 AO1 Monitoring the voltage 1)0.500
05/03/2024 11:17:38 Batch setting function code(F25.26 AO1 The measured voltage 2)5.019
05/03/2024 11:17:38 Batch setting function code(F25.27 AO1 Monitoring the voltage 2)5.000
05/03/2024 11:17:38 Batch setting function code(F25.28 AO1 The measured voltage 3)9.537
05/03/2024 11:17:38 Batch setting function code(F25.29 AO1 Monitoring the voltage 3)9.500
05/03/2024 11:17:38 Batch setting function code(F25.30 AO1 The measured current 1)1.003
05/03/2024 11:17:38 Batch setting function code(F25.31 AO1 Monitor current 1)1.000
05/03/2024 11:17:38 Batch setting function code(F25.32 AO1 The measured current 2)10.039
05/03/2024 11:17:38 Batch setting function code(F25.33 AO1 Monitor current 2)10.000
05/03/2024 11:17:38 Batch setting function code(F25.34 AO1 The measured current 3)19.074
05/03/2024 11:17:38 Batch setting function code(F25.35 AO1 Monitor current 3)19.000
05/03/2024 11:17:39 Batch setting function code(F25.36 AO2 The measured voltage 1)0.501
05/03/2024 11:17:39 Batch setting function code(F25.37 AO2 Monitoring the voltage 1)0.500
05/03/2024 11:17:39 Batch setting function code(F25.38 AO2 The measured voltage 2)5.019
05/03/2024 11:17:39 Function code(F25.39 AO2 Monitoring the voltage 2)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.40 AO2 The measured voltage 3)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.41 AO2 Monitoring the voltage 3)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.42 AO2 The measured current 1)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.43 AO2 Monitor current 1)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.44 AO2 The measured current 2)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.45 AO2 Monitor current 2)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.46 AO2 The measured current 3)Communication failed(code:0x86)
05/03/2024 11:17:39 Function code(F25.47 AO2 Monitor current 3)Communication failed(code:0x86)
05/03/2024 11:17:39 Batch setting function code(Communication Given frequency)0.00
05/03/2024 11:17:39 Batch setting function code(Communication command Setting)0
05/03/2024 11:17:39 Batch setting function code(Communications given  Upper limit frequency )0.00
05/03/2024 11:17:40 Batch setting function code(Communication Given torque)0.0
05/03/2024 11:17:40 Batch setting function code(Torque control is forward Maximum Frequency limitation )0.0
05/03/2024 11:17:40 Batch setting function code(Torque control reverse Maximum Frequency limit)0.0
05/03/2024 11:17:40 Batch setting function code(Communications given PID Setting )0.0
05/03/2024 11:17:40 Batch setting function code(Communications given PID feedback)0.0
05/03/2024 11:17:40 Batch setting function code(Voltage and frequency separation voltage setting)0.0
05/03/2024 11:17:40 Batch setting function code(Tension Setting)0.0
05/03/2024 11:17:40 Batch setting function code(Coil diameter Setting)0.0
05/03/2024 11:17:40 Batch setting function code(Linear velocity  Setting )0.0
05/03/2024 11:17:40 Batch setting function code(Acceleration time 1)1.00
05/03/2024 11:17:40 Batch setting function code(Deceleration time 1)6.00
05/03/2024 11:17:40 Batch setting function code(Torque current component)0.00
05/03/2024 11:17:40 Batch setting function code(Torque filter time )0.100
05/03/2024 11:17:40 Batch setting function code(Reserved)0.0
05/03/2024 11:17:40 Batch setting function code(Reserved)0.0
05/03/2024 11:17:40 Batch setting function code(Reserved)0.0
05/03/2024 11:17:41 Batch setting function code(Reserved)0.0
05/03/2024 11:17:41 Batch setting function code(Reserved)0.0
05/03/2024 11:17:41 Batch setting function code(Terminal  Output )0.0
05/03/2024 11:17:41 Batch setting function code(AO1 Output)0.00
05/03/2024 11:17:41 Batch setting function code(AO2 Output )0.00
05/03/2024 11:17:41 Batch setting function code(CAN Communication Given frequency)0.00
05/03/2024 11:17:41 Batch setting function code(CAN Communication start command )0
05/03/2024 11:17:41 Perform batch write function operation completed
05/03/2024 11:17:55 Read function code(F01.00 Motor 1 way to control )：1:AM Open loop vector 
05/03/2024 11:17:55 Read function code(F01.01 Run command channel)：1:Terminal control 
05/03/2024 11:17:55 Read function code(F01.02 Frequency given source channel A)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:17:55 Read function code(F01.03 Frequency given source channel A gain)：1.0
05/03/2024 11:17:55 Read function code(F01.04 Frequency given source channel B)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:17:55 Read function code(F01.05 Frequency given source channel B  gain)：1.0
05/03/2024 11:17:55 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:17:55 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:17:55 Read function code(F01.08 Run command bundle )：1111
05/03/2024 11:17:55 Read function code(F01.09 Keyboard numbers  Setting  frequency )：1.00
05/03/2024 11:17:55 Read function code(F01.10 Maximum frequency )：1.00
05/03/2024 11:17:55 Read function code(F01.11 Upper frequency source selection)：1:Reserved
05/03/2024 11:17:55 Read function code(F01.12 Digital setting of upper limit frequency)：1.00
05/03/2024 11:17:55 Read function code(F01.13 Lower limit frequency )：1.00
05/03/2024 11:17:55 Read function code(F01.14 Frequency Instruction Resolution)：1:0.1Hz
05/03/2024 11:17:55 Read function code(F01.15 Reserved)：0
05/03/2024 11:17:55 Read function code(F01.16 Reserved)：0
05/03/2024 11:17:55 Read function code(F01.17 Reserved)：0
05/03/2024 11:17:55 Read function code(F01.18 Reserved)：0
05/03/2024 11:17:55 Read function code(F01.19 Reserved)：0
05/03/2024 11:17:56 Read function code(F01.20 Base frequency of acceleration and deceleration time )：1:Fixed frequency 50Hz
05/03/2024 11:17:56 Read function code(F01.21 Acceleration time unit)：1:0.1S
05/03/2024 11:17:56 Read function code(F01.22 Acceleration time 1)：1.00
05/03/2024 11:17:56 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:17:56 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:17:56 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:17:56 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:17:56 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:17:56 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:17:56 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:17:56 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:17:56 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:17:56 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:17:56 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:17:56 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:17:56 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:17:56 Read function code(F01.36 Reserved)：0
05/03/2024 11:17:56 Read function code(F01.37 Reserved)：0
05/03/2024 11:17:56 Read function code(F01.38 Reserved)：0
05/03/2024 11:17:56 Read function code(F01.39 Reserved)：0
05/03/2024 11:17:56 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:17:56 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:17:56 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:17:56 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:17:57 Read function code(F01.44 Reserved)：15
05/03/2024 11:17:57 Read function code(F01.45 Reserved)：50
05/03/2024 11:17:57 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:17:57 Read function code(F01.47 Reserved)：0
05/03/2024 11:17:57 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:17:57 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:18:24 Send forward operation command successfully
05/03/2024 11:18:25 Send forward operation command successfully
05/03/2024 11:18:30 Send fault reset command successfully
05/03/2024 11:18:34 Read function code(F01.00 Motor 1 way to control )：1:AM Open loop vector 
05/03/2024 11:18:34 Read function code(F01.01 Run command channel)：2:RS485 Communication control
05/03/2024 11:18:34 Read function code(F01.02 Frequency given source channel A)：6:RS485 communication setting
05/03/2024 11:18:34 Read function code(F01.03 Frequency given source channel A gain)：1.0
05/03/2024 11:18:34 Read function code(F01.04 Frequency given source channel B)：1:Keyboard analog potentiometer setting (AC10)
05/03/2024 11:18:34 Read function code(F01.05 Frequency given source channel B  gain)：1.0
05/03/2024 11:18:34 Read function code(F01.06 Frequency channel B reference source)：1:Take A set frequency as reference source 
05/03/2024 11:18:34 Read function code(F01.07 Frequency given source selection)：1:Channel B
05/03/2024 11:18:34 Read function code(F01.08 Run command bundle )：1111
05/03/2024 11:18:34 Read function code(F01.09 Keyboard numbers  Setting  frequency )：1.00
05/03/2024 11:18:34 Read function code(F01.10 Maximum frequency )：1.00
05/03/2024 11:18:34 Read function code(F01.11 Upper frequency source selection)：1:Reserved
05/03/2024 11:18:34 Read function code(F01.12 Digital setting of upper limit frequency)：1.00
05/03/2024 11:18:34 Read function code(F01.13 Lower limit frequency )：1.00
05/03/2024 11:18:34 Read function code(F01.14 Frequency Instruction Resolution)：1:0.1Hz
05/03/2024 11:18:34 Read function code(F01.15 Reserved)：0
05/03/2024 11:18:34 Read function code(F01.16 Reserved)：0
05/03/2024 11:18:34 Read function code(F01.17 Reserved)：0
05/03/2024 11:18:34 Read function code(F01.18 Reserved)：0
05/03/2024 11:18:34 Read function code(F01.19 Reserved)：0
05/03/2024 11:18:35 Read function code(F01.20 Base frequency of acceleration and deceleration time )：1:Fixed frequency 50Hz
05/03/2024 11:18:35 Read function code(F01.21 Acceleration time unit)：1:0.1S
05/03/2024 11:18:35 Read function code(F01.22 Acceleration time 1)：1.00
05/03/2024 11:18:35 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:18:35 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:18:35 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:18:35 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:18:35 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:18:35 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:18:35 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:18:35 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:18:35 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:18:35 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:18:35 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:18:35 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:18:35 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:18:35 Read function code(F01.36 Reserved)：0
05/03/2024 11:18:35 Read function code(F01.37 Reserved)：0
05/03/2024 11:18:35 Read function code(F01.38 Reserved)：0
05/03/2024 11:18:36 Read function code(F01.39 Reserved)：0
05/03/2024 11:18:36 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:18:36 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:18:36 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:18:36 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:18:36 Read function code(F01.44 Reserved)：15
05/03/2024 11:18:36 Read function code(F01.45 Reserved)：50
05/03/2024 11:18:36 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:18:36 Read function code(F01.47 Reserved)：0
05/03/2024 11:18:36 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:18:36 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:18:36 Read function code(F00.00 Parameter access level )：0:Standard parameter 
05/03/2024 11:18:37 Read function code(F00.01 Purpose selection)：0:Universal 
05/03/2024 11:18:37 Read function code(F00.02 Motor selection)：0
05/03/2024 11:18:37 Read function code(F00.03 Initialization)：0:Not initialized 
05/03/2024 11:18:37 Read function code(F00.04 Keyboard parameter copy)：0:No function 
05/03/2024 11:18:37 Read function code(F00.05 User password)：0000
05/03/2024 11:18:37 Read function code(F00.06 LCD keyboard language selection)：0
05/03/2024 11:18:37 Read function code(F00.07 Free parameters 1)：0
05/03/2024 11:18:37 Read function code(F00.08 Free parameters 2)：0
05/03/2024 11:18:37 Read function code(F00.09 Reserved)：0
05/03/2024 11:18:37 Read function code(F00.10 Common parameters 1Address setting)：0100
05/03/2024 11:18:37 Read function code(F00.11 Common parameters 2Address setting)：0101
05/03/2024 11:18:37 Read function code(F00.12 Common parameters 3Address setting)：0102
05/03/2024 11:18:37 Read function code(F00.13 Common parameters 4Address setting)：0710
05/03/2024 11:18:37 Read function code(F00.14 Common parameters 5Address setting)：0122
05/03/2024 11:18:37 Read function code(F00.15 Common parameters 6Address setting)：0123
05/03/2024 11:18:37 Read function code(F00.16 Common parameters 7Address setting)：0110
05/03/2024 11:18:37 Read function code(F00.17 Common parameters 8Address setting)：0112
05/03/2024 11:18:37 Read function code(F00.18 Common parameters 9Address setting)：0140
05/03/2024 11:18:37 Read function code(F00.19 Common parameters 10Address setting)：0730
05/03/2024 11:18:37 Read function code(F00.20 Common parameters 11Address setting)：0201
05/03/2024 11:18:37 Read function code(F00.21 Common parameters 12Address setting)：0202
05/03/2024 11:18:37 Read function code(F00.22 Common parameters 13Address setting)：0203
05/03/2024 11:18:37 Read function code(F00.23 Common parameters 14Address setting)：0204
05/03/2024 11:18:37 Read function code(F00.24 Common parameters 15Address setting)：0205
05/03/2024 11:18:37 Read function code(F00.25 Common parameters 16Address setting)：0206
05/03/2024 11:18:38 Read function code(F00.26 Common parameters 17Address setting)：0207
05/03/2024 11:18:38 Read function code(F00.27 Common parameters 18Address setting)：1201
05/03/2024 11:18:38 Read function code(F00.28 Common parameters 19Address setting)：1202
05/03/2024 11:18:38 Read function code(F00.29 Common parameters 20Address setting)：1203
05/03/2024 11:18:38 Read function code(F00.30 Common parameters 21Address setting)：0700
05/03/2024 11:18:38 Read function code(F00.31 Common parameters 22Address setting)：0705
05/03/2024 11:18:38 Read function code(F00.32 Common parameters 23Address setting)：0502
05/03/2024 11:18:38 Read function code(F00.33 Common parameters 24Address setting)：0503
05/03/2024 11:18:38 Read function code(F00.34 Common parameters 25Address setting)：0504
05/03/2024 11:18:38 Read function code(F00.35 Common parameters 26Address setting)：0601
05/03/2024 11:18:38 Read function code(F00.36 Common parameters 27Address setting)：0600
05/03/2024 11:18:38 Read function code(F00.37 Common parameters 28Address setting)：0621
05/03/2024 11:18:38 Read function code(F00.38 Common parameters 29Address setting)：0622
05/03/2024 11:18:38 Read function code(F00.39 Common parameters 30Address setting)：0400
05/03/2024 11:18:38 Read function code(F00.40 Single board debugging options)：0000
05/03/2024 11:18:38 Read function code(F00.41 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.42 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.43 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.44 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.45 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.46 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.47 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.48 Reserved)：0
05/03/2024 11:18:38 Read function code(F00.49 Reserved)：0
05/03/2024 11:18:43 Set function code(F00.03 Initialization)：0-->22:All Parameter initialization
05/03/2024 11:18:48 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
05/03/2024 11:18:48 Read function code(F01.01 Run command channel)：0:Keyboard control (External keyboard first)
05/03/2024 11:18:48 Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
05/03/2024 11:18:48 Read function code(F01.03 Frequency given source channel A gain)：100.0
05/03/2024 11:18:48 Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
05/03/2024 11:18:48 Read function code(F01.05 Frequency given source channel B  gain)：100.0
05/03/2024 11:18:48 Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
05/03/2024 11:18:48 Read function code(F01.07 Frequency given source selection)：0:Channel A
05/03/2024 11:18:48 Read function code(F01.08 Run command bundle )：0000
05/03/2024 11:18:48 Read function code(F01.09 Keyboard numbers  Setting  frequency )：50.00
05/03/2024 11:18:48 Read function code(F01.10 Maximum frequency )：50.00
05/03/2024 11:18:48 Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
05/03/2024 11:18:48 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
05/03/2024 11:18:48 Read function code(F01.13 Lower limit frequency )：0.00
05/03/2024 11:18:48 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
05/03/2024 11:18:48 Read function code(F01.15 Reserved)：0
05/03/2024 11:18:48 Read function code(F01.16 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.17 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.18 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.19 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
05/03/2024 11:18:49 Read function code(F01.21 Acceleration time unit)：2:0.01S
05/03/2024 11:18:49 Read function code(F01.22 Acceleration time 1)：6.00
05/03/2024 11:18:49 Read function code(F01.23 Deceleration time 1)：6.00
05/03/2024 11:18:49 Read function code(F01.24 Acceleration time 2)：10.00
05/03/2024 11:18:49 Read function code(F01.25 Deceleration time 2)：10.00
05/03/2024 11:18:49 Read function code(F01.26 Acceleration time 3)：10.00
05/03/2024 11:18:49 Read function code(F01.27 Deceleration time 3)：10.00
05/03/2024 11:18:49 Read function code(F01.28 Acceleration time 4)：10.00
05/03/2024 11:18:49 Read function code(F01.29 Deceleration time 4)：10.00
05/03/2024 11:18:49 Read function code(F01.30 S Curve acceleration and deceleration selection )：1
05/03/2024 11:18:49 Read function code(F01.31 Acceleration start S-curve time )：0.20
05/03/2024 11:18:49 Read function code(F01.32 Acceleration end S curve time )：0.20
05/03/2024 11:18:49 Read function code(F01.33 S-curve time to start deceleration )：0.20
05/03/2024 11:18:49 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
05/03/2024 11:18:49 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
05/03/2024 11:18:49 Read function code(F01.36 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.37 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.38 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.39 Reserved)：0
05/03/2024 11:18:49 Read function code(F01.40 PWM Carrier frequency )：4.0
05/03/2024 11:18:49 Read function code(F01.41 PWM Control mode )：1111
05/03/2024 11:18:50 Read function code(F01.42 PWM way to control 1)：9101
05/03/2024 11:18:50 Read function code(F01.43 Dead zone compensation gain )：306
05/03/2024 11:18:50 Read function code(F01.44 Reserved)：15
05/03/2024 11:18:50 Read function code(F01.45 Reserved)：50
05/03/2024 11:18:50 Read function code(F01.46 Random carrier depth )：0
05/03/2024 11:18:50 Read function code(F01.47 Reserved)：0
05/03/2024 11:18:50 Read function code(F01.48 Reserved)：0.00
05/03/2024 11:18:50 Read function code(F01.49 Reserved)：6.0
05/03/2024 11:18:52 Send forward operation command successfully
05/03/2024 11:18:54 Send forward operation command successfully
05/03/2024 11:18:57 Send forward operation command successfully
05/03/2024 11:18:59 Send the reversal operation command successfully
05/03/2024 11:19:27 Send fault reset command successfully
05/03/2024 11:19:29 Send fault reset command successfully
05/03/2024 11:19:30 Free stop command sent successfully
05/03/2024 11:19:33 Send forward operation command successfully
05/03/2024 11:19:34 Send forward operation command successfully
05/03/2024 11:19:34 Send the reversal operation command successfully
05/03/2024 11:19:37 Send deceleration to stop command successfully
05/03/2024 11:19:40 Send deceleration to stop command successfully
05/03/2024 11:19:41 Free stop command sent successfully
05/03/2024 11:19:42 Send deceleration to stop command successfully
05/03/2024 11:19:45 Send forward operation command successfully
05/03/2024 11:19:48 Send deceleration to stop command successfully
05/03/2024 11:19:53 Send forward jog command successfully
05/03/2024 11:19:58 Send deceleration to stop command successfully
05/03/2024 11:39:40 The serial port is unplugged, please check the line
05/03/2024 11:39:40 Communication(COM3)Disconnected
